[    4.009019] usb usb2: Product: OHCI Host Controller

[    4.009021] usb usb2: Manufacturer: Linux 2.6.28.4 ohci_hcd

[    4.009024] usb usb2: SerialNumber: 0000:00:02.0

[    4.009076] uhci_hcd: USB Universal Host Controller Interface driver

[    4.009275] Initializing USB Mass Storage driver...

[    4.009330] usbcore: registered new interface driver usb-storage

[    4.009333] USB Mass Storage support registered.

[    4.009372] usbcore: registered new interface driver libusual

[    4.009448] PNP: PS/2 Controller [PNP0303:PS2K] at 0x60,0x64 irq 1

[    4.009451] PNP: PS/2 appears to have AUX port disabled, if this is incorrect please boot with i8042.nopnp

[    4.009921] serio: i8042 KBD port at 0x60,0x64 irq 1

[    4.010463] mice: PS/2 mouse device common for all mice

[    4.011097] rtc_cmos 00:02: RTC can wake from S4

[    4.011268] rtc_cmos 00:02: rtc core: registered rtc_cmos as rtc0

[    4.011304] rtc0: alarms up to one year, y3k, 114 bytes nvram

[    4.011423] EISA: Probing bus 0 at eisa.0

[    4.011463] cpuidle: using governor ladder

[    4.011466] cpuidle: using governor menu

[    4.012090] usbcore: registered new interface driver hiddev

[    4.012123] usbcore: registered new interface driver usbhid

[    4.012126] usbhid: v2.6:USB HID core driver

[    4.012172] Advanced Linux Sound Architecture Driver Version 1.0.18rc3.

[    4.012825] ALSA device list:

[    4.012827]   No soundcards found.

[    4.013307] TCP cubic registered

[    4.013309] Initializing XFRM netlink socket

[    4.013315] NET: Registered protocol family 17

[    4.013321] NET: Registered protocol family 15

[    4.013441] Using IPI No-Shortcut mode

[    4.014045] rtc_cmos 00:02: setting system clock to 2009-04-06 19:05:52 UTC (1239044752)

[    4.014345] Freeing unused kernel memory: 428k freed

[    4.529995] cdrom: sr0: mrw address space DMA selected

[    4.660372] ISO 9660 Extensions: Microsoft Joliet Level 3

[    4.689800] ISO 9660 Extensions: RRIP_1991A

[    4.756375] usb 2-1: new low speed USB device using ohci_hcd and address 2

[    4.797954] cloop: Initializing cloop v2.628

[    4.798699] cloop: loaded (max 8 devices)

[    4.926859] aufs 20081208

[    4.943655] usb 2-1: configuration #1 chosen from 1 choice

[    4.954829] input: HID 046a:0023 as /class/input/input3

[    4.955201] cherry 0003:046A:0023.0001: input,hidraw0: USB HID v1.11 Keyboard [HID 046a:0023] on usb-0000:00:02.0-1/input0

[    4.966621] input: HID 046a:0023 as /class/input/input4

[    4.966991] cherry 0003:046A:0023.0002: input,hidraw1: USB HID v1.11 Device [HID 046a:0023] on usb-0000:00:02.0-1/input1

[    4.967329] usb 2-1: New USB device found, idVendor=046a, idProduct=0023

[    4.967332] usb 2-1: New USB device strings: Mfr=0, Product=0, SerialNumber=0

[    4.997380] cloop: losetup_file: 13487 blocks, 131072 bytes/block, largest block is 131158 bytes.

[    5.245597] cloop: preloaded 32 blocks into cache.

[    5.249673] usb 2-2: new low speed USB device using ohci_hcd and address 3

[    5.335371] ISO 9660 Extensions: RRIP_1991A

[    5.337056] aufs test_add:432:busybox[1408]: uid/gid/perm /KNOPPIX 0/0/0755, 0/0/01777

[    5.556674] usb 2-2: configuration #1 chosen from 1 choice

[    5.566845] input: Logitech USB Optical Mouse as /class/input/input5

[    5.567388] generic-usb 0003:046D:C046.0003: input,hidraw2: USB HID v1.10 Mouse [Logitech USB Optical Mouse] on usb-0000:00:02.0-2/input0

[    5.567763] usb 2-2: New USB device found, idVendor=046d, idProduct=c046

[    5.567767] usb 2-2: New USB device strings: Mfr=1, Product=2, SerialNumber=0

[    5.567770] usb 2-2: Product: USB Optical Mouse

[    5.567772] usb 2-2: Manufacturer: Logitech

[    5.846299] usb 2-3: new full speed USB device using ohci_hcd and address 4

[    6.037675] usb 2-3: configuration #1 chosen from 1 choice

[    6.041957] usb 2-3: New USB device found, idVendor=04f9, idProduct=0186

[    6.041961] usb 2-3: New USB device strings: Mfr=0, Product=0, SerialNumber=3

[    6.041964] usb 2-3: SerialNumber: 000D6J464460

[    6.319600] usb 2-7: new full speed USB device using ohci_hcd and address 5

[    6.486271] usb 2-7: device descriptor read/64, error -62

[    6.756231] usb 2-7: device descriptor read/64, error -62

[    7.019553] usb 2-7: new full speed USB device using ohci_hcd and address 6

[    7.186207] usb 2-7: device descriptor read/64, error -62

[    7.456188] usb 2-7: device descriptor read/64, error -62

[    7.719499] usb 2-7: new full speed USB device using ohci_hcd and address 7

[    8.126136] usb 2-7: device not accepting address 7, error -62

[    8.286227] usb 2-7: new full speed USB device using ohci_hcd and address 8

[    8.692766] usb 2-7: device not accepting address 8, error -62

[    8.692783] hub 2-0:1.0: unable to enumerate USB device on port 7

[   12.409113] i2c-adapter i2c-0: nForce2 SMBus adapter at 0x5000

[   12.409133] i2c-adapter i2c-1: nForce2 SMBus adapter at 0x6000

[   12.513118] ACPI: PCI Interrupt Link [LAZA] enabled at IRQ 23

[   12.513125] HDA Intel 0000:00:05.0: PCI INT B -> Link[LAZA] -> GSI 23 (level, low) -> IRQ 23

[   12.513241] HDA Intel 0000:00:05.0: setting latency timer to 64

[   12.839147] hda_codec: Unknown model for ALC883, trying auto-probe from BIOS...

[   13.206486] forcedeth: Reverse Engineered nForce ethernet driver. Version 0.61.

[   13.206870] ACPI: PCI Interrupt Link [LMAC] enabled at IRQ 22

[   13.206875] forcedeth 0000:00:07.0: PCI INT A -> Link[LMAC] -> GSI 22 (level, low) -> IRQ 22

[   13.206881] forcedeth 0000:00:07.0: setting latency timer to 64

[   13.723392] forcedeth 0000:00:07.0: ifname eth0, PHY OUI 0x732 @ 1, addr 00:13:8f:dc:2e:ba

[   13.723397] forcedeth 0000:00:07.0: highdma pwrctl mgmt timirq gbit lnktim msi desc-v3

[   17.459138] parport_pc 00:05: reported by Plug and Play ACPI

[   17.459190] parport0: PC-style at 0x378 (0x778), irq 7, dma 3 [PCSPP,TRISTATE,COMPAT,ECP,DMA]

[   17.542236] Serial: 8250/16550 driver4 ports, IRQ sharing disabled

[   17.542346] serial8250: ttyS0 at I/O 0x3f8 (irq = 4) is a 16550A

[   17.673168] 00:09: ttyS0 at I/O 0x3f8 (irq = 4) is a 16550A

[   17.682603] usblp0: USB Bidirectional printer dev 4 if 0 alt 0 proto 2 vid 0x04F9 pid 0x0186

[   17.682625] usbcore: registered new interface driver usblp

[   32.485296] lp0: using parport0 (interrupt-driven).

[   32.485301] lp0: console ready

[   32.811597] ppdev: user-space parallel port driver

[   37.004774] forcedeth 0000:00:07.0: irq 508 for MSI/MSI-X

[   38.840006] NET: Registered protocol family 10

[   38.840488] lo: Disabled Privacy Extensions

[   49.379989] eth0: no IPv6 routers present

