[    0.000000] Initializing cgroup subsys cpuset
[    0.000000] Initializing cgroup subsys cpu
[    0.000000] Linux version 3.2.0-37-generic (buildd@allspice) (gcc version 4.6.3 (Ubuntu/Linaro 4.6.3-1ubuntu5) ) #58-Ubuntu SMP Thu Jan 24 15:28:10 UTC 2013 (Ubuntu 3.2.0-37.58-generic 3.2.35)
[    0.000000] Command line: BOOT_IMAGE=/boot/vmlinuz-3.2.0-37-generic root=UUID=084b103c-8fe1-49ea-9701-debccb02b54d ro quiet splash vt.handoff=7
[    0.000000] KERNEL supported cpus:
[    0.000000]   Intel GenuineIntel
[    0.000000]   AMD AuthenticAMD
[    0.000000]   Centaur CentaurHauls
[    0.000000] BIOS-provided physical RAM map:
[    0.000000]  BIOS-e820: 0000000000000000 - 000000000009fc00 (usable)
[    0.000000]  BIOS-e820: 000000000009fc00 - 00000000000a0000 (reserved)
[    0.000000]  BIOS-e820: 00000000000e0000 - 0000000000100000 (reserved)
[    0.000000]  BIOS-e820: 0000000000100000 - 00000000bfdbd000 (usable)
[    0.000000]  BIOS-e820: 00000000bfdbd000 - 00000000bfddf000 (ACPI NVS)
[    0.000000]  BIOS-e820: 00000000bfddf000 - 00000000bfe05000 (reserved)
[    0.000000]  BIOS-e820: 00000000bfe05000 - 00000000bfe07000 (ACPI NVS)
[    0.000000]  BIOS-e820: 00000000bfe07000 - 00000000bfe13000 (reserved)
[    0.000000]  BIOS-e820: 00000000bfe13000 - 00000000bfe14000 (ACPI NVS)
[    0.000000]  BIOS-e820: 00000000bfe14000 - 00000000bfe1a000 (reserved)
[    0.000000]  BIOS-e820: 00000000bfe1a000 - 00000000bfe20000 (ACPI data)
[    0.000000]  BIOS-e820: 00000000bfe20000 - 00000000bfe21000 (reserved)
[    0.000000]  BIOS-e820: 00000000bfe21000 - 00000000bfe22000 (ACPI NVS)
[    0.000000]  BIOS-e820: 00000000bfe22000 - 00000000bfe24000 (ACPI data)
[    0.000000]  BIOS-e820: 00000000bfe24000 - 00000000bfe29000 (ACPI NVS)
[    0.000000]  BIOS-e820: 00000000bfe29000 - 00000000bfe34000 (reserved)
[    0.000000]  BIOS-e820: 00000000bfe34000 - 00000000bff00000 (usable)
[    0.000000]  BIOS-e820: 00000000fed1c000 - 00000000fed20000 (reserved)
[    0.000000]  BIOS-e820: 00000000ffb00000 - 00000000ffc00000 (reserved)
[    0.000000]  BIOS-e820: 00000000fff00000 - 0000000100000000 (reserved)
[    0.000000] NX (Execute Disable) protection: active
[    0.000000] DMI 2.4 present.
[    0.000000] DMI: MICRO-STAR INTERNATIONAL CO., LTD MS-163A/To be filled by O.E.M., BIOS V1.0Z 06/30/2008
[    0.000000] e820 update range: 0000000000000000 - 0000000000010000 (usable) ==> (reserved)
[    0.000000] e820 remove range: 00000000000a0000 - 0000000000100000 (usable)
[    0.000000] No AGP bridge found
[    0.000000] last_pfn = 0xbff00 max_arch_pfn = 0x400000000
[    0.000000] MTRR default type: uncachable
[    0.000000] MTRR fixed ranges enabled:
[    0.000000]   00000-9FFFF write-back
[    0.000000]   A0000-BFFFF uncachable
[    0.000000]   C0000-E7FFF write-through
[    0.000000]   E8000-FFFFF write-protect
[    0.000000] MTRR variable ranges enabled:
[    0.000000]   0 base 000000000 mask F80000000 write-back
[    0.000000]   1 base 080000000 mask FC0000000 write-back
[    0.000000]   2 base 0BFF00000 mask FFFF00000 uncachable
[    0.000000]   3 base 0FFF00000 mask FFFF00000 write-protect
[    0.000000]   4 disabled
[    0.000000]   5 disabled
[    0.000000]   6 disabled
[    0.000000]   7 disabled
[    0.000000] x86 PAT enabled: cpu 0, old 0x7040600070406, new 0x7010600070106
[    0.000000] found SMP MP-table at [ffff8800000fd3d0] fd3d0
[    0.000000] initial memory mapped : 0 - 20000000
[    0.000000] Base memory trampoline at [ffff88000009a000] 9a000 size 20480
[    0.000000] init_memory_mapping: 0000000000000000-00000000bff00000
[    0.000000]  0000000000 - 00bfe00000 page 2M
[    0.000000]  00bfe00000 - 00bff00000 page 4k
[    0.000000] kernel direct mapping tables up to bff00000 @ 1fffb000-20000000
[    0.000000] RAMDISK: 364d0000 - 37260000
[    0.000000] ACPI: RSDP 00000000000f03c0 00024 (v02 MSI_NB)
[    0.000000] ACPI: XSDT 00000000bfe22f10 0004C (v01 MSI_NB MEGABOOK 20070707 MSFT 00010013)
[    0.000000] ACPI: FACP 00000000bfe13c10 000F4 (v04 MSI_NB MEGABOOK 20070707 MSFT 00010013)
[    0.000000] ACPI Warning: 32/64 FACS address mismatch in FADT - two FACS tables! (20110623/tbfadt-365)
[    0.000000] ACPI Warning: 32/64X FACS address mismatch in FADT - 0xBFE21F40/0x00000000BFE21E40, using 32 (20110623/tbfadt-489)
[    0.000000] ACPI: DSDT 00000000bfe1a010 0517C (v01 MSI_NB MEGABOOK 00000000 INTL 20051117)
[    0.000000] ACPI: FACS 00000000bfe21f40 00040
[    0.000000] ACPI: APIC 00000000bfe23e90 0005C (v02 MSI_NB MEGABOOK 20070707 MSFT 00010013)
[    0.000000] ACPI: MCFG 00000000bfe27c90 0003C (v01 MSI_NB MEGABOOK 20070707 MSFT 00000097)
[    0.000000] ACPI: SLIC 00000000bfe24c10 00176 (v01 MSI_NB MEGABOOK 20070707 MSFT 00000097)
[    0.000000] ACPI: SSDT 00000000bfe05a10 004C4 (v01  PmRef    CpuPm 00003000 INTL 20051117)
[    0.000000] ACPI: Local APIC address 0xfee00000
[    0.000000] No NUMA configuration found
[    0.000000] Faking a node at 0000000000000000-00000000bff00000
[    0.000000] Initmem setup node 0 0000000000000000-00000000bff00000
[    0.000000]   NODE_DATA [00000000bfefb000 - 00000000bfefffff]
[    0.000000]  [ffffea0000000000-ffffea0002ffffff] PMD -> [ffff8800bc400000-ffff8800bf3fffff] on node 0
[    0.000000] Zone PFN ranges:
[    0.000000]   DMA      0x00000010 -> 0x00001000
[    0.000000]   DMA32    0x00001000 -> 0x00100000
[    0.000000]   Normal   empty
[    0.000000] Movable zone start PFN for each node
[    0.000000] early_node_map[3] active PFN ranges
[    0.000000]     0: 0x00000010 -> 0x0000009f
[    0.000000]     0: 0x00000100 -> 0x000bfdbd
[    0.000000]     0: 0x000bfe34 -> 0x000bff00
[    0.000000] On node 0 totalpages: 785944
[    0.000000]   DMA zone: 64 pages used for memmap
[    0.000000]   DMA zone: 5 pages reserved
[    0.000000]   DMA zone: 3914 pages, LIFO batch:0
[    0.000000]   DMA32 zone: 12220 pages used for memmap
[    0.000000]   DMA32 zone: 769741 pages, LIFO batch:31
[    0.000000] ACPI: PM-Timer IO Port: 0x408
[    0.000000] ACPI: Local APIC address 0xfee00000
[    0.000000] ACPI: LAPIC (acpi_id[0x01] lapic_id[0x00] enabled)
[    0.000000] ACPI: LAPIC (acpi_id[0x02] lapic_id[0x01] enabled)
[    0.000000] ACPI: IOAPIC (id[0x02] address[0xfec00000] gsi_base[0])
[    0.000000] IOAPIC[0]: apic_id 2, version 32, address 0xfec00000, GSI 0-23
[    0.000000] ACPI: INT_SRC_OVR (bus 0 bus_irq 0 global_irq 2 dfl dfl)
[    0.000000] ACPI: INT_SRC_OVR (bus 0 bus_irq 9 global_irq 9 high level)
[    0.000000] ACPI: IRQ0 used by override.
[    0.000000] ACPI: IRQ2 used by override.
[    0.000000] ACPI: IRQ9 used by override.
[    0.000000] Using ACPI (MADT) for SMP configuration information
[    0.000000] SMP: Allowing 2 CPUs, 0 hotplug CPUs
[    0.000000] nr_irqs_gsi: 40
[    0.000000] PM: Registered nosave memory: 000000000009f000 - 00000000000a0000
[    0.000000] PM: Registered nosave memory: 00000000000a0000 - 00000000000e0000
[    0.000000] PM: Registered nosave memory: 00000000000e0000 - 0000000000100000
[    0.000000] PM: Registered nosave memory: 00000000bfdbd000 - 00000000bfddf000
[    0.000000] PM: Registered nosave memory: 00000000bfddf000 - 00000000bfe05000
[    0.000000] PM: Registered nosave memory: 00000000bfe05000 - 00000000bfe07000
[    0.000000] PM: Registered nosave memory: 00000000bfe07000 - 00000000bfe13000
[    0.000000] PM: Registered nosave memory: 00000000bfe13000 - 00000000bfe14000
[    0.000000] PM: Registered nosave memory: 00000000bfe14000 - 00000000bfe1a000
[    0.000000] PM: Registered nosave memory: 00000000bfe1a000 - 00000000bfe20000
[    0.000000] PM: Registered nosave memory: 00000000bfe20000 - 00000000bfe21000
[    0.000000] PM: Registered nosave memory: 00000000bfe21000 - 00000000bfe22000
[    0.000000] PM: Registered nosave memory: 00000000bfe22000 - 00000000bfe24000
[    0.000000] PM: Registered nosave memory: 00000000bfe24000 - 00000000bfe29000
[    0.000000] PM: Registered nosave memory: 00000000bfe29000 - 00000000bfe34000
[    0.000000] Allocating PCI resources starting at bff00000 (gap: bff00000:3ee1c000)
[    0.000000] Booting paravirtualized kernel on bare hardware
[    0.000000] setup_percpu: NR_CPUS:256 nr_cpumask_bits:256 nr_cpu_ids:2 nr_node_ids:1
[    0.000000] PERCPU: Embedded 28 pages/cpu @ffff8800bfa00000 s83136 r8192 d23360 u1048576
[    0.000000] pcpu-alloc: s83136 r8192 d23360 u1048576 alloc=1*2097152
[    0.000000] pcpu-alloc: [0] 0 1 
[    0.000000] Built 1 zonelists in Node order, mobility grouping on.  Total pages: 773655
[    0.000000] Policy zone: DMA32
[    0.000000] Kernel command line: BOOT_IMAGE=/boot/vmlinuz-3.2.0-37-generic root=UUID=084b103c-8fe1-49ea-9701-debccb02b54d ro quiet splash vt.handoff=7
[    0.000000] PID hash table entries: 4096 (order: 3, 32768 bytes)
[    0.000000] Checking aperture...
[    0.000000] No AGP bridge found
[    0.000000] Calgary: detecting Calgary via BIOS EBDA area
[    0.000000] Calgary: Unable to locate Rio Grande table in EBDA - bailing!
[    0.000000] Memory: 3064676k/3144704k available (6569k kernel code, 928k absent, 79100k reserved, 6634k data, 924k init)
[    0.000000] SLUB: Genslabs=15, HWalign=64, Order=0-3, MinObjects=0, CPUs=2, Nodes=1
[    0.000000] Hierarchical RCU implementation.
[    0.000000] 
RCU dyntick-idle grace-period acceleration is enabled.
[    0.000000] NR_IRQS:16640 nr_irqs:512 16
[    0.000000] Extended CMOS year: 2000
[    0.000000] spurious 8259A interrupt: IRQ7.
[    0.000000] vt handoff: transparent VT on vt#7
[    0.000000] Console: colour dummy device 80x25
[    0.000000] console [tty0] enabled
[    0.000000] allocated 25165824 bytes of page_cgroup
[    0.000000] please try 'cgroup_disable=memory' option if you don't want memory cgroups
[    0.000000] Fast TSC calibration using PIT
[    0.000000] Detected 2195.576 MHz processor.
[    0.008006] Calibrating delay loop (skipped), value calculated using timer frequency.. 4391.15 BogoMIPS (lpj=8782304)
[    0.008011] pid_max:

 default: 32768 minimum: 301
[    0.008039] Security Framework initialized
[    0.008065] AppArmor: AppArmor initialized
[    0.008067] Yama: becoming mindful.
[    0.008497] Dentry cache hash table entries: 524288 (order: 10, 4194304 bytes)
[    0.014592] Inode-cache hash table entries: 262144 (order: 9, 2097152 bytes)
[    0.016359] Mount-cache hash table entries: 256
[    0.016551] Initializing cgroup subsys cpuacct
[    0.016557] Initializing cgroup subsys memory
[    0.016568] Initializing cgroup subsys devices
[    0.016571] Initializing cgroup subsys freezer
[    0.016573] Initializing cgroup subsys blkio
[    0.016581] Initializing cgroup subsys perf_event
[    0.016620] CPU: Physical Processor ID: 0
[    0.016621] CPU: Processor Core ID: 0
[    0.016624] mce: CPU supports 6 MCE banks
[    0.016634] CPU0: Thermal monitoring enabled (TM2)
[    0.016639] using mwait in idle threads.
[    0.019360] ACPI: Core revision 20110623
[    0.023975] ftrace: allocating 27033 entries in 107 pages
[    0.028436] ..TIMER: vector=0x30 apic1=0 pin1=2 apic2=0 pin2=0
[    0.071548] CPU0: Intel(R) Core(TM)2 Duo CPU     T7500  @ 2.20GHz stepping 0b
[    0.072003] Performance Events: PEBS fmt0+, Core2 events, Intel PMU driver.
[    0.072003] PEBS disabled due to CPU errata.
[    0.072003] ... version:                2
[    0.072003] ... bit width:              40
[    0.072003] ... generic registers:      2
[    0.072003] ... value mask:             000000ffffffffff
[    0.072003] ... max period:             000000007fffffff
[    0.072003] ... fixed-purpose events:   3
[    0.072003] ... event mask:             0000000700000003
[    0.072003] NMI watchdog enabled, takes one hw-pmu counter.
[    0.072003] Booting Node   0, Processors  #1 Ok.
[    0.072003] smpboot cpu 1: start_ip = 9a000
[    0.160043] NMI watchdog enabled, takes one hw-pmu counter.
[    0.160092] Brought up 2 CPUs
[    0.160094] Total of 2 processors activated (8782.76 BogoMIPS).
[    0.162121] devtmpfs: initialized
[    0.162121] EVM: security.selinux
[    0.162121] EVM: security.SMACK64
[    0.162121] EVM: security.capability
[    0.162121] PM: Registering ACPI NVS region at bfdbd000 (139264 bytes)
[    0.162121] PM: Registering ACPI NVS region at bfe05000 (8192 bytes)
[    0.162121] PM: Registering ACPI NVS region at bfe13000 (4096 bytes)
[    0.162121] PM: Registering ACPI NVS region at bfe21000 (4096 bytes)
[    0.162121] PM: Registering ACPI NVS region at bfe24000 (20480 bytes)
[    0.164132] print_constraints: dummy: 
[    0.164171] RTC time: 12:41:40, date: 02/12/13
[    0.164207] NET: Registered protocol family 16
[    0.164355] Trying to unpack rootfs image as initramfs...
[    0.164355] ACPI: bus type pci registered
[    0.164428] PCI: MMCONFIG for domain 0000 [bus 00-ff] at [mem 0xe0000000-0xefffffff] (base 0xe0000000)
[    0.164432] PCI: not using MMCONFIG
[    0.164434] PCI: Using configuration type 1 for base access
[    0.165548] bio: create slab <bio-0> at 0
[    0.165633] ACPI: Added _OSI(Module Device)
[    0.165636] ACPI: Added _OSI(Processor Device)
[    0.165638] ACPI: Added _OSI(3.0 _SCP Extensions)
[    0.165640] ACPI: Added _OSI(Processor Aggregator Device)
[    0.166687] ACPI: EC: Look up EC in DSDT
[    0.167745] ACPI: Executed 1 blocks of module-level executable AML code
[    0.168978] [Firmware Bug]: ACPI: BIOS _OSI(Linux) query ignored
[    0.169268] ACPI: SSDT 00000000bfe06c10 00288 (v01  PmRef  Cpu0Ist 00003000 INTL 20051117)
[    0.169525] ACPI: Dynamic OEM Table Load:
[    0.169529] ACPI: SSDT           (null) 00288 (v01  PmRef  Cpu0Ist 00003000 INTL 20051117)
[    0.169632] ACPI: SSDT 00000000bfe26b90 00427 (v01  PmRef  Cpu0Cst 00003001 INTL 20051117)
[    0.169876] ACPI: Dynamic OEM Table Load:
[    0.169879] ACPI: SSDT           (null) 00427 (v01  PmRef  Cpu0Cst 00003001 INTL 20051117)
[    0.204273] ACPI: SSDT 00000000bfe06f10 000C4 (v01  PmRef  Cpu1Ist 00003000 INTL 20051117)
[    0.204534] ACPI: Dynamic OEM Table Load:
[    0.204537] ACPI: SSDT           (null) 000C4 (v01  PmRef  Cpu1Ist 00003000 INTL 20051117)
[    0.204617] ACPI: SSDT 00000000bfe13f10 00083 (v01  PmRef  Cpu1Cst 00003000 INTL 20051117)
[    0.204862] ACPI: Dynamic OEM Table Load:
[    0.204865] ACPI: SSDT           (null) 00083 (v01  PmRef  Cpu1Cst 00003000 INTL 20051117)
[    0.228300] ACPI: Interpreter enabled
[    0.228308] ACPI: (supports S0 S1 S3 S4 S5)
[    0.228331] ACPI: Using IOAPIC for interrupt routing
[    0.228363] PCI: MMCONFIG for domain 0000 [bus 00-ff] at [mem 0xe0000000-0xefffffff] (base 0xe0000000)
[    0.228470] PCI: MMCONFIG at [mem 0xe0000000-0xefffffff] reserved in ACPI motherboard resources
[    0.289810] ACPI: EC: GPE storm detected, transactions will use polling mode
[    0.307417] ACPI: EC: GPE = 0x17, I/O: command/status = 0x66, data = 0x62
[    0.307556] ACPI: No dock devices found.
[    0.307559] HEST: Table not found.
[    0.307563] PCI: Using host bridge windows from ACPI; if necessary, use "pci=nocrs" and report a bug
[    0.307705] ACPI: PCI Root Bridge [PCI0] (domain 0000 [bus 00-ff])
[    0.307825] pci_root PNP0A08:00: host bridge window [io  0x0000-0x0cf7]
[    0.307828] pci_root PNP0A08:00: host bridge window [io  0x0d00-0xffff]
[    0.307831] pci_root PNP0A08:00: host bridge window [mem 0x000a0000-0x000bffff]
[    0.307834] pci_root PNP0A08:00: host bridge window [mem 0xc0000000-0xe0203fff]
[    0.307849] pci 0000:00:00.0: [8086:2a00] type 0 class 0x000600
[    0.307908] pci 0000:00:01.0: [8086:2a01] type 1 class 0x000604
[    0.307959] pci 0000:00:01.0: PME# supported from D0 D3hot D3cold
[    0.307963] pci 0000:00:01.0: PME# disabled
[    0.308027] pci 0000:00:1a.0: [8086:2834] type 0 class 0x000c03
[    0.308087] pci 0000:00:1a.0: reg 20: [io  0x60c0-0x60df]
[    0.308133] pci 0000:00:1a.1: [8086:2835] type 0 class 0x000c03
[    0.308193] pci 0000:00:1a.1: reg 20: [io  0x60a0-0x60bf]
[    0.308256] pci 0000:00:1a.7: [8086:283a] type 0 class 0x000c03
[    0.308282] pci 0000:00:1a.7: reg 10: [mem 0xd8204c00-0xd8204fff]
[    0.308393] pci 0000:00:1a.7: PME# supported from D0 D3hot D3cold
[    0.308399] pci 0000:00:1a.7: PME# disabled
[    0.308435] pci 0000:00:1b.0: [8086:284b] type 0 class 0x000403
[    0.308459] pci 0000:00:1b.0: reg 10: [mem 0xd8200000-0xd8203fff 64bit]
[    0.308569] pci 0000:00:1b.0: PME# supported from D0 D3hot D3cold
[    0.308574] pci 0000:00:1b.0: PME# disabled
[    0.308605] pci 0000:00:1c.0: [8086:283f] type 1 class 0x000604
[    0.308722] pci 0000:00:1c.0: PME# supported from D0 D3hot D3cold
[    0.308727] pci 0000:00:1c.0: PME# disabled
[    0.308763] pci 0000:00:1c.2: [8086:2843] type 1 class 0x000604
[    0.308877] pci 0000:00:1c.2: PME# supported from D0 D3hot D3cold
[    0.308882] pci 0000:00:1c.2: PME# disabled
[    0.308917] pci 0000:00:1c.3: [8086:2845] type 1 class 0x000604
[    0.309033] pci 0000:00:1c.3: PME# supported from D0 D3hot D3cold
[    0.309039] pci 0000:00:1c.3: PME# disabled
[    0.309073] pci 0000:00:1c.4: [8086:2847] type 1 class 0x000604
[    0.309187] pci 0000:00:1c.4: PME# supported from D0 D3hot D3cold
[    0.309192] pci 0000:00:1c.4: PME# disabled
[    0.309226] pci 0000:00:1d.0: [8086:2830] type 0 class 0x000c03
[    0.309285] pci 0000:00:1d.0: reg 20: [io  0x6080-0x609f]
[    0.309330] pci 0000:00:1d.1: [8086:2831] type 0 class 0x000c03
[    0.309388] pci 0000:00:1d.1: reg 20: [io  0x6060-0x607f]
[    0.309435] pci 0000:00:1d.2: [8086:2832] type 0 class 0x000c03
[    0.309494] pci 0000:00:1d.2: reg 20: [io  0x6040-0x605f]
[    0.309555] pci 0000:00:1d.7: [8086:2836] type 0 class 0x000c03
[    0.309580] pci 0000:00:1d.7: reg 10: [mem 0xd8204800-0xd8204bff]
[    0.309690] pci 0000:00:1d.7: PME# supported from D0 D3hot D3cold
[    0.309696] pci 0000:00:1d.7: PME# disabled
[    0.309723] pci 0000:00:1e.0: [8086:2448] type 1 class 0x000604
[    0.309825] pci 0000:00:1f.0: [8086:2815] type 0 class 0x000601
[    0.309961] pci 0000:00:1f.0: Force enabled HPET at 0xfed00000
[    0.309975] pci 0000:00:1f.0: ICH7 LPC Generic IO decode 1 PIO at 004c (mask 0007)
[    0.310040] pci 0000:00:1f.1: [8086:2850] type 0 class 0x000101
[    0.310057] pci 0000:00:1f.1: reg 10: [io  0x6160-0x6167]
[    0.310070] pci 0000:00:1f.1: reg 14: [io  0x6150-0x6153]
[    0.310083] pci 0000:00:1f.1: reg 18: [io  0x6140-0x6147]
[    0.310097] pci 0000:00:1f.1: reg 1c: [io  0x6130-0x6133]
[    0.310109] pci 0000:00:1f.1: reg 20: [io  0x6120-0x612f]
[    0.310167] pci 0000:00:1f.2: [8086:2829] type 0 class 0x000106
[    0.310195] pci 0000:00:1f.2: reg 10: [io  0x6110-0x6117]
[    0.310207] pci 0000:00:1f.2: reg 14: [io  0x6100-0x6103]
[    0.310220] pci 0000:00:1f.2: reg 18: [io  0x60f0-0x60f7]
[    0.310233] pci 0000:00:1f.2: reg 1c: [io  0x60e0-0x60e3]
[    0.310245] pci 0000:00:1f.2: reg 20: [io  0x6020-0x603f]
[    0.310258] pci 0000:00:1f.2: reg 24: [mem 0xd8204000-0xd82047ff]
[    0.310326] pci 0000:00:1f.2: PME# supported from D3hot
[    0.310331] pci 0000:00:1f.2: PME# disabled
[    0.310355] pci 0000:00:1f.3: [8086:283e] type 0 class 0x000c05
[    0.310372] pci 0000:00:1f.3: reg 10: [mem 0xd8205000-0xd82050ff]
[    0.310418] pci 0000:00:1f.3: reg 20: [io  0x6000-0x601f]
[    0.310512] pci 0000:01:00.0: [10de:0407] type 0 class 0x000300
[    0.310532] pci 0000:01:00.0: reg 10: [mem 0xd2000000-0xd2ffffff]
[    0.310553] pci 0000:01:00.0: reg 14: [mem 0xc0000000-0xcfffffff 64bit pref]
[    0.310574] pci 0000:01:00.0: reg 1c: [mem 0xd0000000-0xd1ffffff 64bit]
[    0.310589] pci 0000:01:00.0: reg 24: [io  0x5000-0x507f]
[    0.310603] pci 0000:01:00.0: reg 30: [mem 0xd3000000-0xd301ffff pref]
[    0.310713] pci 0000:00:01.0: PCI bridge to [bus 01-01]
[    0.310717] pci 0000:00:01.0:   bridge window [io  0x5000-0x5fff]
[    0.310721] pci 0000:00:01.0:   bridge window [mem 0xc0000000-0xd30fffff]
[    0.310827] pci 0000:02:00.0: [8086:4229] type 0 class 0x000280
[    0.310871] pci 0000:02:00.0:

 reg 10: [mem 0xd6d00000-0xd6d01fff 64bit]
[    0.311083] pci 0000:02:00.0: PME# supported from D0 D3hot D3cold
[    0.311092] pci 0000:02:00.0: PME# disabled
[    0.311173] pci 0000:00:1c.0: PCI bridge to [bus 02-02]
[    0.311178] pci 0000:00:1c.0:   bridge window [io  0x4000-0x4fff]
[    0.311183] pci 0000:00:1c.0:   bridge window [mem 0xd6d00000-0xd80fffff]
[    0.311284] pci 0000:03:00.0: [1095:3531] type 0 class 0x000180
[    0.311320] pci 0000:03:00.0: reg 10: [mem 0xd5902000-0xd590207f 64bit]
[    0.311349] pci 0000:03:00.0: reg 18: [mem 0xd5900000-0xd5901fff 64bit]
[    0.311368] pci 0000:03:00.0: reg 20: [io  0x3000-0x307f]
[    0.311494] pci 0000:03:00.0: supports D1 D2
[    0.316042] pci 0000:00:1c.2: PCI bridge to [bus 03-03]
[    0.316048] pci 0000:00:1c.2:   bridge window [io  0x3000-0x3fff]
[    0.316053] pci 0000:00:1c.2:   bridge window [mem 0xd5900000-0xd6cfffff]
[    0.316124] pci 0000:00:1c.3: PCI bridge to [bus 04-04]
[    0.316129] pci 0000:00:1c.3:   bridge window [io  0x2000-0x2fff]
[    0.316135] pci 0000:00:1c.3:   bridge window [mem 0xd4500000-0xd58fffff]
[    0.316296] pci 0000:05:00.0: [10ec:8168] type 0 class 0x000200
[    0.316364] pci 0000:05:00.0: reg 10: [io  0x1000-0x10ff]
[    0.316483] pci 0000:05:00.0: reg 18: [mem 0xd3120000-0xd3120fff 64bit]
[    0.316621] pci 0000:05:00.0: reg 30: [mem 0xd3100000-0xd311ffff pref]
[    0.316932] pci 0000:05:00.0: supports D1 D2
[    0.316934] pci 0000:05:00.0: PME# supported from D1 D2 D3hot D3cold
[    0.316950] pci 0000:05:00.0: PME# disabled
[    0.317040] pci 0000:05:00.0: disabling ASPM on pre-1.1 PCIe device.  You can enable it with 'pcie_aspm=force'
[    0.317067] pci 0000:00:1c.4: PCI bridge to [bus 05-05]
[    0.317072] pci 0000:00:1c.4:   bridge window [io  0x1000-0x1fff]
[    0.317077] pci 0000:00:1c.4:   bridge window [mem 0xd3100000-0xd44fffff]
[    0.317141] pci 0000:06:04.0: [1180:0832] type 0 class 0x000c00
[    0.317158] pci 0000:06:04.0: proprietary Ricoh MMC controller disabled (via firewire function)
[    0.317161] pci 0000:06:04.0: MMC cards are now supported by standard SDHCI controller
[    0.317177] pci 0000:06:04.0: reg 10: [mem 0xd8100000-0xd81007ff]
[    0.317279] pci 0000:06:04.0: supports D1 D2
[    0.317281] pci 0000:06:04.0: PME# supported from D0 D1 D2 D3hot D3cold
[    0.317287] pci 0000:06:04.0: PME# disabled
[    0.317309] pci 0000:06:04.1: [1180:0822] type 0 class 0x000805
[    0.317333] pci 0000:06:04.1: reg 10: [mem 0xd8100a00-0xd8100aff]
[    0.317436] pci 0000:06:04.1: supports D1 D2
[    0.317439] pci 0000:06:04.1: PME# supported from D0 D1 D2 D3hot D3cold
[    0.317444] pci 0000:06:04.1: PME# disabled
[    0.317467] pci 0000:06:04.2: [1180:0592] type 0 class 0x000880
[    0.317490] pci 0000:06:04.2: reg 10: [mem 0xd8100800-0xd81008ff]
[    0.317592] pci 0000:06:04.2: supports D1 D2
[    0.317595] pci 0000:06:04.2: PME# supported from D0 D1 D2 D3hot D3cold
[    0.317600] pci 0000:06:04.2: PME# disabled
[    0.317670] pci 0000:00:1e.0: PCI bridge to [bus 06-06] (subtractive decode)
[    0.317678] pci 0000:00:1e.0:   bridge window [mem 0xd8100000-0xd81fffff]
[    0.317687] pci 0000:00:1e.0:   bridge window [io  0x0000-0x0cf7] (subtractive decode)
[    0.317690] pci 0000:00:1e.0:   bridge window [io  0x0d00-0xffff] (subtractive decode)
[    0.317693] pci 0000:00:1e.0:   bridge window [mem 0x000a0000-0x000bffff] (subtractive decode)
[    0.317696] pci 0000:00:1e.0:   bridge window [mem 0xc0000000-0xe0203fff] (subtractive decode)
[    0.317738] ACPI: PCI Interrupt Routing Table [\_SB_.PCI0._PRT]
[    0.317840] ACPI: PCI Interrupt Routing Table [\_SB_.PCI0.P0P1._PRT]
[    0.317922] ACPI: PCI Interrupt Routing Table [\_SB_.PCI0.RP01._PRT]
[    0.317953] ACPI: PCI Interrupt Routing Table [\_SB_.PCI0.RP03._PRT]
[    0.317987] ACPI: PCI Interrupt Routing Table [\_SB_.PCI0.RP04._PRT]
[    0.318021] ACPI: PCI Interrupt Routing Table [\_SB_.PCI0.RP05._PRT]
[    0.318135]  pci0000:00: Requesting ACPI _OSC control (0x1d)
[    0.318266]  pci0000:00: ACPI _OSC request failed (AE_SUPPORT), returned control mask: 0x0d
[    0.318269] ACPI _OSC control for PCIe not granted, disabling ASPM
[    0.325013] ACPI: PCI Interrupt Link [LNKA] (IRQs 3 4 5 6 7 10 *11 12 14 15)
[    0.325067] ACPI: PCI Interrupt Link [LNKB] (IRQs 3 4 5 6 7 10 *11 12 14 15)
[    0.325116] ACPI: PCI Interrupt Link [LNKC] (IRQs 3 4 5 6 7 10 *11 12 14 15)
[    0.325165] ACPI: PCI Interrupt Link [LNKD] (IRQs 3 4 5 6 7 10 *11 12 14 15)
[    0.325214] ACPI: PCI Interrupt Link [LNKE] (IRQs 3 4 5 6 7 10 11 12 14 15) *0, disabled.
[    0.325265] ACPI: PCI Interrupt Link [LNKF] (IRQs 3 4 5 6 7 *10 11 12 14 15)
[    0.325314] ACPI: PCI Interrupt Link [LNKG] (IRQs 3 4 5 6 7 *10 11 12 14 15)
[    0.325363] ACPI: PCI Interrupt Link [LNKH] (IRQs 3 4 5 6 7 *10 11 12 14 15)
[    0.325525] vgaarb: device added: PCI:0000:01:00.0,decodes=io+mem,owns=io+mem,locks=none
[    0.325530] vgaarb: loaded
[    0.325532] vgaarb: bridge control possible 0000:01:00.0
[    0.325663] i2c-core: driver [aat2870] using legacy suspend method
[    0.325665] i2c-core: driver [aat2870] using legacy resume method
[    0.325743] SCSI subsystem initialized
[    0.325820] libata version 3.00 loaded.
[    0.325887] usbcore: registered new interface driver usbfs
[    0.325899] usbcore: registered new interface driver hub
[    0.325929] usbcore: registered new device driver usb
[    0.326029] PCI: Using ACPI for IRQ routing
[    0.337097] PCI: pci_cache_line_size set to 64 bytes
[    0.337251] reserve RAM buffer: 000000000009fc00 - 000000000009ffff 
[    0.337253] reserve RAM buffer: 00000000bfdbd000 - 00000000bfffffff 
[    0.337257] reserve RAM buffer: 00000000bff00000 - 00000000bfffffff 
[    0.337411] NetLabel: Initializing
[    0.337413] NetLabel:  domain hash size = 128
[    0.337415] NetLabel:  protocols = UNLABELED CIPSOv4
[    0.337428] NetLabel:  unlabeled traffic allowed by default
[    0.337616] hpet clockevent registered
[    0.337620] HPET: 3 timers in total, 0 timers will be used for per-cpu timer
[    0.337626] hpet0: at MMIO 0xfed00000, IRQs 2, 8, 0
[    0.337630] hpet0: 3 comparators, 64-bit 14.318180 MHz counter
[    0.340094] Switching to clocksource hpet
[    0.348897] AppArmor: AppArmor Filesystem Enabled
[    0.348938] pnp: PnP ACPI init
[    0.348970] ACPI: bus type pnp registered
[    0.349078] pnp 00:00: [bus 00-ff]
[    0.349081] pnp 00:00: [io  0x0cf8-0x0cff]
[    0.349083] pnp 00:00: [io  0x0000-0x0cf7 window]
[    0.349086] pnp 00:00: [io  0x0d00-0xffff window]
[    0.349089] pnp 00:00: [mem 0x000a0000-0x000bffff window]
[    0.349092] pnp 00:00: [mem 0x00000000 window]
[    0.349094] pnp 00:00: [mem 0xc0000000-0xe0203fff window]
[    0.349173] pnp 00:00: Plug and Play ACPI device, IDs PNP0a08 PNP0a03 (active)
[    0.349273] pnp 00:01: [mem 0xfed14000-0xfed17fff]
[    0.349276] pnp 00:01: [mem 0xfed19000-0xfed19fff]
[    0.349278] pnp 00:01: [mem 0xfed18000-0xfed18fff]
[    0.349280] pnp 00:01: [mem 0xe0000000-0xefffffff]
[    0.349282] pnp 00:01: [mem 0xfed13000-0xfed13fff]
[    0.349284] pnp 00:01: [mem 0xfed20000-0xfed3ffff]
[    0.349353] system 00:01: [mem 0xfed14000-0xfed17fff] has been reserved
[    0.349356] system 00:01: [mem 0xfed19000-0xfed19fff] has been reserved
[    0.349359] system 00:01: [mem 0xfed18000-0xfed18fff] has been reserved
[    0.349362] system 00:01: [mem 0xe0000000-0xefffffff] could not be reserved
[    0.349365] system 00:01: [mem 0xfed13000-0xfed13fff] has been reserved
[    0.349371] system 00:01: [mem 0xfed20000-0xfed3ffff] has been reserved
[    0.349375] system 00:01: Plug and Play ACPI device, IDs PNP0c01 (active)
[    0.349405] pnp 00:02: [dma 4]
[    0.349407] pnp 00:02: [io  0x0000-0x000f]
[    0.349409] pnp 00:02: [io  0x0081-0x0083]
[    0.349411] pnp 00:02: [io  0x0087]
[    0.349413] pnp 00:02: [io  0x0089-0x008b]
[    0.349415] pnp 00:02: [io  0x008f]
[    0.349417] pnp 00:02: [io  0x00c0-0x00df]
[    0.349449] pnp 00:02: Plug and Play ACPI device, IDs PNP0200 (active)
[    0.349460] pnp 00:03: [io  0x0070-0x0071]
[    0.349480] pnp 00:03: [irq 8]
[    0.349511] pnp 00:03: Plug and Play ACPI device, IDs PNP0b00 (active)
[    0.349520] pnp 00:04: [io  0x0061]
[    0.349547] pnp 00:04: Plug and Play ACPI device, IDs PNP0800 (active)
[    0.349566] pnp 00:05: [io  0x0010-0x001f]
[    0.349568] pnp 00:05: [io  0x0022-0x003f]
[    0.349570] pnp 00:05: [io  0x0044-0x005f]
[    0.349571] pnp 00:05: [io  0x0063]
[    0.349573] pnp 00:05: [io  0x0065]
[    0.349575] pnp 00:05: [io  0x0067-0x006f]
[    0.349577] pnp 00:05: [io  0x0072-0x007f]
[    0.349579] pnp 00:05: [io  0x0080]
[    0.349581] pnp 00:05: [io  0x0084-0x0086]
[    0.349583] pnp 00:05: [io  0x0088]
[    0.349585] pnp 00:05: [io  0x008c-0x008e]
[    0.349586] pnp 00:05: [io  0x0090-0x009f]
[    0.349588] pnp 00:05: [io  0x00a2-0x00bf]
[    0.349593] pnp 00:05: [io  0x00e0-0x00ef]
[    0.349595] pnp 00:05: [io  0x04d0-0x04d1]
[    0.349598] pnp 00:05: [io  0x0000-0xffffffffffffffff disabled]
[    0.349600] pnp 00:05: [io  0x0000-0xffffffffffffffff disabled]
[    0.349666] system 00:05: [io  0x04d0-0x04d1] has been reserved
[    0.349670] system 00:05: Plug and Play ACPI device, IDs PNP0c02 (active)
[    0.349679] pnp 00:06: [io  0x00f0-0x00ff]
[    0.349686] pnp 00:06: [irq 13]
[    0.349718] pnp 00:06: Plug and Play ACPI device, IDs PNP0c04 (active)
[    0.349744] pnp 00:07: [io  0x0060]
[    0.349746] pnp 00:07: [io  0x0064]
[    0.349752] pnp 00:07: [irq 1]
[    0.349786] pnp 00:07: Plug and Play ACPI device, IDs PNP0303 PNP030b (active)
[    0.349812] pnp 00:08: [irq 12]
[    0.349842] pnp 00:08: Plug and Play ACPI device, IDs PNP0f03 PNP0f13 (active)
[    0.349874] pnp 00:09: [io  0x004c-0x004f]
[    0.349881] pnp 00:09: [irq 4]
[    0.349914] pnp 00:09: Plug and Play ACPI device, IDs ENE0100 (active)
[    0.364198] pnp 00:0a: [io  0x0400-0x047f]
[    0.364201] pnp

 00:0a: [io  0xefa0-0xefaf]
[    0.364204] pnp 00:0a: [io  0x0500-0x053f]
[    0.364206] pnp 00:0a: [mem 0xfec00000-0xfec00fff]
[    0.364208] pnp 00:0a: [mem 0xfee00000-0xfee00fff]
[    0.364210] pnp 00:0a: [mem 0xfed1c000-0xfed1ffff]
[    0.364212] pnp 00:0a: [mem 0xffb00000-0xffbfffff]
[    0.364214] pnp 00:0a: [mem 0xfc800400-0xfc800fff]
[    0.364334] system 00:0a: [io  0x0400-0x047f] has been reserved
[    0.364338] system 00:0a: [io  0xefa0-0xefaf] has been reserved
[    0.364341] system 00:0a: [io  0x0500-0x053f] has been reserved
[    0.364344] system 00:0a: [mem 0xfec00000-0xfec00fff] could not be reserved
[    0.364347] system 00:0a: [mem 0xfee00000-0xfee00fff] has been reserved
[    0.364350] system 00:0a: [mem 0xfed1c000-0xfed1ffff] has been reserved
[    0.364353] system 00:0a: [mem 0xffb00000-0xffbfffff] has been reserved
[    0.364356] system 00:0a: [mem 0xfc800400-0xfc800fff] has been reserved
[    0.364360] system 00:0a: Plug and Play ACPI device, IDs PNP0c01 (active)
[    0.364550] pnp: PnP ACPI: found 11 devices
[    0.364553] ACPI: ACPI bus type pnp unregistered
[    0.371052] PCI: max bus depth: 1 pci_try_num: 2
[    0.371127] pci 0000:00:1c.4: BAR 15: assigned [mem 0xd8300000-0xd84fffff 64bit pref]
[    0.371132] pci 0000:00:1c.3: BAR 15: assigned [mem 0xd8500000-0xd86fffff 64bit pref]
[    0.371135] pci 0000:00:1c.2: BAR 15: assigned [mem 0xd8700000-0xd88fffff 64bit pref]
[    0.371139] pci 0000:00:1c.0: BAR 15: assigned [mem 0xd8900000-0xd8afffff 64bit pref]
[    0.371143] pci 0000:00:01.0: BAR 15: assigned [mem 0xd8b00000-0xd8cfffff 64bit pref]
[    0.371146] pci 0000:00:01.0: PCI bridge to [bus 01-01]
[    0.371149] pci 0000:00:01.0:   bridge window [io  0x5000-0x5fff]
[    0.371154] pci 0000:00:01.0:   bridge window [mem 0xc0000000-0xd30fffff]
[    0.371157] pci 0000:00:01.0:   bridge window [mem 0xd8b00000-0xd8cfffff 64bit pref]
[    0.371162] pci 0000:00:1c.0: PCI bridge to [bus 02-02]
[    0.371166] pci 0000:00:1c.0:   bridge window [io  0x4000-0x4fff]
[    0.371173] pci 0000:00:1c.0:   bridge window [mem 0xd6d00000-0xd80fffff]
[    0.371178] pci 0000:00:1c.0:   bridge window [mem 0xd8900000-0xd8afffff 64bit pref]
[    0.371186] pci 0000:00:1c.2: PCI bridge to [bus 03-03]
[    0.371190] pci 0000:00:1c.2:   bridge window [io  0x3000-0x3fff]
[    0.371197] pci 0000:00:1c.2:   bridge window [mem 0xd5900000-0xd6cfffff]
[    0.371202] pci 0000:00:1c.2:   bridge window [mem 0xd8700000-0xd88fffff 64bit pref]
[    0.371211] pci 0000:00:1c.3: PCI bridge to [bus 04-04]
[    0.371214] pci 0000:00:1c.3:   bridge window [io  0x2000-0x2fff]
[    0.371221] pci 0000:00:1c.3:   bridge window [mem 0xd4500000-0xd58fffff]
[    0.371226] pci 0000:00:1c.3:   bridge window [mem 0xd8500000-0xd86fffff 64bit pref]
[    0.371234] pci 0000:00:1c.4: PCI bridge to [bus 05-05]
[    0.371238] pci 0000:00:1c.4:   bridge window [io  0x1000-0x1fff]
[    0.371245] pci 0000:00:1c.4:   bridge window [mem 0xd3100000-0xd44fffff]
[    0.371250] pci 0000:00:1c.4:   bridge window [mem 0xd8300000-0xd84fffff 64bit pref]
[    0.371260] pci 0000:00:1e.0: PCI bridge to [bus 06-06]
[    0.371268] pci 0000:00:1e.0:   bridge window [mem 0xd8100000-0xd81fffff]
[    0.371299] pci 0000:00:01.0: PCI INT A -> GSI 16 (level, low) -> IRQ 16
[    0.371304] pci 0000:00:01.0: setting latency timer to 64
[    0.371312] pci 0000:00:1c.0: PCI INT A -> GSI 16 (level, low) -> IRQ 16
[    0.371317] pci 0000:00:1c.0: setting latency timer to 64
[    0.371329] pci 0000:00:1c.2: PCI INT C -> GSI 18 (level, low) -> IRQ 18
[    0.371334] pci 0000:00:1c.2: setting latency timer to 64
[    0.371345] pci 0000:00:1c.3: PCI INT D -> GSI 19 (level, low) -> IRQ 19
[    0.371350] pci 0000:00:1c.3: setting latency timer to 64
[    0.371358] pci 0000:00:1c.4: PCI INT A -> GSI 16 (level, low) -> IRQ 16
[    0.371364] pci 0000:00:1c.4: setting latency timer to 64
[    0.371373] pci 0000:00:1e.0: setting latency timer to 64
[    0.371378] pci_bus 0000:00: resource 4 [io  0x0000-0x0cf7]
[    0.371380] pci_bus 0000:00: resource 5 [io  0x0d00-0xffff]
[    0.371383] pci_bus 0000:00: resource 6 [mem 0x000a0000-0x000bffff]
[    0.371385] pci_bus 0000:00: resource 7 [mem 0xc0000000-0xe0203fff]
[    0.371388] pci_bus 0000:01: resource 0 [io  0x5000-0x5fff]
[    0.371391] pci_bus 0000:01: resource 1 [mem 0xc0000000-0xd30fffff]
[    0.371394] pci_bus 0000:01: resource 2 [mem 0xd8b00000-0xd8cfffff 64bit pref]
[    0.371398] pci_bus 0000:02: resource 0 [io  0x4000-0x4fff]
[    0.371401] pci_bus 0000:02: resource 1 [mem 0xd6d00000-0xd80fffff]
[    0.371404] pci_bus 0000:02: resource 2 [mem 0xd8900000-0xd8afffff 64bit pref]
[    0.371408] pci_bus 0000:03: resource 0 [io  0x3000-0x3fff]
[    0.371411] pci_bus 0000:03: resource 1 [mem 0xd5900000-0xd6cfffff]
[    0.371414] pci_bus 0000:03: resource 2 [mem 0xd8700000-0xd88fffff 64bit pref]
[    0.371417] pci_bus 0000:04: resource 0 [io  0x2000-0x2fff]
[    0.371420] pci_bus 0000:04: resource 1 [mem 0xd4500000-0xd58fffff]
[    0.371424] pci_bus 0000:04: resource 2 [mem 0xd8500000-0xd86fffff 64bit pref]
[    0.371427] pci_bus 0000:05: resource 0 [io  0x1000-0x1fff]
[    0.371430] pci_bus 0000:05: resource 1 [mem 0xd3100000-0xd44fffff]
[    0.371434] pci_bus 0000:05: resource 2 [mem 0xd8300000-0xd84fffff 64bit pref]
[    0.371438] pci_bus 0000:06: resource 1 [mem 0xd8100000-0xd81fffff]
[    0.371441] pci_bus 0000:06: resource 4 [io  0x0000-0x0cf7]
[    0.371444] pci_bus 0000:06: resource 5 [io  0x0d00-0xffff]
[    0.371447] pci_bus 0000:06: resource 6 [mem 0x000a0000-0x000bffff]
[    0.371451] pci_bus 0000:06: resource 7 [mem 0xc0000000-0xe0203fff]
[    0.371502] NET: Registered protocol family 2
[    0.371659] IP route cache hash table entries: 131072 (order: 8, 1048576 bytes)
[    0.373172] TCP established hash table entries: 524288 (order: 11, 8388608 bytes)
[    0.379884] TCP bind hash table entries: 65536 (order: 8, 1048576 bytes)
[    0.380805] TCP: Hash tables configured (established 524288 bind 65536)
[    0.380808] TCP reno registered
[    0.380821] UDP hash table entries: 2048 (order: 4, 65536 bytes)
[    0.380877] UDP-Lite hash table entries: 2048 (order: 4, 65536 bytes)
[    0.381068] NET: Registered protocol family 1
[    0.381108] pci 0000:00:1a.0: PCI INT A -> GSI 16 (level, low) -> IRQ 16
[    0.381129] pci 0000:00:1a.0: PCI INT A disabled
[    0.381149] pci 0000:00:1a.1: PCI INT B -> GSI 21 (level, low) -> IRQ 21
[    0.381170] pci 0000:00:1a.1: PCI INT B disabled
[    0.381181] pci 0000:00:1a.7: PCI INT C -> GSI 18 (level, low) -> IRQ 18
[    0.381318] pci 0000:00:1a.7: PCI INT C disabled
[    0.381344] pci 0000:00:1d.0: PCI INT A -> GSI 23 (level, low) -> IRQ 23
[    0.381364] pci 0000:00:1d.0: PCI INT A disabled
[    0.381373] pci 0000:00:1d.1: PCI INT B -> GSI 19 (level, low) -> IRQ 19
[    0.381393] pci 0000:00:1d.1: PCI INT B disabled
[    0.381401] pci 0000:00:1d.2: PCI INT C -> GSI 18 (level, low) -> IRQ 18
[    0.381422] pci 0000:00:1d.2: PCI INT C disabled
[    0.381433] pci 0000:00:1d.7: PCI INT A -> GSI 23 (level, low) -> IRQ 23
[    0.381553] pci 0000:00:1d.7: PCI INT A disabled
[    0.381590] pci 0000:01:00.0: Boot video device
[    0.381615] PCI: CLS 64 bytes, default 64
[    0.382028] audit: initializing netlink socket (disabled)
[    0.382042] type=2000 audit(1360672900.376:1): initialized
[    0.405507] HugeTLB registered 2 MB page size, pre-allocated 0 pages
[    0.407965] VFS: Disk quotas dquot_6.5.2
[    0.408051] Dquot-cache hash table entries: 512 (order 0, 4096 bytes)
[    0.408624] fuse init (API version 7.17)
[    0.408718] msgmni has been set to 5985
[    0.409074] Block layer SCSI generic (bsg) driver version 0.4 loaded (major 253)
[    0.409104] io scheduler noop registered
[    0.409106] io scheduler deadline registered
[    0.409140] io scheduler cfq registered (default)
[    0.409286] pcieport 0000:00:01.0: setting latency timer to 64
[    0.409327] pcieport 0000:00:01.0: irq 40 for MSI/MSI-X
[    0.409381] pcieport 0000:00:1c.0: setting latency timer to 64
[    0.409437] pcieport 0000:00:1c.0: irq 41 for MSI/MSI-X
[    0.409521] pcieport 0000:00:1c.2: setting latency timer to 64
[    0.409579] pcieport 0000:00:1c.2: irq 42 for MSI/MSI-X
[    0.409660] pcieport 0000:00:1c.3: setting latency timer to 64
[    0.409716] pcieport 0000:00:1c.3: irq 43 for MSI/MSI-X
[    0.409805] pcieport 0000:00:1c.4: setting latency timer to 64
[    0.409862] pcieport 0000:00:1c.4: irq 44 for MSI/MSI-X
[    0.409966] pci_hotplug: PCI Hot Plug PCI Core version: 0.5
[    0.409992] pciehp: PCI Express Hot Plug Controller Driver version: 0.4
[    0.410061] intel_idle: MWAIT substates: 0x22220
[    0.410063] intel_idle: does not run on family 6 model 15
[    0.424050] ACPI: Deprecated procfs I/F for AC is loaded, please retry with CONFIG_ACPI_PROCFS_POWER cleared
[    0.440067] ACPI: AC Adapter [ADP1] (on-line)
[    0.440186] input: Lid Switch as /devices/LNXSYSTM:00/device:00/PNP0A08:00/device:0b/PNP0C09:00/PNP0C0D:00/input/input0
[    0.448162] Freeing initrd memory: 13888k freed
[    0.456100] ACPI: Lid Switch [LID0]
[    0.456227] input: Power Button as /devices/LNXSYSTM:00/device:00/PNP0C0C:00/input/input1
[    0.456234] ACPI: Power Button [PWRB]
[    0.456282] input: Sleep Button as /devices/LNXSYSTM:00/device:00/PNP0C0E:00/input/input2
[    0.456285] ACPI: Sleep Button [SLPB]
[    0.456335] input: Power Button as /devices/LNXSYSTM:00/LNXPWRBN:00/input/input3
[    0.456338] ACPI: Power Button [PWRF]
[    0.457903] Monitor-Mwait will be used to enter C-1 state
[    0.457909] Monitor-Mwait will be used to enter C-2 state
[    0.457913] Marking TSC unstable due to TSC halts in idle
[    0.457919] ACPI: acpi_idle registered with cpuidle
[    0.536049] thermal LNXTHERM:00: registered as thermal_zone0
[    0.536052] ACPI: Thermal Zone [THRM] (57 C)
[    0.536078] ACPI: Deprecated procfs I/F for battery is loaded,

 please retry with CONFIG_ACPI_PROCFS_POWER cleared
[    0.536086] ACPI: Battery Slot [BAT1] (battery absent)
[    0.536114] ERST: Table is not found!
[    0.536116] GHES: HEST is not enabled!
[    0.536252] Serial: 8250/16550 driver, 32 ports, IRQ sharing enabled
[    0.552030] ACPI: Battery Slot [BAT1] (battery absent)
[    0.612327] Linux agpgart interface v0.103
[    0.614105] brd: module loaded
[    0.614977] loop: module loaded
[    0.615128] ahci 0000:00:1f.2: version 3.0
[    0.615138] ahci 0000:00:1f.2: enabling device (0005 -> 0007)
[    0.615157] ahci 0000:00:1f.2: PCI INT B -> GSI 17 (level, low) -> IRQ 17
[    0.615215] ahci 0000:00:1f.2: irq 45 for MSI/MSI-X
[    0.615292] ahci 0000:00:1f.2: AHCI 0001.0100 32 slots 3 ports 3 Gbps 0x7 impl SATA mode
[    0.615296] ahci 0000:00:1f.2: flags: 64bit ncq sntf pm led clo pio slum part ccc ems 
[    0.615302] ahci 0000:00:1f.2: setting latency timer to 64
[    0.628358] scsi0 : ahci
[    0.628461] scsi1 : ahci
[    0.628549] scsi2 : ahci
[    0.628601] ata1: SATA max UDMA/133 abar m2048@0xd8204000 port 0xd8204100 irq 45
[    0.628605] ata2: SATA max UDMA/133 abar m2048@0xd8204000 port 0xd8204180 irq 45
[    0.628609] ata3: SATA max UDMA/133 abar m2048@0xd8204000 port 0xd8204200 irq 45
[    0.628680] ata_piix 0000:00:1f.1: version 2.13
[    0.628692] ata_piix 0000:00:1f.1: PCI INT A -> GSI 16 (level, low) -> IRQ 16
[    0.628733] ata_piix 0000:00:1f.1: setting latency timer to 64
[    0.629048] scsi3 : ata_piix
[    0.629134] scsi4 : ata_piix
[    0.630027] ata4: PATA max UDMA/100 cmd 0x6160 ctl 0x6150 bmdma 0x6120 irq 16
[    0.630030] ata5: PATA max UDMA/100 cmd 0x6140 ctl 0x6130 bmdma 0x6128 irq 16
[    0.630416] Fixed MDIO Bus: probed
[    0.630436] tun: Universal TUN/TAP device driver, 1.6
[    0.630438] tun: (C) 1999-2004 Max Krasnyansky <maxk@qualcomm.com>
[    0.630599] PPP generic driver version 2.4.2
[    0.630722] ehci_hcd: USB 2.0 'Enhanced' Host Controller (EHCI) Driver
[    0.630741] ehci_hcd 0000:00:1a.7: PCI INT C -> GSI 18 (level, low) -> IRQ 18
[    0.630760] ehci_hcd 0000:00:1a.7: setting latency timer to 64
[    0.630764] ehci_hcd 0000:00:1a.7: EHCI Host Controller
[    0.630820] ehci_hcd 0000:00:1a.7: new USB bus registered, assigned bus number 1
[    0.630856] ehci_hcd 0000:00:1a.7: debug port 1
[    0.634734] ehci_hcd 0000:00:1a.7: cache line size of 64 is not supported
[    0.634751] ehci_hcd 0000:00:1a.7: irq 18, io mem 0xd8204c00
[    0.648019] ehci_hcd 0000:00:1a.7: USB 2.0 started, EHCI 1.00
[    0.648188] hub 1-0:1.0: USB hub found
[    0.648193] hub 1-0:1.0: 4 ports detected
[    0.648269] ehci_hcd 0000:00:1d.7: PCI INT A -> GSI 23 (level, low) -> IRQ 23
[    0.648284] ehci_hcd 0000:00:1d.7: setting latency timer to 64
[    0.648287] ehci_hcd 0000:00:1d.7: EHCI Host Controller
[    0.648336] ehci_hcd 0000:00:1d.7: new USB bus registered, assigned bus number 2
[    0.648369] ehci_hcd 0000:00:1d.7: debug port 1
[    0.652254] ehci_hcd 0000:00:1d.7: cache line size of 64 is not supported
[    0.652268] ehci_hcd 0000:00:1d.7: irq 23, io mem 0xd8204800
[    0.668020] ehci_hcd 0000:00:1d.7: USB 2.0 started, EHCI 1.00
[    0.668140] hub 2-0:1.0: USB hub found
[    0.668144] hub 2-0:1.0: 6 ports detected
[    0.668225] ohci_hcd: USB 1.1 'Open' Host Controller (OHCI) Driver
[    0.668242] uhci_hcd: USB Universal Host Controller Interface driver
[    0.668260] uhci_hcd 0000:00:1a.0: PCI INT A -> GSI 16 (level, low) -> IRQ 16
[    0.668268] uhci_hcd 0000:00:1a.0: setting latency timer to 64
[    0.668272] uhci_hcd 0000:00:1a.0: UHCI Host Controller
[    0.668320] uhci_hcd 0000:00:1a.0: new USB bus registered, assigned bus number 3
[    0.668349] uhci_hcd 0000:00:1a.0: irq 16, io base 0x000060c0
[    0.668485] hub 3-0:1.0: USB hub found
[    0.668490] hub 3-0:1.0: 2 ports detected
[    0.668563] uhci_hcd 0000:00:1a.1: PCI INT B -> GSI 21 (level, low) -> IRQ 21
[    0.668571] uhci_hcd 0000:00:1a.1: setting latency timer to 64
[    0.668575] uhci_hcd 0000:00:1a.1: UHCI Host Controller
[    0.668631] uhci_hcd 0000:00:1a.1: new USB bus registered, assigned bus number 4
[    0.668669] uhci_hcd 0000:00:1a.1: irq 21, io base 0x000060a0
[    0.668803] hub 4-0:1.0: USB hub found
[    0.668807] hub 4-0:1.0: 2 ports detected
[    0.668882] uhci_hcd 0000:00:1d.0: PCI INT A -> GSI 23 (level, low) -> IRQ 23
[    0.668890] uhci_hcd 0000:00:1d.0: setting latency timer to 64
[    0.668894] uhci_hcd 0000:00:1d.0: UHCI Host Controller
[    0.668943] uhci_hcd 0000:00:1d.0: new USB bus registered, assigned bus number 5
[    0.668973] uhci_hcd 0000:00:1d.0: irq 23, io base 0x00006080
[    0.669120] hub 5-0:1.0: USB hub found
[    0.669124] hub 5-0:1.0: 2 ports detected
[    0.669197] uhci_hcd 0000:00:1d.1: PCI INT B -> GSI 19 (level, low) -> IRQ 19
[    0.669205] uhci_hcd 0000:00:1d.1: setting latency timer to 64
[    0.669209] uhci_hcd 0000:00:1d.1: UHCI Host Controller
[    0.669263] uhci_hcd 0000:00:1d.1: new USB bus registered, assigned bus number 6
[    0.669301] uhci_hcd 0000:00:1d.1: irq 19, io base 0x00006060
[    0.669435] hub 6-0:1.0: USB hub found
[    0.669439] hub 6-0:1.0: 2 ports detected
[    0.669510] uhci_hcd 0000:00:1d.2: PCI INT C -> GSI 18 (level, low) -> IRQ 18
[    0.669518] uhci_hcd 0000:00:1d.2: setting latency timer to 64
[    0.669522] uhci_hcd 0000:00:1d.2: UHCI Host Controller
[    0.669568] uhci_hcd 0000:00:1d.2: new USB bus registered, assigned bus number 7
[    0.669598] uhci_hcd 0000:00:1d.2: irq 18, io base 0x00006040
[    0.669735] hub 7-0:1.0: USB hub found
[    0.669739] hub 7-0:1.0: 2 ports detected
[    0.669861] usbcore: registered new interface driver libusual
[    0.669902] i8042: PNP: PS/2 Controller [PNP0303:PS2K,PNP0f03:PS2M] at 0x60,0x64 irq 1,12
[    0.684497] serio: i8042 KBD port at 0x60,0x64 irq 1
[    0.684503] serio: i8042 AUX port at 0x60,0x64 irq 12
[    0.684648] mousedev: PS/2 mouse device common for all mice
[    0.685628] rtc_cmos 00:03: RTC can wake from S4
[    0.685769] rtc_cmos 00:03: rtc core: registered rtc_cmos as rtc0
[    0.685801] rtc0: alarms up to one year, y3k, 114 bytes nvram, hpet irqs
[    0.685894] device-mapper: uevent: version 1.0.3
[    0.685976] device-mapper: ioctl: 4.22.0-ioctl (2011-10-19) initialised: dm-devel@redhat.com
[    0.686031] cpuidle: using governor ladder
[    0.686102] cpuidle: using governor menu
[    0.686104] EFI Variables Facility v0.08 2004-May-17
[    0.686365] TCP cubic registered
[    0.686494] NET: Registered protocol family 10
[    0.686986] NET: Registered protocol family 17
[    0.686991] Registering the dns_resolver key type
[    0.687163] PM: Hibernation image not present or could not be loaded.
[    0.687177] registered taskstats version 1
[    0.694380]   Magic number: 1:281:683
[    0.694521] rtc_cmos 00:03: setting system clock to 2013-02-12 12:41:40 UTC (1360672900)
[    0.696103] BIOS EDD facility v0.16 2004-Jun-25, 0 devices found
[    0.696105] EDD information not available.
[    0.697542] input: AT Translated Set 2 keyboard as /devices/platform/i8042/serio0/input/input4
[    0.795888] ata4.00: ATAPI: Optiarc DVD RW AD-7580A, ZX08, max UDMA/33
[    0.812373] ata4.00: configured for UDMA/33
[    0.948048] ata3: SATA link down (SStatus 0 SControl 300)
[    0.948079] ata2: SATA link down (SStatus 0 SControl 300)
[    0.948115] ata1: SATA link up 1.5 Gbps (SStatus 113 SControl 300)
[    1.004462] ata1.00: ATA-8: WDC WD2500BEVS-22UST0, 01.01A01, max UDMA/133
[    1.004468] ata1.00: 488397168 sectors, multi 16: LBA48 NCQ (depth 31/32), AA
[    1.005375] ata1.00: configured for UDMA/133
[    1.005519] scsi 0:0:0:0: Direct-Access     ATA      WDC WD2500BEVS-2 01.0 PQ: 0 ANSI: 5
[    1.005651] sd 0:0:0:0: [sda] 488397168 512-byte logical blocks: (250 GB/232 GiB)
[    1.005670] sd 0:0:0:0: Attached scsi generic sg0 type 0
[    1.005703] sd 0:0:0:0: [sda] Write Protect is off
[    1.005706] sd 0:0:0:0: [sda] Mode Sense: 00 3a 00 00
[    1.005734] sd 0:0:0:0: [sda] Write cache: enabled, read cache: enabled, doesn't support DPO or FUA
[    1.006823] scsi 3:0:0:0: CD-ROM            Optiarc  DVD RW AD-7580A  ZX08 PQ: 0 ANSI: 5
[    1.010553] sr0: scsi3-mmc drive: 24x/24x writer dvd-ram cd/rw xa/form2 cdda tray
[    1.010559] cdrom: Uniform CD-ROM driver Revision: 3.20
[    1.010754] sr 3:0:0:0: Attached scsi CD-ROM sr0
[    1.010891] sr 3:0:0:0: Attached scsi generic sg1 type 5
[    1.013531]  sda: sda1
[    1.013913] sd 0:0:0:0: [sda] Attached SCSI disk
[    1.015578] Freeing unused kernel memory: 924k freed
[    1.015918] Write protecting the kernel read-only data: 12288k
[    1.021580] Freeing unused kernel memory: 1604k freed
[    1.026352] Freeing unused kernel memory: 1196k freed
[    1.042913] udevd[95]: starting version 175
[    1.086875] sata_sil24 0000:03:00.0: version 1.1
[    1.086899] sata_sil24 0000:03:00.0: PCI INT A -> GSI 18 (level, low) -> IRQ 18
[    1.086962] sata_sil24 0000:03:00.0: setting latency timer to 64
[    1.097070] scsi5 : sata_sil24
[    1.097167] ata6: SATA max UDMA/100 host m128@0xd5902000 port 0xd5900000 irq 18
[    1.098923] r8169 Gigabit Ethernet driver 2.3LK-NAPI loaded
[    1.098949] r8169 0000:05:00.0: PCI INT A -> GSI 16 (level, low) -> IRQ 16
[    1.098989] r8169 0000:05:00.0: setting latency timer to 64
[    1.100778] r8169 0000:05:00.0: irq 46 for MSI/MSI-X
[    1.101252] r8169 0000:05:00.0: eth0: RTL8168b/8111b at 0xffffc90000654000, 00:19:db:ee:c7:b9, XID 18000000 IRQ 46
[    1.101256] r8169 0000:05:00.0: eth0: jumbo features [frames: 4080 bytes, tx checksumming: ko]
[    1.120741] sdhci: Secure Digital Host Controller Interface driver
[    1.120744] sdhci: Copyright(c) Pierre Ossman
[    1.204046] usb 3-2: new low-speed USB device number 2 using uhci_hcd
[    1.292087] EXT4-fs (sda1): mounted filesystem with ordered data mode. Opts: (null)
[    1.640116] usb 7-1: new low-speed USB device number 2 using uhci_hcd
[  

  3.176057] ata6: SATA link down (SStatus 0 SControl 0)
[    3.176713] sdhci-pci 0000:06:04.1: SDHCI controller found [1180:0822] (rev 22)
[    3.176735] sdhci-pci 0000:06:04.1: PCI INT B -> GSI 17 (level, low) -> IRQ 17
[    3.177760] sdhci-pci 0000:06:04.1: Will use DMA mode even though HW doesn't fully claim to support it.
[    3.177792] mmc0: no vmmc regulator found
[    3.178816] Registered led device: mmc0::
[    3.180854] mmc0: SDHCI controller on PCI [0000:06:04.1] using DMA
[    3.180942] firewire_ohci 0000:06:04.0: PCI INT A -> GSI 16 (level, low) -> IRQ 16
[    3.244084] firewire_ohci: Added fw-ohci device 0000:06:04.0, OHCI v1.10, 4 IR + 4 IT contexts, quirks 0x11
[    3.744214] firewire_core: created device fw0: GUID 00cd0100ac4e3310, S400
[   15.900885] ADDRCONF(NETDEV_UP): eth0: link is not ready
[   15.939369] EXT4-fs (sda1): re-mounted. Opts: errors=remount-ro
[   15.959074] udevd[348]: starting version 175
[   16.080484] lp: driver loaded but no devices found
[   16.109347] cfg80211: Calling CRDA to update world regulatory domain
[   16.165831] ene_ir: chip is 0x3909 - kbver = 0x24, rev = 0xc0
[   16.165835] ene_ir: PLL freq = 1406
[   16.165837] ene_ir: KB3926B detected
[   16.168463] iwl4965: Intel(R) Wireless WiFi 4965 driver for Linux, in-tree:
[   16.168466] iwl4965: Copyright(c) 2003-2011 Intel Corporation
[   16.168547] iwl4965 0000:02:00.0: PCI INT A -> GSI 16 (level, low) -> IRQ 16
[   16.168560] iwl4965 0000:02:00.0: setting latency timer to 64
[   16.168595] iwl4965 0000:02:00.0: Detected Intel(R) Wireless WiFi Link 4965AGN, REV=0x4
[   16.171495] IR NEC protocol handler initialized
[   16.202508] input: HID 046a:0011 as /devices/pci0000:00/0000:00:1a.0/usb3/3-2/3-2:1.0/input/input5
[   16.211164] iwl4965 0000:02:00.0: device EEPROM VER=0x36, CALIB=0x5
[   16.212140] Registered IR keymap rc-rc6-mce
[   16.212314] input: ENE eHome Infrared Remote Receiver as /devices/virtual/rc/rc0/input6
[   16.216954] rc0: ENE eHome Infrared Remote Receiver as /devices/virtual/rc/rc0
[   16.217031] generic-usb 0003:046A:0011.0001: input,hidraw0: USB HID v1.11 Keyboard [HID 046a:0011] on usb-0000:00:1a.0-2/input0
[   16.221274] ene_ir: driver has been successfully loaded
[   16.221825] iwl4965 0000:02:00.0: Tunable channels: 13 802.11bg, 19 802.11a channels
[   16.221917] iwl4965 0000:02:00.0: irq 47 for MSI/MSI-X
[   16.222484] atkbd serio0: Unknown key pressed (translated set 2, code 0xf8 on isa0060/serio0).
[   16.222489] atkbd serio0: Use 'setkeycodes e078 <keycode>' to make it known.
[   16.225350] atkbd serio0: Unknown key released (translated set 2, code 0xf8 on isa0060/serio0).
[   16.225355] atkbd serio0: Use 'setkeycodes e078 <keycode>' to make it known.
[   16.226598] IR RC5(x) protocol handler initialized
[   16.230693] IR RC6 protocol handler initialized
[   16.234241] input: Logitech USB Laser Mouse as /devices/pci0000:00/0000:00:1d.2/usb7/7-1/7-1:1.0/input/input7
[   16.234479] generic-usb 0003:046D:C069.0002: input,hidraw1: USB HID v1.10 Mouse [Logitech USB Laser Mouse] on usb-0000:00:1d.2-1/input0
[   16.234527] usbcore: registered new interface driver usbhid
[   16.234529] usbhid: USB HID core driver
[   16.238862] IR JVC protocol handler initialized
[   16.242688] atkbd serio0: Unknown key pressed (translated set 2, code 0xf8 on isa0060/serio0).
[   16.242693] atkbd serio0: Use 'setkeycodes e078 <keycode>' to make it known.
[   16.243574] IR Sony protocol handler initialized
[   16.245445] atkbd serio0: Unknown key released (translated set 2, code 0xf8 on isa0060/serio0).
[   16.245450] atkbd serio0: Use 'setkeycodes e078 <keycode>' to make it known.
[   16.247052] input: MCE IR Keyboard/Mouse (ene_ir) as /devices/virtual/input/input8
[   16.247246] IR MCE Keyboard/mouse protocol handler initialized
[   16.252285] acpi device:03: registered as cooling_device2
[   16.252375] input: Video Bus as /devices/LNXSYSTM:00/device:00/PNP0A08:00/device:01/LNXVIDEO:00/input/input9
[   16.252490] ACPI: Video Device [NVGA] (multi-head: yes  rom: no  post: no)
[   16.258162] lirc_dev: IR Remote Control driver registered, major 249 
[   16.258415] rc rc0: lirc_dev: driver ir-lirc-codec (ene_ir) registered at minor = 0
[   16.258418] IR LIRC bridge handler initialized
[   16.262549] snd_hda_intel 0000:00:1b.0: PCI INT A -> GSI 22 (level, low) -> IRQ 22
[   16.262625] snd_hda_intel 0000:00:1b.0: irq 48 for MSI/MSI-X
[   16.262661] snd_hda_intel 0000:00:1b.0: setting latency timer to 64
[   16.271959] r592 0000:06:04.2: PCI INT B -> GSI 17 (level, low) -> IRQ 17
[   16.273587] r592: driver successfully loaded
[   16.351859] hda_codec: ALC888: BIOS auto-probing.
[   16.351864] hda_codec: ALC888: SKU not ready 0x598301f0
[   16.381963] input: HDA Intel Line as /devices/pci0000:00/0000:00:1b.0/sound/card0/input10
[   16.392919] input: HDA Intel Mic as /devices/pci0000:00/0000:00:1b.0/sound/card0/input11
[   16.393592] input: HDA Intel Headphone as /devices/pci0000:00/0000:00:1b.0/sound/card0/input12
[   16.398684] cfg80211: World regulatory domain updated:
[   16.398688] cfg80211:     (start_freq - end_freq @ bandwidth), (max_antenna_gain, max_eirp)
[   16.398691] cfg80211:     (2402000 KHz - 2472000 KHz @ 40000 KHz), (300 mBi, 2000 mBm)
[   16.398694] cfg80211:     (2457000 KHz - 2482000 KHz @ 20000 KHz), (300 mBi, 2000 mBm)
[   16.398697] cfg80211:     (2474000 KHz - 2494000 KHz @ 20000 KHz), (300 mBi, 2000 mBm)
[   16.398699] cfg80211:     (5170000 KHz - 5250000 KHz @ 40000 KHz), (300 mBi, 2000 mBm)
[   16.398702] cfg80211:     (5735000 KHz - 5835000 KHz @ 40000 KHz), (300 mBi, 2000 mBm)
[   16.401749] type=1400 audit(1360672916.204:2): apparmor="STATUS" operation="profile_load" name="/sbin/dhclient" pid=568 comm="apparmor_parser"
[   16.402179] type=1400 audit(1360672916.204:3): apparmor="STATUS" operation="profile_load" name="/usr/lib/NetworkManager/nm-dhcp-client.action" pid=568 comm="apparmor_parser"
[   16.402423] type=1400 audit(1360672916.204:4): apparmor="STATUS" operation="profile_load" name="/usr/lib/connman/scripts/dhclient-script" pid=568 comm="apparmor_parser"
[   16.403866] type=1400 audit(1360672916.204:5): apparmor="STATUS" operation="profile_replace" name="/sbin/dhclient" pid=607 comm="apparmor_parser"
[   16.404345] type=1400 audit(1360672916.208:6): apparmor="STATUS" operation="profile_replace" name="/usr/lib/NetworkManager/nm-dhcp-client.action" pid=607 comm="apparmor_parser"
[   16.404589] type=1400 audit(1360672916.208:7): apparmor="STATUS" operation="profile_replace" name="/usr/lib/connman/scripts/dhclient-script" pid=607 comm="apparmor_parser"
[   16.471027] iwl4965 0000:02:00.0: loaded firmware version 228.61.2.24
[   16.471265] Registered led device: phy0-led
[   16.471297] cfg80211: Ignoring regulatory request Set by core since the driver uses its own custom regulatory domain
[   16.478944] ieee80211 phy0: Selected rate control algorithm 'iwl-4965-rs'
[   16.500801] init: failsafe main process (714) killed by TERM signal
[   16.918232] ppdev: user-space parallel port driver
[   17.026696] type=1400 audit(1360672916.828:8): apparmor="STATUS" operation="profile_load" name="/usr/lib/cups/backend/cups-pdf" pid=797 comm="apparmor_parser"
[   17.028168] type=1400 audit(1360672916.832:9): apparmor="STATUS" operation="profile_load" name="/usr/sbin/cupsd" pid=797 comm="apparmor_parser"
[   17.029047] Bluetooth: Core ver 2.16
[   17.029561] NET: Registered protocol family 31
[   17.029564] Bluetooth: HCI device and connection manager initialized
[   17.029567] Bluetooth: HCI socket layer initialized
[   17.029569] Bluetooth: L2CAP socket layer initialized
[   17.029576] Bluetooth: SCO socket layer initialized
[   17.053412] Bluetooth: RFCOMM TTY layer initialized
[   17.053418] Bluetooth: RFCOMM socket layer initialized
[   17.053420] Bluetooth: RFCOMM ver 1.11
[   17.060953] Bluetooth: BNEP (Ethernet Emulation) ver 1.3
[   17.060957] Bluetooth: BNEP filters: protocol multicast
[   17.066928] type=1400 audit(1360672916.868:10): apparmor="STATUS" operation="profile_replace" name="/sbin/dhclient" pid=831 comm="apparmor_parser"
[   17.070580] type=1400 audit(1360672916.872:11): apparmor="STATUS" operation="profile_replace" name="/usr/lib/NetworkManager/nm-dhcp-client.action" pid=831 comm="apparmor_parser"
[   17.116236] psmouse serio1: synaptics: Touchpad model: 1, fw: 6.1, id: 0xa3a0b3, caps: 0xa04713/0x10008/0x0
[   17.128117] nvidia: module license 'NVIDIA' taints kernel.
[   17.128120] Disabling lock debugging due to kernel taint
[   17.367393] nvidia 0000:01:00.0: PCI INT A -> GSI 16 (level, low) -> IRQ 16
[   17.367405] nvidia 0000:01:00.0: setting latency timer to 64
[   17.367412] vgaarb: device changed decodes: PCI:0000:01:00.0,olddecodes=io+mem,decodes=none:owns=io+mem
[   17.367580] NVRM: loading NVIDIA UNIX x86_64 Kernel Module  295.40  Thu Apr  5 21:37:00 PDT 2012
[   17.411486] input: SynPS/2 Synaptics TouchPad as /devices/platform/i8042/serio1/input/input13
[   17.523833] ADDRCONF(NETDEV_UP): wlan0: link is not ready
[   17.527593] r8169 0000:05:00.0: eth0: link down
[   17.528170] ADDRCONF(NETDEV_UP): eth0: link is not ready
[   17.528443] ADDRCONF(NETDEV_UP): eth0: link is not ready
[   17.685368] vesafb: mode is 1680x1050x32, linelength=6720, pages=0
[   17.685371] vesafb: scrolling: redraw
[   17.685374] vesafb: Truecolor: size=8:8:8:8, shift=24:16:8:0
[   17.690049] vesafb: framebuffer at 0xd1000000, mapped to 0xffffc90011800000, using 6912k, total 6912k
[   17.690297] Console: switching to colour frame buffer device 210x65
[   17.690332] fb0: VESA VGA frame buffer device
[   20.401667] NVRM: RmInitAdapter failed! (0x27:0x28:1190)
[   20.401677] NVRM: rm_init_adapter(0) failed
[   20.513575] init: lightdm main process (1102) terminated with status 1
[   35.732827] init: failsafe-x main process (1127) terminated with status 1
[  140.801729] NVRM: RmInitAdapter failed!

 (0x27:0x28:1190)
[  140.801741] NVRM: rm_init_adapter(0) failed
[  188.312086] usb 2-6: new high-speed USB device number 3 using ehci_hcd
[  188.490737] Initializing USB Mass Storage driver...
[  188.490869] scsi6 : usb-storage 2-6:1.0
[  188.490948] usbcore: registered new interface driver usb-storage
[  188.490950] USB Mass Storage support registered.
[  188.503219] usbcore: registered new interface driver uas
[  189.490292] scsi 6:0:0:0: Direct-Access     Generic  Flash Disk       8.07 PQ: 0 ANSI: 2
[  189.492375] sd 6:0:0:0: Attached scsi generic sg2 type 0
[  189.493244] sd 6:0:0:0: [sdb] 3893248 512-byte logical blocks: (1.99 GB/1.85 GiB)
[  189.494081] sd 6:0:0:0: [sdb] Write Protect is off
[  189.494095] sd 6:0:0:0: [sdb] Mode Sense: 03 00 00 00
[  189.494608] sd 6:0:0:0: [sdb] No Caching mode page present
[  189.500924] sd 6:0:0:0: [sdb] Assuming drive cache: write through
[  189.508843] sd 6:0:0:0: [sdb] No Caching mode page present
[  189.511280] sd 6:0:0:0: [sdb] Assuming drive cache: write through
[  189.514728]  sdb: sdb1
[  189.516958] sd 6:0:0:0: [sdb] No Caching mode page present
[  189.519634] sd 6:0:0:0: [sdb] Assuming drive cache: write through
[  189.522257] sd 6:0:0:0: [sdb] Attached SCSI removable disk
[  876.089553] NVRM: RmInitAdapter failed! (0x27:0x28:1190)
[  876.089564] NVRM: rm_init_adapter(0) failed

