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Type DOR3 Channels # Dual
size [ 4096 ibyles DCMode [ Unganged

NB Frequency [ 20157 liHz

- Timings-

ORAl Frequency | 6718MHz

FopoRAM | 30

CAS# Latency (CL) | S0cbcks

RAS#to CAS#Delay (RCD) | Schocks
RAS# Precharge (RP) | 9 clocks.

CycleTime (RAS) | 24cocks

Bank Cyce Tme (RC) | 33clocks

Command Rate (CR) T
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[~ Timings Table

JEDEC#1 JEDEC#2 JEDEC# JEDEC#S
Frequency [ 457MHz | 533MHz | 6091z | 685 MAz
cAS#Latency | 60 70 50 S0

Commanarate [ [ [ [
Votage [ 150V | 150V | 150V | 180V
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