	HWiNFO64 v5.02-2575

	

	 
	
	
	
	

	Creation Time
	
	31.08.2015 11:01
	
	


	PETER-PC

	


	
	 
	

	[Current Computer] 

	
	Computer Name:
	PETER-PC 

	
	Computer Brand Name:
	MSI MS-7641 

	 
	
	

	[Operating System] 

	
	Operating System:
	Microsoft Windows 7 Home Premium (x64) Build 7601 

	
	Service Pack:
	Service Pack 1 

	
	UEFI Boot:
	Not Present 

	 
	
	


	Central Processor(s)

	


	
	 
	

	[CPU Unit Count] 

	
	Number Of Processor Packages (Physical):
	1 

	
	Number Of Processors Cores:
	8 

	
	Number Of Logical Processors:
	8 


	AMD FX-8120

	


	
	 
	

	[General Information] 

	
	Processor Name:
	AMD FX-8120 

	
	Original Processor Frequency:
	3100.0 MHz 

	
	Original Processor Frequency [MHz]:
	3100 

	 
	
	

	
	CPU ID:
	00600F12 

	
	Extended CPU ID:
	00600F12 

	
	CPU Brand Name:
	AMD FX(tm)-8120 Eight-Core Processor 

	
	CPU Vendor:
	AuthenticAMD 

	
	CPU Stepping:
	OR-B2 (Orochi) 

	
	CPU Code Name:
	Zambezi 

	
	CPU Thermal Design Power (TDP):
	95.1 W 

	
	CPU Platform:
	Socket AM3r2 

	
	Microcode Update Revision:
	6000629 

	 
	
	

	
	Number of CPU Cores:
	8 

	
	Number of Logical CPUs:
	8 

	 
	
	

	[Operating Points] 

	
	CPU HFM (Maximum):
	3100.0 MHz = 15.50 x 200.0 MHz [Unlimited] 

	
	CPU CPB:
	4000.0 MHz = 20.00 x 200.0 MHz [Unlimited] 

	
	CPU Current:
	2800.0 MHz = 14.00 x 200.0 MHz @ 1.1500 V 

	
	Northbridge Maximum:
	[Unlimited] 

	
	Northbridge Current:
	2200.0 MHz = 11.00 x 200.0 MHz @ 1.2250 V 

	 
	
	

	
	CPU Bus Type:
	Hyper-Transport v3.00 

	
	Maximum Supported Hyper-Transport Link Clock:
	3200 MHz 

	
	Current Hyper-Transport Link Clock:
	2200 MHz 

	 
	
	

	[Cache and TLB] 

	
	L1 Cache:
	Instruction: 4 x 64 KBytes, Data: 8 x 16 KBytes 

	
	L2 Cache:
	Integrated: 4 x 2 MBytes 

	
	L3 Cache:
	8 MBytes 

	
	Instruction TLB:
	Fully associative, 48 entries 

	
	Data TLB:
	Fully associative, 32 entries 

	 
	
	

	[Standard Feature Flags] 

	
	FPU on Chip
	Present 

	
	Enhanced Virtual-86 Mode
	Present 

	
	I/O Breakpoints
	Present 

	
	Page Size Extensions
	Present 

	
	Time Stamp Counter
	Present 

	
	Pentium-style Model Specific Registers
	Present 

	
	Physical Address Extension
	Present 

	
	Machine Check Exception
	Present 

	
	CMPXCHG8B Instruction
	Present 

	
	APIC On Chip / PGE (AMD)
	Present 

	
	Fast System Call
	Present 

	
	Memory Type Range Registers
	Present 

	
	Page Global Feature
	Present 

	
	Machine Check Architecture
	Present 

	
	CMOV Instruction
	Present 

	
	Page Attribute Table
	Present 

	
	36-bit Page Size Extensions
	Present 

	
	Processor Number
	Not Present 

	
	CLFLUSH Instruction
	Present 

	
	Debug Trace and EMON Store
	Not Present 

	
	Internal ACPI Support
	Not Present 

	
	MMX Technology
	Present 

	
	Fast FP Save/Restore (IA MMX-2)
	Present 

	
	Streaming SIMD Extensions
	Present 

	
	Streaming SIMD Extensions 2
	Present 

	
	Self-Snoop
	Not Present 

	
	Multi-Threading Capable
	Present 

	
	Automatic Clock Control
	Not Present 

	
	IA-64 Processor
	Not Present 

	
	Signal Break on FERR
	Not Present 

	
	Streaming SIMD Extensions 3
	Present 

	
	PCLMULQDQ Instruction Support
	Present 

	
	MONITOR/MWAIT Support
	Present 

	
	Supplemental Streaming SIMD Extensions 3
	Present 

	
	FMA Extension
	Not Present 

	
	CMPXCHG16B Support
	Present 

	
	Streaming SIMD Extensions 4.1
	Present 

	
	Streaming SIMD Extensions 4.2
	Present 

	
	x2APIC
	Not Present 

	
	POPCNT Instruction
	Present 

	
	AES Cryptography Support
	Present 

	
	XSAVE/XRSTOR/XSETBV/XGETBV Instructions
	Present 

	
	XGETBV/XSETBV OS Enabled
	Present 

	
	AVX Support
	Present 

	
	Half-Precision Convert (CVT16)
	Not Present 

	[Extended Feature Flags] 

	
	FPU on Chip
	Present 

	
	Enhanced Virtual-86 Mode
	Present 

	
	I/O Breakpoints
	Present 

	
	Page Size Extensions
	Present 

	
	Time Stamp Counter
	Present 

	
	AMD-style Model Specific Registers
	Present 

	
	Machine Check Exception
	Present 

	
	CMPXCHG8B Instruction
	Present 

	
	APIC On Chip
	Present 

	
	SYSCALL and SYSRET Instructions
	Present 

	
	Memory Type Range Registers
	Present 

	
	Page Global Feature
	Present 

	
	Machine Check Architecture
	Present 

	
	CMOV Instruction
	Present 

	
	Page Attribute Table
	Present 

	
	36-bit Page Size Extensions
	Present 

	
	Multi-Processing / Brand feature
	Not Present 

	
	No Execute
	Present 

	
	MMX Technology
	Present 

	
	MMX+ Extensions
	Present 

	
	Fast FP Save/Restore
	Present 

	
	Fast FP Save/Restore Optimizations
	Present 

	
	1 GB large page support
	Present 

	
	RDTSCP Instruction
	Present 

	
	x86-64 Long Mode
	Present 

	
	3DNow! Technology Extensions
	Not Present 

	
	3DNow! Technology
	Not Present 

	
	Read/Write FS/GS Base Instructions
	Not Present 

	
	TSC_THREAD_OFFSET
	Not Present 

	
	Software Guard Extensions (SGX) Support
	Not Present 

	
	Bit Manipulation Instructions Set 1
	Not Present 

	
	Hardware Lock Elision
	Not Present 

	
	AVX2 Instructions
	Not Present 

	
	Supervisor Mode Execution Protection
	Not Present 

	
	Bit Manipulation Instructions Set 2
	Not Present 

	
	Enhanced Performance String Instruction
	Not Present 

	
	INVPCID Instruction
	Not Present 

	
	Restricted Transactional Memory
	Not Present 

	
	Platform Quality of Service Monitoring (PQM)
	Not Present 

	
	Platform Quality of Service Enforcement (PQE)
	Not Present 

	
	Deprecated FPU CS and FPU DS
	Not Present 

	
	Memory Protection Extensions
	Not Present 

	
	Advanced Vector Extensions 512 (AVX-512)
	Not Present 

	
	AVX-512 Doubleword and Quadword Instructions
	Not Present 

	
	RDSEED Instruction
	Not Present 

	
	Multi-precision Add Carry Instructions
	Not Present 

	
	Supervisor Mode Access Prevention (SMAP)
	Not Present 

	
	AVX-512 52-bit Integer FMA Instructions
	Not Present 

	
	CLFLUSHOPT Instructions
	Not Present 

	
	Intel Processor Trace
	Not Present 

	
	AVX-512 Prefetch Instructions
	Not Present 

	
	AVX-512 Exponential and Reciprocal Instructions
	Not Present 

	
	AVX-512 Conflict Detection Instructions
	Not Present 

	
	Secure Hash Algorithm (SHA) Extensions
	Not Present 

	
	AVX-512 Byte and Word Instructions
	Not Present 

	
	AVX-512 Vector Length Extensions
	Not Present 

	
	PREFETCHWT1 Instruction
	Not Present 

	
	AVX-512 Vector Bit Manipulation Instructions
	Not Present 

	
	LAHF/SAHF Long Mode Support
	Present 

	
	Core Multi-Processing Legacy Mode
	Present 

	
	Secure Virtual Machine
	Present 

	
	Extended APIC Register Space
	Present 

	
	LOCK MOV CR0 Support
	Present 

	
	Advanced Bit Manipulation
	Present 

	
	SSE4A Support
	Present 

	
	Misaligned SSE Mode
	Present 

	
	PREFETCH(W) Support
	Present 

	
	OS Visible Work-around Support
	Present 

	
	Instruction Based Sampling
	Present 

	
	XOP Instruction Support
	Present 

	
	SKINIT, STGI, and DEV Support
	Present 

	
	Watchdog Timer Support
	Present 

	
	TBM0 Instruction Support
	Not Present 

	
	Lightweight Profiling Support
	Present 

	
	FMA4 Instruction Support
	Present 

	
	Translation Cache Extension
	Not Present 

	
	NodeId Support
	Present 

	
	Trailing Bit Manipulation
	Not Present 

	
	Topology Extensions
	Present 

	
	Core Performance Counter Extensions
	Present 

	
	NB Performance Counter Extensions
	Present 

	
	Streaming Performance Monitor Architecture
	Not Present 

	
	Data Breakpoint Extension
	Not Present 

	
	Performance Time-Stamp Counter
	Not Present 

	
	L2I Performance Counter Extensions
	Not Present 

	
	MWAITX/MONITORX Support
	Not Present 

	 
	
	

	[Enhanced Features] 

	
	Core Performance Boost
	Supported, Disabled 

	 
	
	

	[Memory Ranges] 

	
	Maximum Physical Address Size:
	48-bit (256 TBytes) 

	
	Maximum Virtual Address Size:
	48-bit (256 TBytes) 

	[MTRRs] 

	
	Range 0-80000000 (0MB-2048MB) Type:
	Write Back (WB) 

	
	Range 80000000-C0000000 (2048MB-3072MB) Type:
	Write Back (WB) 

	
	Range C0000000-D0000000 (3072MB-3328MB) Type:
	Write Back (WB) 


	Motherboard

	


	
	 
	

	[Computer] 

	
	Computer Brand Name:
	MSI MS-7641 

	 
	
	

	[Motherboard] 

	
	Motherboard Model:
	MSI 760GM-P23(FX) (MS-7641) 

	
	Motherboard Chipset:
	SB750/SB710 

	
	Motherboard Slots:
	1xPCI, 1xPCI Express x1, 1xPCI Express x16 

	
	PCI Express Version Supported:
	v2.0 

	
	USB Version Supported:
	v2.0 

	 
	
	

	[BIOS] 

	
	BIOS Manufacturer:
	American Megatrends 

	
	BIOS Date:
	04/28/13 

	
	BIOS Version:
	V17.15 

	
	UEFI BIOS:
	Not Capable 

	 
	
	

	
	Super-IO/LPC Chip:
	Fintek F71869A/F71868A/F71870A 


	ACPI Devices

	


	
	 
	


	AMD-Prozessor

	


	
	 
	

	
	Device Name:
	AMD-Prozessor 


	AMD-Prozessor

	


	
	 
	

	
	Device Name:
	AMD-Prozessor 


	AMD-Prozessor

	


	
	 
	

	
	Device Name:
	AMD-Prozessor 


	AMD-Prozessor

	


	
	 
	

	
	Device Name:
	AMD-Prozessor 


	AMD-Prozessor

	


	
	 
	

	
	Device Name:
	AMD-Prozessor 


	AMD-Prozessor

	


	
	 
	

	
	Device Name:
	AMD-Prozessor 


	AMD-Prozessor

	


	
	 
	

	
	Device Name:
	AMD-Prozessor 


	AMD-Prozessor

	


	
	 
	

	
	Device Name:
	AMD-Prozessor 


	ACPI-Schalter

	


	
	 
	

	
	Device Name:
	ACPI-Schalter 


	Programmierbarer Interruptcontroller

	


	
	 
	

	
	Device Name:
	Programmierbarer Interruptcontroller 

	 
	
	

	[Assigned Resources] 

	
	I/O Port:
	0020 - 0021 

	
	IRQ:
	65792 

	 
	
	

	[Alternative 1] 

	
	I/O Port:
	0020 - 0021 

	
	I/O Port:
	00A0 - 00A1 


	Systemzeitgeber

	


	
	 
	

	
	Device Name:
	Systemzeitgeber 

	 
	
	

	[Assigned Resources] 

	
	I/O Port:
	0040 - 0043 

	 
	
	

	[Alternative 1] 

	
	I/O Port:
	0040 - 0043 

	
	IRQ:
	0 


	Hochpr?isionsereigniszeitgeber

	


	
	 
	

	
	Device Name:
	Hochpr?isionsereigniszeitgeber 

	 
	
	

	[Assigned Resources] 

	
	Memory Location:
	FED00000 - FED003FF 

	 
	
	

	[Alternative 1] 

	
	Memory Location:
	FED00000 - FED003FF 


	DMA-Controller

	


	
	 
	

	
	Device Name:
	DMA-Controller 

	 
	
	

	[Assigned Resources] 

	
	I/O Port:
	0089 - 008B 

	
	DMA:
	4 

	 
	
	

	[Alternative 1] 

	
	I/O Port:
	0000 - 000F 

	
	I/O Port:
	0081 - 0083 

	
	I/O Port:
	0087 

	
	I/O Port:
	0089 - 008B 

	
	I/O Port:
	008F 

	
	I/O Port:
	00C0 - 00DF 

	
	DMA:
	4 


	Druckeranschluss

	


	
	 
	

	
	Device Name:
	Druckeranschluss 

	 
	
	

	[Assigned Resources] 

	
	I/O Port:
	0378 - 037F 

	 
	
	

	[Alternative 1] 

	
	I/O Port:
	0378 - 037F 

	
	IRQ:
	3 

	
	IRQ:
	4 

	
	IRQ:
	5 

	
	IRQ:
	6 

	
	IRQ:
	7 

	
	IRQ:
	10 

	
	IRQ:
	11 

	
	IRQ:
	12 

	 
	
	

	[Alternative 2] 

	
	I/O Port:
	0278 - 027F 

	
	IRQ:
	3 

	
	IRQ:
	4 

	
	IRQ:
	5 

	
	IRQ:
	6 

	
	IRQ:
	7 

	
	IRQ:
	10 

	
	IRQ:
	11 

	
	IRQ:
	12 

	 
	
	

	[Alternative 3] 

	
	I/O Port:
	03BC - 03BF 

	
	IRQ:
	3 

	
	IRQ:
	4 

	
	IRQ:
	5 

	
	IRQ:
	6 

	
	IRQ:
	7 

	
	IRQ:
	10 

	
	IRQ:
	11 

	
	IRQ:
	12 


	Kommunikationsanschluss

	


	
	 
	

	
	Device Name:
	Kommunikationsanschluss 

	 
	
	

	[Assigned Resources] 

	
	I/O Port:
	03F8 - 03FF 

	 
	
	

	[Alternative 1] 

	
	I/O Port:
	03F8 - 03FF 

	
	IRQ:
	4 

	 
	
	

	[Alternative 2] 

	
	I/O Port:
	03F8 - 03FF 

	
	IRQ:
	3 

	
	IRQ:
	4 

	
	IRQ:
	5 

	
	IRQ:
	6 

	
	IRQ:
	7 

	
	IRQ:
	10 

	
	IRQ:
	11 

	
	IRQ:
	12 

	 
	
	

	[Alternative 3] 

	
	I/O Port:
	02F8 - 02FF 

	
	IRQ:
	3 

	
	IRQ:
	4 

	
	IRQ:
	5 

	
	IRQ:
	6 

	
	IRQ:
	7 

	
	IRQ:
	10 

	
	IRQ:
	11 

	
	IRQ:
	12 

	 
	
	

	[Alternative 4] 

	
	I/O Port:
	03E8 - 03EF 

	
	IRQ:
	3 

	
	IRQ:
	4 

	
	IRQ:
	5 

	
	IRQ:
	6 

	
	IRQ:
	7 

	
	IRQ:
	10 

	
	IRQ:
	11 

	
	IRQ:
	12 

	 
	
	

	[Alternative 5] 

	
	I/O Port:
	02E8 - 02EF 

	
	IRQ:
	3 

	
	IRQ:
	4 

	
	IRQ:
	5 

	
	IRQ:
	6 

	
	IRQ:
	7 

	
	IRQ:
	10 

	
	IRQ:
	11 

	
	IRQ:
	12 


	Systemlautsprecher

	


	
	 
	

	
	Device Name:
	Systemlautsprecher 

	 
	
	

	[Assigned Resources] 

	
	I/O Port:
	0061 

	 
	
	

	[Alternative 1] 

	
	I/O Port:
	0061 


	Pci Bus

	


	
	 
	

	
	Device Name:
	Pci Bus 

	 
	
	

	[Assigned Resources] 

	
	I/O Port:
	0000 - FFFFFFFF 

	
	Memory Location:
	000A0000 - 000BFFFF 

	
	Memory Location:
	D0000000 - CFFFFFFF 

	 
	
	

	[Alternative 1] 

	
	I/O Port:
	0000 - 0CF7 

	
	I/O Port:
	0D00 - FFFF 

	
	Memory Location:
	000A0000 - 000BFFFF 

	
	Memory Location:
	000D0000 - 000DFFFF 

	
	Memory Location:
	D0000000 - DFFFFFFF 

	
	Memory Location:
	F0000000 - FEBFFFFF 


	System CMOS/Echtzeituhr

	


	
	 
	

	
	Device Name:
	System CMOS/Echtzeituhr 

	 
	
	

	[Assigned Resources] 

	
	I/O Port:
	0070 - 0071 

	 
	
	

	[Alternative 1] 

	
	I/O Port:
	0070 - 0071 

	
	IRQ:
	8 


	Systemplatine

	


	
	 
	

	
	Device Name:
	Systemplatine 

	 
	
	

	[Assigned Resources] 

	
	Memory Location:
	00000000 - 0009FFFF 

	 
	
	

	[Alternative 1] 

	
	Memory Location:
	00000000 - 0009FFFF 

	
	Memory Location:
	000C0000 - 000CFFFF 

	
	Memory Location:
	000E0000 - 000FFFFF 

	
	Memory Location:
	00100000 - CFFFFFFF 

	
	Memory Location:
	FEC00000 - FFFFFFFF 


	Hauptplatinenressourcen

	


	
	 
	

	
	Device Name:
	Hauptplatinenressourcen 

	 
	
	

	[Assigned Resources] 

	
	I/O Port:
	0060 

	
	I/O Port:
	0000 - FEBFFFFF 

	 
	
	

	[Alternative 1] 

	
	I/O Port:
	0060 

	
	I/O Port:
	0064 

	
	Memory Location:
	FEC00000 - FEC00FFF 

	
	Memory Location:
	FEE00000 - FEE00FFF 


	Hauptplatinenressourcen

	


	
	 
	

	
	Device Name:
	Hauptplatinenressourcen 

	 
	
	

	[Assigned Resources] 

	
	I/O Port:
	0010 - 001F 

	
	I/O Port:
	0072 - 007F 

	
	I/O Port:
	0000 - 0083 

	
	I/O Port:
	008C - 008E 

	
	I/O Port:
	00E0 - 00EF 

	
	I/O Port:
	0C00 - 0C01 

	
	I/O Port:
	0000 - 0C4F 

	
	I/O Port:
	0C6C 

	
	I/O Port:
	0000 - 0CCF 

	
	I/O Port:
	0CD4 - 0CD5 

	
	I/O Port:
	0B00 - 0B0F 

	
	IRQ:
	1114369 

	
	IRQ:
	1114369 

	 
	
	

	[Alternative 1] 

	
	I/O Port:
	0010 - 001F 

	
	I/O Port:
	0022 - 003F 

	
	I/O Port:
	0062 - 0063 

	
	I/O Port:
	0065 - 006F 

	
	I/O Port:
	0072 - 007F 

	
	I/O Port:
	0080 

	
	I/O Port:
	0084 - 0086 

	
	I/O Port:
	0088 

	
	I/O Port:
	008C - 008E 

	
	I/O Port:
	0090 - 009F 

	
	I/O Port:
	00A2 - 00BF 

	
	I/O Port:
	00B1 

	
	I/O Port:
	00E0 - 00EF 

	
	I/O Port:
	04D0 - 04D1 

	
	I/O Port:
	040B 

	
	I/O Port:
	04D6 

	
	I/O Port:
	0C00 - 0C01 

	
	I/O Port:
	0C14 

	
	I/O Port:
	0C50 - 0C51 

	
	I/O Port:
	0C52 

	
	I/O Port:
	0C6C 

	
	I/O Port:
	0C6F 

	
	I/O Port:
	0CD0 - 0CD1 

	
	I/O Port:
	0CD2 - 0CD3 

	
	I/O Port:
	0CD4 - 0CD5 

	
	I/O Port:
	0CD6 - 0CD7 

	
	I/O Port:
	0CD8 - 0CDF 

	
	I/O Port:
	0800 - 089F 

	
	I/O Port:
	0B00 - 0B0F 

	
	I/O Port:
	0B20 - 0B3F 

	
	I/O Port:
	0900 - 090F 

	
	I/O Port:
	0910 - 091F 

	
	I/O Port:
	FE00 - FEFE 

	
	I/O Port:
	0060 

	
	I/O Port:
	0064 

	
	Memory Location:
	FFB80000 - FFBFFFFF 

	
	Memory Location:
	FEC10000 - FEC1001F 


	Hauptplatinenressourcen

	


	
	 
	

	
	Device Name:
	Hauptplatinenressourcen 

	 
	
	

	[Assigned Resources] 

	
	Memory Location:
	E0000000 - EFFFFFFF 

	 
	
	

	[Alternative 1] 

	
	Memory Location:
	E0000000 - EFFFFFFF 


	Hauptplatinenressourcen

	


	
	 
	

	
	Device Name:
	Hauptplatinenressourcen 


	Hauptplatinenressourcen

	


	
	 
	

	
	Device Name:
	Hauptplatinenressourcen 

	 
	
	

	[Assigned Resources] 

	
	I/O Port:
	0E80 - 0F5F 

	 
	
	

	[Alternative 1] 

	
	I/O Port:
	0E80 - 0F5F 

	
	I/O Port:
	0AE0 - 0AEF 


	Numerischer Coprozessor

	


	
	 
	

	
	Device Name:
	Numerischer Coprozessor 

	 
	
	

	[Assigned Resources] 

	
	I/O Port:
	00F0 - 00FF 

	 
	
	

	[Alternative 1] 

	
	I/O Port:
	00F0 - 00FF 

	
	IRQ:
	13 


	ACPI-Einschaltknopf

	


	
	 
	

	
	Device Name:
	ACPI-Einschaltknopf 


	Microsoft Windows-Verwaltungsschnittstelle f? ACPI

	


	
	 
	

	
	Device Name:
	Microsoft Windows-Verwaltungsschnittstelle f? ACPI 


	SMBIOS DMI

	


	
	 
	

	 
	
	

	 
	
	


	BIOS

	


	
	 
	

	
	BIOS Vendor:
	American Megatrends Inc. 

	
	BIOS Version:
	V17.15 

	
	BIOS Release Date:
	04/28/2013 

	
	BIOS Start Segment:
	F000 

	
	BIOS Size:
	2048 KBytes 

	 
	
	

	
	System BIOS Version:
	8.15 

	 
	
	

	
	ISA Support:
	Present 

	
	MCA Support:
	Not Present 

	
	EISA Support:
	Not Present 

	
	PCI Support:
	Present 

	
	PC Card (PCMCIA) Support:
	Not Present 

	
	Plug-and-Play Support:
	Present 

	
	APM Support:
	Present 

	
	Flash BIOS:
	Present 

	
	BIOS Shadow:
	Present 

	
	VL-VESA Support:
	Not Present 

	
	ESCD Support:
	Present 

	
	Boot from CD:
	Present 

	
	Selectable Boot:
	Present 

	
	BIOS ROM Socketed:
	Present 

	
	Boot from PC Card:
	Not Present 

	
	EDD Support:
	Present 

	
	NEC PC-98 Support:
	Not Present 

	
	ACPI Support:
	Present 

	
	USB Legacy Support:
	Present 

	
	AGP Support:
	Not Present 

	
	I2O Boot Support:
	Not Present 

	
	LS-120 Boot Support:
	Present 

	
	ATAPI ZIP Drive Boot Support:
	Present 

	
	IEE1394 Boot Support:
	Not Present 

	
	Smart Battery Support:
	Not Present 

	
	BIOS Boot Specification Support:
	Present 

	
	Function key-initiated Network Service Boot Support:
	Not Present 

	
	Targeted Content Distribution Support:
	Present 

	
	UEFI Specification Support:
	Not Present 


	System

	


	
	 
	

	
	System Manufacturer:
	MSI 

	
	Product Name:
	MS-7641 

	
	Product Version:
	3.0 

	
	Product Serial Number:
	To Be Filled By O.E.M. 

	
	SKU Number:
	To Be Filled By O.E.M. 

	
	Family:
	To Be Filled By O.E.M. 


	Mainboard

	


	
	 
	

	
	Mainboard Manufacturer:
	MSI 

	
	Mainboard Name:
	760GM-P23(FX) (MS-7641) 

	
	Mainboard Version:
	3.0 

	
	Mainboard Serial Number:
	To be filled by O.E.M. 

	
	Asset Tag:
	To Be Filled By O.E.M. 

	
	Location in chassis:
	To Be Filled By O.E.M. 


	System Enclosure

	


	
	 
	

	
	Manufacturer:
	MSI 

	
	Case Type:
	Desktop 

	
	Version:
	3.0 

	
	Serial Number:
	To Be Filled By O.E.M. 

	
	Asset Tag Number:
	To Be Filled By O.E.M. 


	Processor

	


	
	 
	

	
	Processor Manufacturer:
	AMD 

	
	Processor Version:
	AMD FX(tm)-8120 Eight-Core Processor 

	
	External Clock:
	200 MHz 

	
	Maximum Clock Supported:
	3100 MHz 

	
	Current Clock:
	3100 MHz 

	
	CPU Socket:
	Populated 

	
	CPU Status:
	Disabled by BIOS 

	
	Processor Type:
	Central Processor 

	
	Processor Voltage:
	1.2 V 

	
	Processor Status:
	Enabled 

	
	Processor Upgrade:
	Socket AM3 

	
	Socket Designation:
	CPU1 


	L1-Cache

	


	
	 
	

	
	Socket Designation:
	L1-Cache 

	
	Cache State:
	Enabled 

	
	Cache Type:
	Internal, Unified 

	
	Cache Scheme:
	Write-Back 

	
	Supported SRAM Type:
	Pipeline Burst 

	
	Current SRAM Type:
	Pipeline Burst 

	
	Cache Speed:
	1 ns 

	
	Error Correction Type:
	Unknown 

	
	Maximum Cache Size:
	384 KBytes 

	
	Installed Cache Size:
	384 KBytes 

	
	Cache Associativity:
	2-way Set-Associative 


	L2-Cache

	


	
	 
	

	
	Socket Designation:
	L2-Cache 

	
	Cache State:
	Enabled 

	
	Cache Type:
	Internal, Unified 

	
	Cache Scheme:
	Write-Back 

	
	Supported SRAM Type:
	Pipeline Burst 

	
	Current SRAM Type:
	Pipeline Burst 

	
	Cache Speed:
	1 ns 

	
	Error Correction Type:
	Unknown 

	
	Maximum Cache Size:
	8192 KBytes 

	
	Installed Cache Size:
	8192 KBytes 

	
	Cache Associativity:
	16-way Set-Associative 


	L3-Cache

	


	
	 
	

	
	Socket Designation:
	L3-Cache 

	
	Cache State:
	Enabled 

	
	Cache Type:
	Internal, Unified 

	
	Cache Scheme:
	Write-Back 

	
	Supported SRAM Type:
	Pipeline Burst 

	
	Current SRAM Type:
	Pipeline Burst 

	
	Cache Speed:
	1 ns 

	
	Error Correction Type:
	Unknown 

	
	Maximum Cache Size:
	8192 KBytes 

	
	Installed Cache Size:
	8192 KBytes 

	
	Cache Associativity:
	Unknown 


	BIOS Language

	


	
	 
	

	
	
	en|US|iso8859-1 <Active> 


	System Boot Information

	


	
	 
	

	
	Boot Status:
	No error occured 


	On Board Device

	


	
	 
	

	
	Device Description:
	To Be Filled By O.E.M. 

	
	Device Type:
	Video Adapter 

	
	Device Status:
	Enabled 

	 
	
	


	Memory Devices

	


	
	 
	


	Physical Memory Array

	


	
	 
	

	
	Array Location:
	System board 

	
	Array Use:
	System memory 

	
	Error Detecting Method:
	None 

	
	Memory Capacity:
	8388608 KBytes 

	
	Memory Devices:
	2 


	Memory Array Mapped Address

	


	
	 
	

	
	Starting Address:
	00000000 

	
	Ending Address:
	010BFFFF 

	
	Partition Width:
	1 


	Memory Device

	


	
	 
	

	
	Total Width:
	64 bits 

	
	Data Width:
	64 bits 

	
	Device Size:
	8192 MBytes 

	
	Device Form Factor:
	DIMM 

	
	Device Locator:
	DIMM1 

	
	Bank Locator:
	BANK0 

	
	Device Type:
	Unknown 

	
	Device Type Detail:
	Synchronous 

	
	Memory Speed:
	1333 MHz 

	
	Manufacturer:
	Nanya 

	
	Serial Number:
	3D143A1A 

	
	Part Number:
	M2F8G64CB8HB5N-CG 

	
	Asset Tag:
	AssetTagNum0 


	Memory Device Mapped Address

	


	
	 
	

	
	Starting Address:
	00000000 

	
	Ending Address:
	007FFFFF 

	
	Partition Row Position:
	1 

	
	Interleave Position:
	Non-interleaved 

	
	Interleave Data Depth:
	0 


	Memory Device

	


	
	 
	

	
	Total Width:
	64 bits 

	
	Data Width:
	64 bits 

	
	Device Size:
	8192 MBytes 

	
	Device Form Factor:
	DIMM 

	
	Device Locator:
	DIMM2 

	
	Bank Locator:
	BANK1 

	
	Device Type:
	Unknown 

	
	Device Type Detail:
	Synchronous 

	
	Memory Speed:
	1333 MHz 

	
	Manufacturer:
	Nanya 

	
	Serial Number:
	3E1242A2 

	
	Part Number:
	M2F8G64CB8HB5N-CG 

	
	Asset Tag:
	AssetTagNum1 


	Memory Device Mapped Address

	


	
	 
	

	
	Starting Address:
	00800000 

	
	Ending Address:
	00FFFFFF 

	
	Partition Row Position:
	1 

	
	Interleave Position:
	Non-interleaved 

	
	Interleave Data Depth:
	0 


	Port Connectors

	


	
	 
	


	Mouse Port

	


	
	 
	

	
	Port Type:
	Mouse Port 

	
	Internal Reference:
	PS1 

	
	Internal Connector Type:
	None 

	
	External Reference:
	PS2 Mouse 

	
	External Connector Type:
	PS/2 


	Keyboard Port

	


	
	 
	

	
	Port Type:
	Keyboard Port 

	
	Internal Reference:
	PS1 

	
	Internal Connector Type:
	None 

	
	External Reference:
	PS2 Keyboard 

	
	External Connector Type:
	PS/2 


	Serial Port 16550A Compatible

	


	
	 
	

	
	Port Type:
	Serial Port 16550A Compatible 

	
	Internal Reference:
	COM1 

	
	Internal Connector Type:
	None 

	
	External Reference:
	COM 

	
	External Connector Type:
	DB-9 pin male 


	Audio Port

	


	
	 
	

	
	Port Type:
	Audio Port 

	
	Internal Reference:
	JACK1 

	
	Internal Connector Type:
	None 

	
	External Reference:
	Audio Mic In 

	
	External Connector Type:
	Mini-jack (headphones) 


	Audio Port

	


	
	 
	

	
	Port Type:
	Audio Port 

	
	Internal Reference:
	JACK1 

	
	Internal Connector Type:
	None 

	
	External Reference:
	Audio Line In 

	
	External Connector Type:
	Mini-jack (headphones) 


	Audio Port

	


	
	 
	

	
	Port Type:
	Audio Port 

	
	Internal Reference:
	JACK1 

	
	Internal Connector Type:
	None 

	
	External Reference:
	Audio Line Out 

	
	External Connector Type:
	Mini-jack (headphones) 


	USB

	


	
	 
	

	
	Port Type:
	USB 

	
	Internal Reference:
	USB1 

	
	Internal Connector Type:
	None 

	
	External Reference:
	USB1 

	
	External Connector Type:
	Access Bus (USB) 


	USB

	


	
	 
	

	
	Port Type:
	USB 

	
	Internal Reference:
	USB1 

	
	Internal Connector Type:
	None 

	
	External Reference:
	USB2 

	
	External Connector Type:
	Access Bus (USB) 


	USB

	


	
	 
	

	
	Port Type:
	USB 

	
	Internal Reference:
	USB1 

	
	Internal Connector Type:
	None 

	
	External Reference:
	USB3 

	
	External Connector Type:
	Access Bus (USB) 


	USB

	


	
	 
	

	
	Port Type:
	USB 

	
	Internal Reference:
	USB1 

	
	Internal Connector Type:
	None 

	
	External Reference:
	USB4 

	
	External Connector Type:
	Access Bus (USB) 


	Network Port

	


	
	 
	

	
	Port Type:
	Network Port 

	
	Internal Reference:
	LAN 

	
	Internal Connector Type:
	None 

	
	External Reference:
	LAN 

	
	External Connector Type:
	RJ-45 


	Port Connector

	


	
	 
	

	
	Port Type:
	Unknown 

	
	Internal Reference:
	JBAT1 

	
	Internal Connector Type:
	Unknown 

	
	External Reference:
	Unknown 

	
	External Connector Type:
	None 


	Audio Port

	


	
	 
	

	
	Port Type:
	Audio Port 

	
	Internal Reference:
	CD_IN1 

	
	Internal Connector Type:
	On Board Sound Input from CD-ROM 

	
	External Reference:
	Unknown 

	
	External Connector Type:
	None 


	Port Connector

	


	
	 
	

	
	Port Type:
	Unknown 

	
	Internal Reference:
	JCI1 

	
	Internal Connector Type:
	Unknown 

	
	External Reference:
	Unknown 

	
	External Connector Type:
	None 


	USB

	


	
	 
	

	
	Port Type:
	USB 

	
	Internal Reference:
	JUSB1 

	
	Internal Connector Type:
	Unknown 

	
	External Reference:
	Unknown 

	
	External Connector Type:
	None 


	USB

	


	
	 
	

	
	Port Type:
	USB 

	
	Internal Reference:
	JUSB2 

	
	Internal Connector Type:
	Unknown 

	
	External Reference:
	Unknown 

	
	External Connector Type:
	None 


	USB

	


	
	 
	

	
	Port Type:
	USB 

	
	Internal Reference:
	JUSB3 

	
	Internal Connector Type:
	Unknown 

	
	External Reference:
	Unknown 

	
	External Connector Type:
	None 


	Port Connector

	


	
	 
	

	
	Port Type:
	Unknown 

	
	Internal Reference:
	JFP1 

	
	Internal Connector Type:
	Unknown 

	
	External Reference:
	Unknown 

	
	External Connector Type:
	None 


	Port Connector

	


	
	 
	

	
	Port Type:
	Unknown 

	
	Internal Reference:
	JFP2 

	
	Internal Connector Type:
	Unknown 

	
	External Reference:
	Unknown 

	
	External Connector Type:
	None 


	SATA

	


	
	 
	

	
	Port Type:
	SATA 

	
	Internal Reference:
	SATA1 

	
	Internal Connector Type:
	SAS/SATA Plug Receptacle 

	
	External Reference:
	Unknown 

	
	External Connector Type:
	None 


	SATA

	


	
	 
	

	
	Port Type:
	SATA 

	
	Internal Reference:
	SATA2 

	
	Internal Connector Type:
	SAS/SATA Plug Receptacle 

	
	External Reference:
	Unknown 

	
	External Connector Type:
	None 


	SATA

	


	
	 
	

	
	Port Type:
	SATA 

	
	Internal Reference:
	SATA3 

	
	Internal Connector Type:
	SAS/SATA Plug Receptacle 

	
	External Reference:
	Unknown 

	
	External Connector Type:
	None 


	SATA

	


	
	 
	

	
	Port Type:
	SATA 

	
	Internal Reference:
	SATA4 

	
	Internal Connector Type:
	SAS/SATA Plug Receptacle 

	
	External Reference:
	Unknown 

	
	External Connector Type:
	None 


	SATA

	


	
	 
	

	
	Port Type:
	SATA 

	
	Internal Reference:
	SATA5 

	
	Internal Connector Type:
	SAS/SATA Plug Receptacle 

	
	External Reference:
	Unknown 

	
	External Connector Type:
	None 


	SATA

	


	
	 
	

	
	Port Type:
	SATA 

	
	Internal Reference:
	SATA6 

	
	Internal Connector Type:
	SAS/SATA Plug Receptacle 

	
	External Reference:
	Unknown 

	
	External Connector Type:
	None 


	System Slots

	


	
	 
	


	PCIE1

	


	
	 
	

	
	Slot Designation:
	PCIE1 

	
	Slot Type:
	PCI Express 

	
	Slot Usage:
	Empty 

	
	Slot Data Bus Width:
	1x / x1 

	
	Slot Length:
	Short 


	PCIE2

	


	
	 
	

	
	Slot Designation:
	PCIE2 

	
	Slot Type:
	PCI Express 

	
	Slot Usage:
	In use 

	
	Slot Data Bus Width:
	16x / x16 

	
	Slot Length:
	Long 


	PCI1

	


	
	 
	

	
	Slot Designation:
	PCI1 

	
	Slot Type:
	PCI 

	
	Slot Usage:
	Empty 

	
	Slot Data Bus Width:
	32-bit 

	
	Slot Length:
	Short 


	Memory

	


	
	 
	

	[General information] 

	
	Total Memory Size:
	16 GBytes 

	
	Total Memory Size [MB]:
	16384 

	 
	
	

	[Current Performance Settings] 

	
	Maximum Supported Memory Clock:
	933.3 MHz 

	
	Current Memory Clock:
	666.7 MHz 

	
	Current Timing (tCAS-tRCD-tRP-tRAS):
	9.0-9-9-24 

	 
	
	

	
	Read to Read Delay (tRD_RD) Same Rank:
	1T 

	
	Read to Read Delay (tRD_RD) Different Rank:
	3T 

	
	Read to Read Delay (tRD_RD) Different DIMM:
	3T 

	
	Write to Write Delay (tWR_WR) Same Rank:
	1T 

	
	Write to Write Delay (tWR_WR) Different Rank:
	3T 

	
	Write to Write Delay (tWR_WR) Different DIMM:
	3T 

	
	Write to Read Delay (tWR_RD) Same Rank (tWTR):
	5T 

	
	Read to Precharge Delay (tRTP):
	5T 

	
	Write to Precharge Delay (tWTP):
	21T 

	
	Write Recovery Time (tWR):
	10T 

	
	RAS# to RAS# Delay (tRRD):
	4T 

	
	Row Cycle Time (tRC):
	33T 

	
	Four Activate Window (tFAW):
	20T 


	Row: 0 - 8192 MB PC3-10600 DDR3 SDRAM Nanya Technology M2F8G64CB8HB5N-CG

	


	
	 
	

	[General Module Information] 

	
	Module Number:
	0 

	
	Module Size:
	8192 MBytes 

	
	Memory Type:
	DDR3 SDRAM 

	
	Module Type:
	Unbuffered DIMM (UDIMM) 

	
	Memory Speed:
	666.7 MHz (DDR3-1333 / PC3-10600) 

	
	Module Manufacturer:
	Nanya Technology 

	
	Module Part Number:
	M2F8G64CB8HB5N-CG 

	
	Module Revision:
	0 

	
	Module Serial Number:
	1024735770 

	
	Module Manufacturing Date:
	Year: 2012, Week: 50 

	
	Module Manufacturing Location:
	13 

	
	SDRAM Manufacturer:
	Nanya Technology 

	
	Error Check/Correction:
	None 

	 
	
	

	[Module characteristics] 

	
	Row Address Bits:
	16 

	
	Column Address Bits:
	10 

	
	Number Of Banks:
	8 

	
	Module Density:
	4096 Mb 

	
	Number Of Ranks:
	2 

	
	Device Width:
	8 bits 

	
	Bus Width:
	64 bits 

	
	Module Nominal Voltage (VDD):
	1.5 V 

	 
	
	

	[Module timing] 

	
	Minimum SDRAM Cycle Time (tCKmin):
	1.500 ns 

	
	CAS# Latencies Supported:
	5, 6, 7, 8, 9 

	
	Minimum CAS# Latency Time (tAAmin):
	13.125 ns 

	
	Minimum RAS# to CAS# Delay (tRCDmin):
	13.125 ns 

	
	Minimum Row Precharge Time (tRPmin):
	13.125 ns 

	
	Minimum Active to Precharge Time (tRASmin):
	36.000 ns 

	 
	
	

	
	Supported Module Timing at 666.7 MHz:
	9-9-9-24 

	
	Supported Module Timing at 600.0 MHz:
	8-8-8-22 

	
	Supported Module Timing at 533.3 MHz:
	7-7-7-20 

	
	Supported Module Timing at 466.7 MHz:
	7-7-7-17 

	
	Supported Module Timing at 400.0 MHz:
	6-6-6-15 

	
	Supported Module Timing at 333.3 MHz:
	5-5-5-12 

	 
	
	

	
	Minimum Write Recovery Time (tWRmin):
	15.000 ns 

	
	Minimum Row Active to Row Active Delay (tRRDmin):
	6.000 ns 

	
	Minimum Active to Active/Refresh Time (tRCmin):
	49.125 ns 

	
	Minimum Refresh Recovery Time Delay (tRFCmin):
	260.000 ns 

	
	Minimum Internal Write to Read Command Delay (tWTRmin):
	7.500 ns 

	
	Minimum Internal Read to Precharge Command Delay (tRTPmin):
	7.500 ns 

	
	Minimum Four Activate Window Delay Time (tFAWmin):
	30.000 ns 

	 
	
	

	[Features] 

	
	Partial Array Self Refresh (PASR):
	Not Supported 

	
	On-die Thermal Sensor (ODTS) Readout:
	Not Supported 

	
	Auto Self Refresh (ASR):
	Supported 

	
	Extended Temperature 1X Refresh Rate:
	Not Supported 

	
	Extended Temperature Range:
	Supported 

	
	Module Temperature Sensor:
	Not Supported 

	
	Pseudo Target Row Refresh (pTRR):
	Not Supported 

	
	Module Nominal Height:
	29 - 30 mm 

	
	Module Maximum Thickness (Front):
	1 - 2 mm 

	
	Module Maximum Thickness (Back):
	1 - 2 mm 


	Row: 1 - 8192 MB PC3-10600 DDR3 SDRAM Nanya Technology M2F8G64CB8HB5N-CG

	


	
	 
	

	[General Module Information] 

	
	Module Number:
	1 

	
	Module Size:
	8192 MBytes 

	
	Memory Type:
	DDR3 SDRAM 

	
	Module Type:
	Unbuffered DIMM (UDIMM) 

	
	Memory Speed:
	666.7 MHz (DDR3-1333 / PC3-10600) 

	
	Module Manufacturer:
	Nanya Technology 

	
	Module Part Number:
	M2F8G64CB8HB5N-CG 

	
	Module Revision:
	0 

	
	Module Serial Number:
	1041384098 

	
	Module Manufacturing Date:
	Year: 2012, Week: 49 

	
	Module Manufacturing Location:
	13 

	
	SDRAM Manufacturer:
	Nanya Technology 

	
	Error Check/Correction:
	None 

	 
	
	

	[Module characteristics] 

	
	Row Address Bits:
	16 

	
	Column Address Bits:
	10 

	
	Number Of Banks:
	8 

	
	Module Density:
	4096 Mb 

	
	Number Of Ranks:
	2 

	
	Device Width:
	8 bits 

	
	Bus Width:
	64 bits 

	
	Module Nominal Voltage (VDD):
	1.5 V 

	 
	
	

	[Module timing] 

	
	Minimum SDRAM Cycle Time (tCKmin):
	1.500 ns 

	
	CAS# Latencies Supported:
	5, 6, 7, 8, 9 

	
	Minimum CAS# Latency Time (tAAmin):
	13.125 ns 

	
	Minimum RAS# to CAS# Delay (tRCDmin):
	13.125 ns 

	
	Minimum Row Precharge Time (tRPmin):
	13.125 ns 

	
	Minimum Active to Precharge Time (tRASmin):
	36.000 ns 

	 
	
	

	
	Supported Module Timing at 666.7 MHz:
	9-9-9-24 

	
	Supported Module Timing at 600.0 MHz:
	8-8-8-22 

	
	Supported Module Timing at 533.3 MHz:
	7-7-7-20 

	
	Supported Module Timing at 466.7 MHz:
	7-7-7-17 

	
	Supported Module Timing at 400.0 MHz:
	6-6-6-15 

	
	Supported Module Timing at 333.3 MHz:
	5-5-5-12 

	 
	
	

	
	Minimum Write Recovery Time (tWRmin):
	15.000 ns 

	
	Minimum Row Active to Row Active Delay (tRRDmin):
	6.000 ns 

	
	Minimum Active to Active/Refresh Time (tRCmin):
	49.125 ns 

	
	Minimum Refresh Recovery Time Delay (tRFCmin):
	260.000 ns 

	
	Minimum Internal Write to Read Command Delay (tWTRmin):
	7.500 ns 

	
	Minimum Internal Read to Precharge Command Delay (tRTPmin):
	7.500 ns 

	
	Minimum Four Activate Window Delay Time (tFAWmin):
	30.000 ns 

	 
	
	

	[Features] 

	
	Partial Array Self Refresh (PASR):
	Not Supported 

	
	On-die Thermal Sensor (ODTS) Readout:
	Not Supported 

	
	Auto Self Refresh (ASR):
	Supported 

	
	Extended Temperature 1X Refresh Rate:
	Not Supported 

	
	Extended Temperature Range:
	Supported 

	
	Module Temperature Sensor:
	Not Supported 

	
	Pseudo Target Row Refresh (pTRR):
	Not Supported 

	
	Module Nominal Height:
	29 - 30 mm 

	
	Module Maximum Thickness (Front):
	1 - 2 mm 

	
	Module Maximum Thickness (Back):
	1 - 2 mm 


	Bus

	


	
	 
	


	PCI Bus #0

	


	
	 
	


	AMD RS880(M) Chipset - Host Bridge

	


	
	 
	

	[General Information] 

	
	Device Name:
	AMD RS880(M) Chipset - Host Bridge 

	
	Original Device Name:
	AMD RS880(M) Chipset - Host Bridge 

	
	Device Class:
	Host-to-PCI Bridge 

	
	Revision ID:
	0 

	
	Bus Number:
	0 

	
	Device Number:
	0 

	
	Function Number:
	0 

	
	PCI Latency Timer:
	0 

	
	Hardware ID:
	PCI\VEN_1022&DEV_9600&SUBSYS_96001022&REV_00 

	 
	
	

	[System Resources] 

	
	Interrupt Line:
	N/A 

	
	Interrupt Pin:
	N/A 

	 
	
	

	[Features] 

	
	Bus Mastering:
	Enabled 

	
	Running At 66 MHz:
	Capable 

	
	Fast Back-to-Back Transactions:
	Not Capable 

	 
	
	

	[Driver Information] 

	
	Driver Manufacturer:
	(Standardsystemger?e) 

	
	Driver Description:
	PCI Standard-Host-CPU-Br?ke 

	
	Driver Provider:
	Microsoft 

	
	Driver Version:
	6.1.7601.17514 

	
	Driver Date:
	21-Jun-2006 

	
	DeviceInstanceId
	PCI\VEN_1022&DEV_9600&SUBSYS_96001022&REV_00\3&267A616A&1&00 


	AMD RS880(M) Chipset - PCI Express Graphics Port 0

	


	
	 
	

	[General Information] 

	
	Device Name:
	AMD RS880(M) Chipset - PCI Express Graphics Port 0 

	
	Original Device Name:
	AMD RS880(M) Chipset - PCI Express Graphics Port 0 

	
	Device Class:
	PCI-to-PCI Bridge 

	
	Revision ID:
	0 

	
	Bus Number:
	0 

	
	Device Number:
	2 

	
	Function Number:
	0 

	
	PCI Latency Timer:
	0 

	
	Hardware ID:
	PCI\VEN_1022&DEV_9603&SUBSYS_00000000&REV_00 

	 
	
	

	[PCI Express] 

	
	Version:
	2.0 

	
	Maximum Link Width:
	16x 

	
	Current Link Width:
	16x 

	
	Maximum Link Speed:
	5.0 Gb/s 

	
	Current Link Speed:
	5.0 Gb/s 

	
	Device/Port Type:
	Root Port of PCI Express Root Complex 

	
	Slot Implemented:
	Yes 

	
	Hot-Plug:
	Not Capable 

	
	Hot-Plug Surprise:
	Not Capable 

	
	Slot Power Limit:
	75.000 W 

	
	Active State Power Management (ASPM) Support:
	L0s and L1 

	
	Active State Power Management (ASPM) Status:
	Disabled 

	 
	
	

	[System Resources] 

	
	Interrupt Line:
	IRQ18 

	
	Interrupt Pin:
	INTA# 

	 
	
	

	[Features] 

	
	Bus Mastering:
	Enabled 

	
	Running At 66 MHz:
	Not Capable 

	
	Fast Back-to-Back Transactions:
	Not Capable 

	 
	
	

	[Driver Information] 

	
	Driver Manufacturer:
	(Standardsystemger?e) 

	
	Driver Description:
	PCI Standard-PCI-zu-PCI-Br?ke 

	
	Driver Provider:
	Microsoft 

	
	Driver Version:
	6.1.7601.17514 

	
	Driver Date:
	21-Jun-2006 

	
	DeviceInstanceId
	PCI\VEN_1022&DEV_9603&SUBSYS_96001022&REV_00\3&267A616A&1&10 


	PCI Express x16 Bus #1

	


	
	 
	


	PowerColor Radeon HD 8350

	


	
	 
	

	[General Information] 

	
	Device Name:
	PowerColor Radeon HD 8350 

	
	Original Device Name:
	ATI/AMD Radeon HD 5450/5470/5490/5530/6230/6250/6290 (CEDAR PRO) 

	
	Device Class:
	VGA Compatible Adapter 

	
	Revision ID:
	0 

	
	Bus Number:
	1 

	
	Device Number:
	0 

	
	Function Number:
	0 

	
	PCI Latency Timer:
	0 

	
	Hardware ID:
	PCI\VEN_1002&DEV_68F9&SUBSYS_8350148C&REV_00 

	 
	
	

	[PCI Express] 

	
	Version:
	2.0 

	
	Maximum Link Width:
	16x 

	
	Current Link Width:
	16x 

	
	Maximum Link Speed:
	5.0 Gb/s 

	
	Current Link Speed:
	5.0 Gb/s 

	
	Device/Port Type:
	Legacy PCI Express Endpoint 

	
	Slot Implemented:
	No 

	
	Active State Power Management (ASPM) Support:
	L0s and L1 

	
	Active State Power Management (ASPM) Status:
	Disabled 

	 
	
	

	[System Resources] 

	
	Interrupt Line:
	N/A 

	
	Interrupt Pin:
	INTA# 

	
	Memory Base Address 0
	D0000000 

	
	Memory Base Address 2
	FEBC0000 

	
	I/O Base Address 4
	D000 

	 
	
	

	[Features] 

	
	Bus Mastering:
	Enabled 

	
	Running At 66 MHz:
	Not Capable 

	
	Fast Back-to-Back Transactions:
	Not Capable 

	 
	
	

	[Driver Information] 

	
	Driver Manufacturer:
	Advanced Micro Devices, Inc. 

	
	Driver Description:
	AMD Radeon HD8350 

	
	Driver Provider:
	Advanced Micro Devices, Inc. 

	
	Driver Version:
	14.501.1003.0 

	
	Driver Date:
	20-Nov-2014 

	
	DeviceInstanceId
	PCI\VEN_1002&DEV_68F9&SUBSYS_8350148C&REV_00\4&D378CAC&0&0010 


	ATI/AMD Cedar/Park/Robson - High Definition Audio Controller

	


	
	 
	

	[General Information] 

	
	Device Name:
	ATI/AMD Cedar/Park/Robson - High Definition Audio Controller 

	
	Original Device Name:
	ATI/AMD Cedar/Park/Robson - High Definition Audio Controller 

	
	Device Class:
	Mixed mode device 

	
	Revision ID:
	0 

	
	Bus Number:
	1 

	
	Device Number:
	0 

	
	Function Number:
	1 

	
	PCI Latency Timer:
	0 

	
	Hardware ID:
	PCI\VEN_1002&DEV_AA68&SUBSYS_AA68148C&REV_00 

	 
	
	

	[PCI Express] 

	
	Version:
	2.0 

	
	Maximum Link Width:
	16x 

	
	Current Link Width:
	16x 

	
	Maximum Link Speed:
	5.0 Gb/s 

	
	Current Link Speed:
	5.0 Gb/s 

	
	Device/Port Type:
	Legacy PCI Express Endpoint 

	
	Slot Implemented:
	No 

	
	Active State Power Management (ASPM) Support:
	L0s and L1 

	
	Active State Power Management (ASPM) Status:
	Disabled 

	 
	
	

	[System Resources] 

	
	Interrupt Line:
	IRQ19 

	
	Interrupt Pin:
	INTB# 

	
	Memory Base Address 0
	FEBF8000 

	 
	
	

	[Features] 

	
	Bus Mastering:
	Enabled 

	
	Running At 66 MHz:
	Not Capable 

	
	Fast Back-to-Back Transactions:
	Not Capable 

	 
	
	

	[Driver Information] 

	
	Driver Manufacturer:
	Microsoft 

	
	Driver Description:
	High Definition Audio-Controller 

	
	Driver Provider:
	Microsoft 

	
	Driver Version:
	6.1.7601.17514 

	
	Driver Date:
	19-Nov-2010 

	
	DeviceInstanceId
	PCI\VEN_1002&DEV_AA68&SUBSYS_AA68148C&REV_00\4&D378CAC&0&0110 


	AMD RS880(M) Chipset - PCI Express Port 1

	


	
	 
	

	[General Information] 

	
	Device Name:
	AMD RS880(M) Chipset - PCI Express Port 1 

	
	Original Device Name:
	AMD RS880(M) Chipset - PCI Express Port 1 

	
	Device Class:
	PCI-to-PCI Bridge 

	
	Revision ID:
	0 

	
	Bus Number:
	0 

	
	Device Number:
	5 

	
	Function Number:
	0 

	
	PCI Latency Timer:
	0 

	
	Hardware ID:
	PCI\VEN_1022&DEV_9605&SUBSYS_00000000&REV_00 

	 
	
	

	[PCI Express] 

	
	Version:
	2.0 

	
	Maximum Link Width:
	1x 

	
	Current Link Width:
	1x 

	
	Maximum Link Speed:
	5.0 Gb/s 

	
	Current Link Speed:
	2.5 Gb/s 

	
	Device/Port Type:
	Root Port of PCI Express Root Complex 

	
	Slot Implemented:
	Yes 

	
	Hot-Plug:
	Not Capable 

	
	Hot-Plug Surprise:
	Not Capable 

	
	Slot Power Limit:
	25.000 W 

	
	Active State Power Management (ASPM) Support:
	L0s and L1 

	
	Active State Power Management (ASPM) Status:
	Disabled 

	 
	
	

	[System Resources] 

	
	Interrupt Line:
	IRQ17 

	
	Interrupt Pin:
	INTA# 

	 
	
	

	[Features] 

	
	Bus Mastering:
	Enabled 

	
	Running At 66 MHz:
	Not Capable 

	
	Fast Back-to-Back Transactions:
	Not Capable 

	 
	
	

	[Driver Information] 

	
	Driver Manufacturer:
	(Standardsystemger?e) 

	
	Driver Description:
	PCI Standard-PCI-zu-PCI-Br?ke 

	
	Driver Provider:
	Microsoft 

	
	Driver Version:
	6.1.7601.17514 

	
	Driver Date:
	21-Jun-2006 

	
	DeviceInstanceId
	PCI\VEN_1022&DEV_9605&SUBSYS_96001022&REV_00\3&267A616A&1&28 


	PCI Express x1 Bus #2

	


	
	 
	


	RealTek Semiconductor RTL8168/8111 PCI-E Gigabit Ethernet NIC

	


	
	 
	

	[General Information] 

	
	Device Name:
	RealTek Semiconductor RTL8168/8111 PCI-E Gigabit Ethernet NIC 

	
	Original Device Name:
	RealTek Semiconductor RTL8168/8111 PCI-E Gigabit Ethernet NIC 

	
	Device Class:
	Ethernet Adapter 

	
	Revision ID:
	6 

	
	Bus Number:
	2 

	
	Device Number:
	0 

	
	Function Number:
	0 

	
	PCI Latency Timer:
	0 

	
	Hardware ID:
	PCI\VEN_10EC&DEV_8168&SUBSYS_76411462&REV_06 

	 
	
	

	[PCI Express] 

	
	Version:
	1.1 

	
	Maximum Link Width:
	1x 

	
	Current Link Width:
	1x 

	
	Maximum Link Speed:
	2.5 Gb/s 

	
	Current Link Speed:
	2.5 Gb/s 

	
	Device/Port Type:
	PCI Express Endpoint 

	
	Slot Implemented:
	No 

	
	Active State Power Management (ASPM) Support:
	L0s and L1 

	
	Active State Power Management (ASPM) Status:
	Disabled 

	 
	
	

	[System Resources] 

	
	Interrupt Line:
	N/A 

	
	Interrupt Pin:
	INTA# 

	
	I/O Base Address 0
	E800 

	
	Memory Base Address 2
	FDFFF000 

	
	Memory Base Address 4
	FDFF8000 

	 
	
	

	[Features] 

	
	Bus Mastering:
	Enabled 

	
	Running At 66 MHz:
	Not Capable 

	
	Fast Back-to-Back Transactions:
	Not Capable 

	 
	
	

	[Driver Information] 

	
	Driver Manufacturer:
	Realtek 

	
	Driver Description:
	Realtek PCIe GBE Family Controller 

	
	Driver Provider:
	Realtek 

	
	Driver Version:
	7.67.1226.2012 

	
	Driver Date:
	26-Dec-2012 

	
	DeviceInstanceId
	PCI\VEN_10EC&DEV_8168&SUBSYS_76411462&REV_06\4&3411228A&0&0028 


	ATI/AMD SP5100 (SB700) - SATA (Native IDE) Controller

	


	
	 
	

	[General Information] 

	
	Device Name:
	ATI/AMD SP5100 (SB700) - SATA (Native IDE) Controller 

	
	Original Device Name:
	ATI/AMD SP5100 (SB700) - SATA (Native IDE) Controller 

	
	Device Class:
	IDE Controller 

	
	Revision ID:
	0 

	
	Bus Number:
	0 

	
	Device Number:
	17 

	
	Function Number:
	0 

	
	PCI Latency Timer:
	64 

	
	Hardware ID:
	PCI\VEN_1002&DEV_4390&SUBSYS_76411462&REV_00 

	 
	
	

	[System Resources] 

	
	Interrupt Line:
	IRQ22 

	
	Interrupt Pin:
	INTA# 

	
	I/O Base Address 0
	C000 

	
	I/O Base Address 1
	B000 

	
	I/O Base Address 2
	A000 

	
	I/O Base Address 3
	9000 

	
	I/O Base Address 4
	8000 

	
	Memory Base Address 5
	FEAFFC00 

	 
	
	

	[Features] 

	
	Bus Mastering:
	Enabled 

	
	Running At 66 MHz:
	Capable 

	
	Fast Back-to-Back Transactions:
	Not Capable 

	 
	
	

	[Driver Information] 

	
	Driver Manufacturer:
	(Standard-IDE-ATA/ATAPI-Controller) 

	
	Driver Description:
	Standard-Zweikanal-PCI-IDE-Controller 

	
	Driver Provider:
	Microsoft 

	
	Driver Version:
	6.1.7601.18231 

	
	Driver Date:
	21-Jun-2006 

	
	DeviceInstanceId
	PCI\VEN_1002&DEV_4390&SUBSYS_76411462&REV_00\3&267A616A&1&88 


	ATI/AMD SP5100 (SB700/SB800) - USB OHCI Controller

	


	
	 
	

	[General Information] 

	
	Device Name:
	ATI/AMD SP5100 (SB700/SB800) - USB OHCI Controller 

	
	Original Device Name:
	ATI/AMD SP5100 (SB700/SB800) - USB OHCI Controller 

	
	Device Class:
	Universal Serial Bus (USB) 

	
	Revision ID:
	0 

	
	Bus Number:
	0 

	
	Device Number:
	18 

	
	Function Number:
	0 

	
	PCI Latency Timer:
	64 

	
	Hardware ID:
	PCI\VEN_1002&DEV_4397&SUBSYS_76411462&REV_00 

	 
	
	

	[System Resources] 

	
	Interrupt Line:
	IRQ16 

	
	Interrupt Pin:
	INTA# 

	
	Memory Base Address 0
	FEAFE000 

	 
	
	

	[Features] 

	
	Bus Mastering:
	Enabled 

	
	Running At 66 MHz:
	Capable 

	
	Fast Back-to-Back Transactions:
	Capable 

	 
	
	

	
	USB Version Supported:
	1.0 

	 
	
	

	[Driver Information] 

	
	Driver Manufacturer:
	(Standard-USB-Hostcontroller) 

	
	Driver Description:
	Standard OpenHCD USB-Hostcontroller 

	
	Driver Provider:
	Microsoft 

	
	Driver Version:
	6.1.7601.18328 

	
	Driver Date:
	21-Jun-2006 

	
	DeviceInstanceId
	PCI\VEN_1002&DEV_4397&SUBSYS_76411462&REV_00\3&267A616A&1&90 


	USB Root Hub

	


	
	 
	


	[Port1] : No Device Connected

	


	
	 
	


	[Port2] : No Device Connected

	


	
	 
	


	[Port3] : No Device Connected

	


	
	 
	


	ATI/AMD SP5100 (SB700/SB800) - USB OHCI Controller

	


	
	 
	

	[General Information] 

	
	Device Name:
	ATI/AMD SP5100 (SB700/SB800) - USB OHCI Controller 

	
	Original Device Name:
	ATI/AMD SP5100 (SB700/SB800) - USB OHCI Controller 

	
	Device Class:
	Universal Serial Bus (USB) 

	
	Revision ID:
	0 

	
	Bus Number:
	0 

	
	Device Number:
	18 

	
	Function Number:
	1 

	
	PCI Latency Timer:
	64 

	
	Hardware ID:
	PCI\VEN_1002&DEV_4398&SUBSYS_76411462&REV_00 

	 
	
	

	[System Resources] 

	
	Interrupt Line:
	IRQ16 

	
	Interrupt Pin:
	INTA# 

	
	Memory Base Address 0
	FEAFD000 

	 
	
	

	[Features] 

	
	Bus Mastering:
	Enabled 

	
	Running At 66 MHz:
	Capable 

	
	Fast Back-to-Back Transactions:
	Capable 

	 
	
	

	
	USB Version Supported:
	1.0 

	 
	
	

	[Driver Information] 

	
	Driver Manufacturer:
	(Standard-USB-Hostcontroller) 

	
	Driver Description:
	Standard OpenHCD USB-Hostcontroller 

	
	Driver Provider:
	Microsoft 

	
	Driver Version:
	6.1.7601.18328 

	
	Driver Date:
	21-Jun-2006 

	
	DeviceInstanceId
	PCI\VEN_1002&DEV_4398&SUBSYS_76411462&REV_00\3&267A616A&1&91 


	USB Root Hub

	


	
	 
	


	[Port1] : No Device Connected

	


	
	 
	


	[Port2] : USB-Verbundger?

	


	
	 
	

	[Device Information] 

	
	Device Manufacturer:
	

	
	Product Name:
	

	
	Serial Number:
	

	
	USB Version Supported:
	2.00 

	
	USB Device Speed:
	USB 1.1 Low-speed 

	
	Driver Description:
	USB-Verbundger? 

	
	Hardware ID:
	USB\VID_04F3&PID_0103 

	 
	
	

	[Driver Information] 

	
	Driver Manufacturer:
	(Standard-USB-Hostcontroller) 

	
	Driver Description:
	USB-Verbundger? 

	
	Driver Provider:
	Microsoft 

	
	Driver Version:
	6.1.7601.18328 

	
	Driver Date:
	21-Jun-2006 

	
	DeviceInstanceId
	USB\VID_04F3&PID_0103\5&2BA28D42&0&2 


	[Port3] : USB-Eingabeger?

	


	
	 
	

	[Device Information] 

	
	Device Manufacturer:
	Logitech 

	
	Product Name:
	USB Optical Mouse 

	
	Serial Number:
	N/A 

	
	USB Version Supported:
	2.00 

	
	USB Device Speed:
	USB 1.1 Low-speed 

	
	Driver Description:
	USB-Eingabeger? 

	
	Hardware ID:
	USB\VID_046D&PID_C018 

	 
	
	

	[Driver Information] 

	
	Driver Manufacturer:
	(Standardsystemger?e) 

	
	Driver Description:
	USB-Eingabeger? 

	
	Driver Provider:
	Microsoft 

	
	Driver Version:
	6.1.7601.18199 

	
	Driver Date:
	21-Jun-2006 

	
	DeviceInstanceId
	USB\VID_046D&PID_C018\5&2BA28D42&0&3 


	ATI/AMD SP5100 (SB700/SB800) - USB 2.0 EHCI Controller

	


	
	 
	

	[General Information] 

	
	Device Name:
	ATI/AMD SP5100 (SB700/SB800) - USB 2.0 EHCI Controller 

	
	Original Device Name:
	ATI/AMD SP5100 (SB700/SB800) - USB 2.0 EHCI Controller 

	
	Device Class:
	Universal Serial Bus (USB) 

	
	Revision ID:
	0 

	
	Bus Number:
	0 

	
	Device Number:
	18 

	
	Function Number:
	2 

	
	PCI Latency Timer:
	64 

	
	Hardware ID:
	PCI\VEN_1002&DEV_4396&SUBSYS_76411462&REV_00 

	 
	
	

	[System Resources] 

	
	Interrupt Line:
	IRQ17 

	
	Interrupt Pin:
	INTB# 

	
	Memory Base Address 0
	FEAFF800 

	 
	
	

	[Features] 

	
	Bus Mastering:
	Enabled 

	
	Running At 66 MHz:
	Capable 

	
	Fast Back-to-Back Transactions:
	Capable 

	 
	
	

	
	USB Version Supported:
	2.0 

	 
	
	

	[Driver Information] 

	
	Driver Manufacturer:
	(Standard-USB-Hostcontroller) 

	
	Driver Description:
	Standard PCI-zu-USB erweiterter Hostcontroller 

	
	Driver Provider:
	Microsoft 

	
	Driver Version:
	6.1.7601.18328 

	
	Driver Date:
	21-Jun-2006 

	
	DeviceInstanceId
	PCI\VEN_1002&DEV_4396&SUBSYS_76411462&REV_00\3&267A616A&1&92 


	USB Root Hub

	


	
	 
	


	[Port1] : D-Link DWA-140 Wireless N USB Adapter(rev.D)

	


	
	 
	

	[Device Information] 

	
	Device Manufacturer:
	Ralink 

	
	Product Name:
	802.11 n WLAN 

	
	Serial Number:
	1.0 

	
	USB Version Supported:
	2.00 

	
	USB Device Speed:
	USB 2.0 High-speed 

	
	Driver Description:
	D-Link DWA-140 Wireless N USB Adapter(rev.D) 

	
	Hardware ID:
	USB\VID_2001&PID_3C20 

	 
	
	

	[Driver Information] 

	
	Driver Manufacturer:
	D-Link Corporation 

	
	Driver Description:
	D-Link DWA-140 Wireless N USB Adapter(rev.D) 

	
	Driver Provider:
	D-Link Corporation 

	
	Driver Version:
	5.0.1.0 

	
	Driver Date:
	09-Oct-2012 

	
	DeviceInstanceId
	USB\VID_2001&PID_3C20\1.0 


	[Port2] : No Device Connected

	


	
	 
	


	[Port3] : No Device Connected

	


	
	 
	


	[Port4] : No Device Connected

	


	
	 
	


	[Port5] : No Device Connected

	


	
	 
	


	[Port6] : No Device Connected

	


	
	 
	


	ATI/AMD SP5100 (SB700/SB800) - USB OHCI Controller

	


	
	 
	

	[General Information] 

	
	Device Name:
	ATI/AMD SP5100 (SB700/SB800) - USB OHCI Controller 

	
	Original Device Name:
	ATI/AMD SP5100 (SB700/SB800) - USB OHCI Controller 

	
	Device Class:
	Universal Serial Bus (USB) 

	
	Revision ID:
	0 

	
	Bus Number:
	0 

	
	Device Number:
	19 

	
	Function Number:
	0 

	
	PCI Latency Timer:
	64 

	
	Hardware ID:
	PCI\VEN_1002&DEV_4397&SUBSYS_76411462&REV_00 

	 
	
	

	[System Resources] 

	
	Interrupt Line:
	IRQ18 

	
	Interrupt Pin:
	INTA# 

	
	Memory Base Address 0
	FEAFC000 

	 
	
	

	[Features] 

	
	Bus Mastering:
	Enabled 

	
	Running At 66 MHz:
	Capable 

	
	Fast Back-to-Back Transactions:
	Capable 

	 
	
	

	
	USB Version Supported:
	1.0 

	 
	
	

	[Driver Information] 

	
	Driver Manufacturer:
	(Standard-USB-Hostcontroller) 

	
	Driver Description:
	Standard OpenHCD USB-Hostcontroller 

	
	Driver Provider:
	Microsoft 

	
	Driver Version:
	6.1.7601.18328 

	
	Driver Date:
	21-Jun-2006 

	
	DeviceInstanceId
	PCI\VEN_1002&DEV_4397&SUBSYS_76411462&REV_00\3&267A616A&1&98 


	USB Root Hub

	


	
	 
	


	[Port1] : No Device Connected

	


	
	 
	


	[Port2] : No Device Connected

	


	
	 
	


	[Port3] : No Device Connected

	


	
	 
	


	ATI/AMD SP5100 (SB700/SB800) - USB OHCI Controller

	


	
	 
	

	[General Information] 

	
	Device Name:
	ATI/AMD SP5100 (SB700/SB800) - USB OHCI Controller 

	
	Original Device Name:
	ATI/AMD SP5100 (SB700/SB800) - USB OHCI Controller 

	
	Device Class:
	Universal Serial Bus (USB) 

	
	Revision ID:
	0 

	
	Bus Number:
	0 

	
	Device Number:
	19 

	
	Function Number:
	1 

	
	PCI Latency Timer:
	64 

	
	Hardware ID:
	PCI\VEN_1002&DEV_4398&SUBSYS_76411462&REV_00 

	 
	
	

	[System Resources] 

	
	Interrupt Line:
	IRQ18 

	
	Interrupt Pin:
	INTA# 

	
	Memory Base Address 0
	FEAFB000 

	 
	
	

	[Features] 

	
	Bus Mastering:
	Enabled 

	
	Running At 66 MHz:
	Capable 

	
	Fast Back-to-Back Transactions:
	Capable 

	 
	
	

	
	USB Version Supported:
	1.0 

	 
	
	

	[Driver Information] 

	
	Driver Manufacturer:
	(Standard-USB-Hostcontroller) 

	
	Driver Description:
	Standard OpenHCD USB-Hostcontroller 

	
	Driver Provider:
	Microsoft 

	
	Driver Version:
	6.1.7601.18328 

	
	Driver Date:
	21-Jun-2006 

	
	DeviceInstanceId
	PCI\VEN_1002&DEV_4398&SUBSYS_76411462&REV_00\3&267A616A&1&99 


	USB Root Hub

	


	
	 
	


	[Port1] : No Device Connected

	


	
	 
	


	[Port2] : No Device Connected

	


	
	 
	


	[Port3] : No Device Connected

	


	
	 
	


	ATI/AMD SP5100 (SB700/SB800) - USB 2.0 EHCI Controller

	


	
	 
	

	[General Information] 

	
	Device Name:
	ATI/AMD SP5100 (SB700/SB800) - USB 2.0 EHCI Controller 

	
	Original Device Name:
	ATI/AMD SP5100 (SB700/SB800) - USB 2.0 EHCI Controller 

	
	Device Class:
	Universal Serial Bus (USB) 

	
	Revision ID:
	0 

	
	Bus Number:
	0 

	
	Device Number:
	19 

	
	Function Number:
	2 

	
	PCI Latency Timer:
	64 

	
	Hardware ID:
	PCI\VEN_1002&DEV_4396&SUBSYS_43961002&REV_00 

	 
	
	

	[System Resources] 

	
	Interrupt Line:
	IRQ19 

	
	Interrupt Pin:
	INTB# 

	
	Memory Base Address 0
	FEAFF400 

	 
	
	

	[Features] 

	
	Bus Mastering:
	Enabled 

	
	Running At 66 MHz:
	Capable 

	
	Fast Back-to-Back Transactions:
	Capable 

	 
	
	

	
	USB Version Supported:
	2.0 

	 
	
	

	[Driver Information] 

	
	Driver Manufacturer:
	(Standard-USB-Hostcontroller) 

	
	Driver Description:
	Standard PCI-zu-USB erweiterter Hostcontroller 

	
	Driver Provider:
	Microsoft 

	
	Driver Version:
	6.1.7601.18328 

	
	Driver Date:
	21-Jun-2006 

	
	DeviceInstanceId
	PCI\VEN_1002&DEV_4396&SUBSYS_43961002&REV_00\3&267A616A&1&9A 


	USB Root Hub

	


	
	 
	


	[Port1] : USB-Massenspeicherger?

	


	
	 
	

	[Device Information] 

	
	Device Manufacturer:
	Western Digital 

	
	Product Name:
	Ext HDD 1021 

	
	Serial Number:
	5743415A414C333630383738 

	
	USB Version Supported:
	2.00 

	
	USB Device Speed:
	USB 2.0 High-speed 

	
	Driver Description:
	USB-Massenspeicherger? 

	
	Hardware ID:
	USB\VID_1058&PID_1021 

	 
	
	

	[Driver Information] 

	
	Driver Manufacturer:
	Kompatibles USB-Speicherger? 

	
	Driver Description:
	USB-Massenspeicherger? 

	
	Driver Provider:
	Microsoft 

	
	Driver Version:
	6.1.7601.17577 

	
	Driver Date:
	21-Jun-2006 

	
	DeviceInstanceId
	USB\VID_1058&PID_1021\5743415A414C333630383738 


	[Port2] : USB-Massenspeicherger?

	


	
	 
	

	[Device Information] 

	
	Device Manufacturer:
	Generic 

	
	Product Name:
	Mass Storage Device 

	
	Serial Number:
	058F63666471 

	
	USB Version Supported:
	2.00 

	
	USB Device Speed:
	USB 2.0 High-speed 

	
	Driver Description:
	USB-Massenspeicherger? 

	
	Hardware ID:
	USB\VID_058F&PID_6366 

	 
	
	

	[Driver Information] 

	
	Driver Manufacturer:
	Kompatibles USB-Speicherger? 

	
	Driver Description:
	USB-Massenspeicherger? 

	
	Driver Provider:
	Microsoft 

	
	Driver Version:
	6.1.7601.17577 

	
	Driver Date:
	21-Jun-2006 

	
	DeviceInstanceId
	USB\VID_058F&PID_6366\058F63666471 


	[Port3] : No Device Connected

	


	
	 
	


	[Port4] : No Device Connected

	


	
	 
	


	[Port5] : No Device Connected

	


	
	 
	


	[Port6] : No Device Connected

	


	
	 
	


	ATI/AMD SP5100 (SB700) - SMBus and ACPI Controller [A14]

	


	
	 
	

	[General Information] 

	
	Device Name:
	ATI/AMD SP5100 (SB700) - SMBus and ACPI Controller [A14] 

	
	Original Device Name:
	ATI/AMD SP5100 (SB700) - SMBus and ACPI Controller [A14] 

	
	Device Class:
	SMBus (System Management Bus) 

	
	Revision ID:
	3C 

	
	Bus Number:
	0 

	
	Device Number:
	20 

	
	Function Number:
	0 

	
	PCI Latency Timer:
	0 

	
	Hardware ID:
	PCI\VEN_1002&DEV_4385&SUBSYS_76411462&REV_3C 

	 
	
	

	[System Resources] 

	
	Interrupt Line:
	N/A 

	
	Interrupt Pin:
	N/A 

	 
	
	

	[Features] 

	
	Bus Mastering:
	Disabled 

	
	Running At 66 MHz:
	Capable 

	
	Fast Back-to-Back Transactions:
	Not Capable 

	 
	
	

	[Driver Information] 

	
	Driver Manufacturer:
	Advanced Micro Devices, Inc 

	
	Driver Description:
	AMD SMBus 

	
	Driver Provider:
	Advanced Micro Devices, Inc 

	
	Driver Version:
	5.12.0.15 

	
	Driver Date:
	16-Mar-2011 

	
	DeviceInstanceId
	PCI\VEN_1002&DEV_4385&SUBSYS_76411462&REV_3C\3&267A616A&1&A0 


	ATI/AMD SP5100 (SB700) - IDE Controller

	


	
	 
	

	[General Information] 

	
	Device Name:
	ATI/AMD SP5100 (SB700) - IDE Controller 

	
	Original Device Name:
	ATI/AMD SP5100 (SB700) - IDE Controller 

	
	Device Class:
	IDE Controller 

	
	Revision ID:
	0 

	
	Bus Number:
	0 

	
	Device Number:
	20 

	
	Function Number:
	1 

	
	PCI Latency Timer:
	0 

	
	Hardware ID:
	PCI\VEN_1002&DEV_439C&SUBSYS_76411462&REV_00 

	 
	
	

	[System Resources] 

	
	Interrupt Line:
	N/A 

	
	Interrupt Pin:
	INTA# 

	
	I/O Base Address 0
	0 

	
	I/O Base Address 1
	0 

	
	I/O Base Address 2
	0 

	
	I/O Base Address 3
	0 

	
	I/O Base Address 4
	FF00 

	 
	
	

	[Features] 

	
	Bus Mastering:
	Enabled 

	
	Running At 66 MHz:
	Capable 

	
	Fast Back-to-Back Transactions:
	Not Capable 

	 
	
	

	[Driver Information] 

	
	Driver Manufacturer:
	(Standard-IDE-ATA/ATAPI-Controller) 

	
	Driver Description:
	Standard-Zweikanal-PCI-IDE-Controller 

	
	Driver Provider:
	Microsoft 

	
	Driver Version:
	6.1.7601.18231 

	
	Driver Date:
	21-Jun-2006 

	
	DeviceInstanceId
	PCI\VEN_1002&DEV_439C&SUBSYS_76411462&REV_00\3&267A616A&1&A1 


	ATI/AMD SB600 - High Definition Audio Controller

	


	
	 
	

	[General Information] 

	
	Device Name:
	ATI/AMD SB600 - High Definition Audio Controller 

	
	Original Device Name:
	ATI/AMD SB600 - High Definition Audio Controller 

	
	Device Class:
	Mixed mode device 

	
	Revision ID:
	0 

	
	Bus Number:
	0 

	
	Device Number:
	20 

	
	Function Number:
	2 

	
	PCI Latency Timer:
	64 

	
	Hardware ID:
	PCI\VEN_1002&DEV_4383&SUBSYS_F6411462&REV_00 

	 
	
	

	[System Resources] 

	
	Interrupt Line:
	IRQ16 

	
	Interrupt Pin:
	INTA# 

	
	Memory Base Address 0
	FEAF4000 

	 
	
	

	[Features] 

	
	Bus Mastering:
	Enabled 

	
	Running At 66 MHz:
	Not Capable 

	
	Fast Back-to-Back Transactions:
	Not Capable 

	 
	
	

	[Driver Information] 

	
	Driver Manufacturer:
	Microsoft 

	
	Driver Description:
	High Definition Audio-Controller 

	
	Driver Provider:
	Microsoft 

	
	Driver Version:
	6.1.7601.17514 

	
	Driver Date:
	19-Nov-2010 

	
	DeviceInstanceId
	PCI\VEN_1002&DEV_4383&SUBSYS_F6411462&REV_00\3&267A616A&1&A2 


	ATI/AMD SP5100 (SB700) - LPC Bridge

	


	
	 
	

	[General Information] 

	
	Device Name:
	ATI/AMD SP5100 (SB700) - LPC Bridge 

	
	Original Device Name:
	ATI/AMD SP5100 (SB700) - LPC Bridge 

	
	Device Class:
	PCI-to-ISA Bridge 

	
	Revision ID:
	0 

	
	Bus Number:
	0 

	
	Device Number:
	20 

	
	Function Number:
	3 

	
	PCI Latency Timer:
	0 

	
	Hardware ID:
	PCI\VEN_1002&DEV_439D&SUBSYS_76411462&REV_00 

	 
	
	

	[System Resources] 

	
	Interrupt Line:
	N/A 

	
	Interrupt Pin:
	N/A 

	 
	
	

	[Features] 

	
	Bus Mastering:
	Enabled 

	
	Running At 66 MHz:
	Capable 

	
	Fast Back-to-Back Transactions:
	Not Capable 

	 
	
	

	[Driver Information] 

	
	Driver Manufacturer:
	(Standardsystemger?e) 

	
	Driver Description:
	PCI Standard-ISA-Br?ke 

	
	Driver Provider:
	Microsoft 

	
	Driver Version:
	6.1.7601.17514 

	
	Driver Date:
	21-Jun-2006 

	
	DeviceInstanceId
	PCI\VEN_1002&DEV_439D&SUBSYS_76411462&REV_00\3&267A616A&1&A3 


	ATI/AMD SB600/SB700 - PCI-to-PCI Host Bridge

	


	
	 
	

	[General Information] 

	
	Device Name:
	ATI/AMD SB600/SB700 - PCI-to-PCI Host Bridge 

	
	Original Device Name:
	ATI/AMD SB600/SB700 - PCI-to-PCI Host Bridge 

	
	Device Class:
	PCI-to-PCI Bridge 

	
	Revision ID:
	0 

	
	Bus Number:
	0 

	
	Device Number:
	20 

	
	Function Number:
	4 

	
	PCI Latency Timer:
	64 

	
	Hardware ID:
	PCI\VEN_1002&DEV_4384&SUBSYS_00000000&REV_00 

	 
	
	

	[System Resources] 

	
	Interrupt Line:
	N/A 

	
	Interrupt Pin:
	N/A 

	 
	
	

	[Features] 

	
	Bus Mastering:
	Enabled 

	
	Running At 66 MHz:
	Capable 

	
	Fast Back-to-Back Transactions:
	Capable 

	 
	
	

	[Driver Information] 

	
	Driver Manufacturer:
	ATI 

	
	Driver Description:
	ATI E/A-Kommunikationsprozessor-PCI-Buscontroller 

	
	Driver Provider:
	Microsoft 

	
	Driver Version:
	6.1.7601.17514 

	
	Driver Date:
	21-Jun-2006 

	
	DeviceInstanceId
	PCI\VEN_1002&DEV_4384&SUBSYS_00000000&REV_00\3&267A616A&1&A4 


	PCI Bus #3

	


	
	 
	


	ATI/AMD SP5100 (SB700/SB800) - USB OHCI Controller

	


	
	 
	

	[General Information] 

	
	Device Name:
	ATI/AMD SP5100 (SB700/SB800) - USB OHCI Controller 

	
	Original Device Name:
	ATI/AMD SP5100 (SB700/SB800) - USB OHCI Controller 

	
	Device Class:
	Universal Serial Bus (USB) 

	
	Revision ID:
	0 

	
	Bus Number:
	0 

	
	Device Number:
	20 

	
	Function Number:
	5 

	
	PCI Latency Timer:
	64 

	
	Hardware ID:
	PCI\VEN_1002&DEV_4399&SUBSYS_43961002&REV_00 

	 
	
	

	[System Resources] 

	
	Interrupt Line:
	IRQ18 

	
	Interrupt Pin:
	INTC# 

	
	Memory Base Address 0
	FEAFA000 

	 
	
	

	[Features] 

	
	Bus Mastering:
	Enabled 

	
	Running At 66 MHz:
	Capable 

	
	Fast Back-to-Back Transactions:
	Capable 

	 
	
	

	
	USB Version Supported:
	1.0 

	 
	
	

	[Driver Information] 

	
	Driver Manufacturer:
	(Standard-USB-Hostcontroller) 

	
	Driver Description:
	Standard OpenHCD USB-Hostcontroller 

	
	Driver Provider:
	Microsoft 

	
	Driver Version:
	6.1.7601.18328 

	
	Driver Date:
	21-Jun-2006 

	
	DeviceInstanceId
	PCI\VEN_1002&DEV_4399&SUBSYS_43961002&REV_00\3&267A616A&1&A5 


	USB Root Hub

	


	
	 
	


	[Port1] : No Device Connected

	


	
	 
	


	[Port2] : No Device Connected

	


	
	 
	


	AMD Family 15h Models 00h-0Fh CPU - HyperTransport Technology Configuration

	


	
	 
	

	[General Information] 

	
	Device Name:
	AMD Family 15h Models 00h-0Fh CPU - HyperTransport Technology Configuration 

	
	Original Device Name:
	AMD Family 15h Models 00h-0Fh CPU - HyperTransport Technology Configuration 

	
	Device Class:
	Host-to-PCI Bridge 

	
	Revision ID:
	0 

	
	Bus Number:
	0 

	
	Device Number:
	24 

	
	Function Number:
	0 

	
	PCI Latency Timer:
	0 

	
	Hardware ID:
	PCI\VEN_1022&DEV_1600&SUBSYS_00000000&REV_00 

	 
	
	

	[System Resources] 

	
	Interrupt Line:
	N/A 

	
	Interrupt Pin:
	N/A 

	 
	
	

	[Features] 

	
	Bus Mastering:
	Disabled 

	
	Running At 66 MHz:
	Not Capable 

	
	Fast Back-to-Back Transactions:
	Not Capable 

	 
	
	

	[Driver Information] 

	
	Driver Manufacturer:
	(Standardsystemger?e) 

	
	Driver Description:
	PCI Standard-Host-CPU-Br?ke 

	
	Driver Provider:
	Microsoft 

	
	Driver Version:
	6.1.7601.17514 

	
	Driver Date:
	21-Jun-2006 

	
	DeviceInstanceId
	PCI\VEN_1022&DEV_1600&SUBSYS_00000000&REV_00\3&267A616A&1&C0 


	AMD Family 15h Models 00h-0Fh CPU - Address Map

	


	
	 
	

	[General Information] 

	
	Device Name:
	AMD Family 15h Models 00h-0Fh CPU - Address Map 

	
	Original Device Name:
	AMD Family 15h Models 00h-0Fh CPU - Address Map 

	
	Device Class:
	Host-to-PCI Bridge 

	
	Revision ID:
	0 

	
	Bus Number:
	0 

	
	Device Number:
	24 

	
	Function Number:
	1 

	
	PCI Latency Timer:
	0 

	
	Hardware ID:
	PCI\VEN_1022&DEV_1601&SUBSYS_00000000&REV_00 

	 
	
	

	[System Resources] 

	
	Interrupt Line:
	N/A 

	
	Interrupt Pin:
	N/A 

	 
	
	

	[Features] 

	
	Bus Mastering:
	Disabled 

	
	Running At 66 MHz:
	Not Capable 

	
	Fast Back-to-Back Transactions:
	Not Capable 

	 
	
	

	[Driver Information] 

	
	Driver Manufacturer:
	(Standardsystemger?e) 

	
	Driver Description:
	PCI Standard-Host-CPU-Br?ke 

	
	Driver Provider:
	Microsoft 

	
	Driver Version:
	6.1.7601.17514 

	
	Driver Date:
	21-Jun-2006 

	
	DeviceInstanceId
	PCI\VEN_1022&DEV_1601&SUBSYS_00000000&REV_00\3&267A616A&1&C1 


	AMD Family 15h Models 00h-0Fh CPU - DRAM Controller

	


	
	 
	

	[General Information] 

	
	Device Name:
	AMD Family 15h Models 00h-0Fh CPU - DRAM Controller 

	
	Original Device Name:
	AMD Family 15h Models 00h-0Fh CPU - DRAM Controller 

	
	Device Class:
	Host-to-PCI Bridge 

	
	Revision ID:
	0 

	
	Bus Number:
	0 

	
	Device Number:
	24 

	
	Function Number:
	2 

	
	PCI Latency Timer:
	0 

	
	Hardware ID:
	PCI\VEN_1022&DEV_1602&SUBSYS_00000000&REV_00 

	 
	
	

	[System Resources] 

	
	Interrupt Line:
	N/A 

	
	Interrupt Pin:
	N/A 

	 
	
	

	[Features] 

	
	Bus Mastering:
	Disabled 

	
	Running At 66 MHz:
	Not Capable 

	
	Fast Back-to-Back Transactions:
	Not Capable 

	 
	
	

	[Driver Information] 

	
	Driver Manufacturer:
	(Standardsystemger?e) 

	
	Driver Description:
	PCI Standard-Host-CPU-Br?ke 

	
	Driver Provider:
	Microsoft 

	
	Driver Version:
	6.1.7601.17514 

	
	Driver Date:
	21-Jun-2006 

	
	DeviceInstanceId
	PCI\VEN_1022&DEV_1602&SUBSYS_00000000&REV_00\3&267A616A&1&C2 


	AMD Family 15h Models 00h-0Fh CPU - Miscellaneous Control

	


	
	 
	

	[General Information] 

	
	Device Name:
	AMD Family 15h Models 00h-0Fh CPU - Miscellaneous Control 

	
	Original Device Name:
	AMD Family 15h Models 00h-0Fh CPU - Miscellaneous Control 

	
	Device Class:
	Host-to-PCI Bridge 

	
	Revision ID:
	0 

	
	Bus Number:
	0 

	
	Device Number:
	24 

	
	Function Number:
	3 

	
	PCI Latency Timer:
	0 

	
	Hardware ID:
	PCI\VEN_1022&DEV_1603&SUBSYS_00000000&REV_00 

	 
	
	

	[System Resources] 

	
	Interrupt Line:
	N/A 

	
	Interrupt Pin:
	N/A 

	 
	
	

	[Features] 

	
	Bus Mastering:
	Disabled 

	
	Running At 66 MHz:
	Not Capable 

	
	Fast Back-to-Back Transactions:
	Not Capable 

	 
	
	

	[Driver Information] 

	
	Driver Manufacturer:
	(Standardsystemger?e) 

	
	Driver Description:
	PCI Standard-Host-CPU-Br?ke 

	
	Driver Provider:
	Microsoft 

	
	Driver Version:
	6.1.7601.17514 

	
	Driver Date:
	21-Jun-2006 

	
	DeviceInstanceId
	PCI\VEN_1022&DEV_1603&SUBSYS_00000000&REV_00\3&267A616A&1&C3 


	AMD Family 15h Models 00h-0Fh CPU - Miscellaneous Control 2

	


	
	 
	

	[General Information] 

	
	Device Name:
	AMD Family 15h Models 00h-0Fh CPU - Miscellaneous Control 2 

	
	Original Device Name:
	AMD Family 15h Models 00h-0Fh CPU - Miscellaneous Control 2 

	
	Device Class:
	Host-to-PCI Bridge 

	
	Revision ID:
	0 

	
	Bus Number:
	0 

	
	Device Number:
	24 

	
	Function Number:
	4 

	
	PCI Latency Timer:
	0 

	
	Hardware ID:
	PCI\VEN_1022&DEV_1604&SUBSYS_00000000&REV_00 

	 
	
	

	[System Resources] 

	
	Interrupt Line:
	N/A 

	
	Interrupt Pin:
	N/A 

	 
	
	

	[Features] 

	
	Bus Mastering:
	Disabled 

	
	Running At 66 MHz:
	Not Capable 

	
	Fast Back-to-Back Transactions:
	Not Capable 

	 
	
	

	[Driver Information] 

	
	Driver Manufacturer:
	(Standardsystemger?e) 

	
	Driver Description:
	PCI Standard-Host-CPU-Br?ke 

	
	Driver Provider:
	Microsoft 

	
	Driver Version:
	6.1.7601.17514 

	
	Driver Date:
	21-Jun-2006 

	
	DeviceInstanceId
	PCI\VEN_1022&DEV_1604&SUBSYS_00000000&REV_00\3&267A616A&1&C4 


	AMD Family 15h Models 00h-0Fh CPU - Miscellaneous Control 3

	


	
	 
	

	[General Information] 

	
	Device Name:
	AMD Family 15h Models 00h-0Fh CPU - Miscellaneous Control 3 

	
	Original Device Name:
	AMD Family 15h Models 00h-0Fh CPU - Miscellaneous Control 3 

	
	Device Class:
	Host-to-PCI Bridge 

	
	Revision ID:
	0 

	
	Bus Number:
	0 

	
	Device Number:
	24 

	
	Function Number:
	5 

	
	PCI Latency Timer:
	0 

	
	Hardware ID:
	PCI\VEN_1022&DEV_1605&SUBSYS_00000000&REV_00 

	 
	
	

	[System Resources] 

	
	Interrupt Line:
	N/A 

	
	Interrupt Pin:
	N/A 

	 
	
	

	[Features] 

	
	Bus Mastering:
	Disabled 

	
	Running At 66 MHz:
	Not Capable 

	
	Fast Back-to-Back Transactions:
	Not Capable 

	 
	
	

	[Driver Information] 

	
	Driver Manufacturer:
	(Standardsystemger?e) 

	
	Driver Description:
	PCI Standard-Host-CPU-Br?ke 

	
	Driver Provider:
	Microsoft 

	
	Driver Version:
	6.1.7601.17514 

	
	Driver Date:
	21-Jun-2006 

	
	DeviceInstanceId
	PCI\VEN_1022&DEV_1605&SUBSYS_00000000&REV_00\3&267A616A&1&C5 


	Video Adapter

	


	
	 
	


	ATI/AMD Radeon HD 5450/5470/5490/5530/6230/6250/6290

	


	
	 
	

	[Video chipset] 

	
	Video Chipset:
	ATI/AMD Radeon HD 5450/5470/5490/5530/6230/6250/6290 

	
	Video Chipset Codename:
	CEDAR PRO 

	
	Video Memory:
	1024 MBytes of DDR3 SDRAM 

	 
	
	

	[Video Card] 

	
	Video Card:
	PowerColor Radeon HD 8350 

	
	Video Bus:
	PCIe v2.0 x16 (5.0 Gb/s) @ x16 (5.0 Gb/s) 

	
	Video RAMDAC:
	Internal DAC(400MHz) 

	
	Video BIOS Version:
	012.020.000.062.000000 

	 
	
	

	[Performance] 

	
	Processor Clock:
	157.0 MHz 

	
	Memory Clock:
	399.9 MHz (Effective 799.9 MHz) 

	
	Memory Bus Width:
	64-bit 

	
	Number Of ROPs:
	8 

	
	Number Of Unified Shaders:
	80 

	 
	
	

	
	ASIC Serial Number:
	3815067049175 

	 
	
	

	
	Hardware ID:
	PCI\VEN_1002&DEV_68F9&SUBSYS_8350148C&REV_00 

	
	PCI Location (Bus:Dev:Fnc):
	1:00:0 

	 
	
	

	[Driver Information] 

	
	Driver Manufacturer:
	Advanced Micro Devices, Inc. 

	
	Driver Description:
	AMD Radeon HD8350 

	
	Driver Provider:
	Advanced Micro Devices, Inc. 

	
	Driver Version:
	14.501.1003.0 

	
	Driver Date:
	20-Nov-2014 

	
	DeviceInstanceId
	PCI\VEN_1002&DEV_68F9&SUBSYS_8350148C&REV_00\4&D378CAC&0&0010 


	Monitor

	


	
	 
	


	Acer [Unknown Model: ACR02FF]

	


	
	 
	

	[General information] 

	
	Monitor Name:
	Acer [Unknown Model: ACR02FF] 

	
	Monitor Name (Manuf):
	G246HL 

	
	Serial Number:
	LWAEE0188563 

	
	Date Of Manufacture:
	Week: 13, Year: 2013 

	
	Monitor Hardware ID:
	Monitor\ACR02FF 

	 
	
	

	
	Max. Vertical Size:
	30 cm 

	
	Max. Horizontal Size:
	53 cm 

	
	Horizontal Frequency:
	30 - 80 kHz 

	
	Vertical Frequency:
	55 - 76 Hz 

	
	Maximum Pixel Clock:
	170 MHz 

	 
	
	

	[Advanced parameters] 

	
	Input Signal:
	Analog: 0.700 V / 0.000 V (0.700 V p-p) 

	
	Display Type:
	RGB color 

	
	Gamma Factor:
	2.20 

	 
	
	

	[DPMS Modes] 

	
	Standby:
	Supported 

	
	Suspend:
	Supported 

	
	Active Off:
	Not Supported 

	
	Standard Colour Space:
	Not Supported 

	
	Preferred Timing Mode:
	Supported 

	
	Default GTF Supported:
	Not Supported 

	 
	
	

	[DPMS Input Signal] 

	
	Serration VSync:
	Not Supported 

	
	Sync On Green:
	Not Supported 

	
	Composite Sync:
	Not Supported 

	
	Separate Syncs:
	Supported 

	
	Blank-to-black Setup:
	Not Supported 

	 
	
	

	[Supported Video Modes] 

	
	1152 x 864
	75 Hz 

	
	1280 x 960
	60 Hz 

	
	1280 x 1024
	60 Hz 

	
	1280 x 720
	60 Hz 

	
	1280 x 800
	60 Hz 

	
	1440 x 900
	60 Hz 

	
	1680 x 1050
	60 Hz 

	
	1920 x 1080
	60 Hz 

	
	1920 x 1080
	531 x 299 mm, Pixel Clock 148.50 MHz 


	Drives

	


	
	 
	


	Floppy Drives

	


	
	 
	


	(S)ATA/ATAPI Drives

	


	
	 
	


	Hitachi HDS5C3020BLE630

	


	
	 
	

	[General Information] 

	
	Drive Controller:
	Serial ATA 6Gb/s @ 3Gb/s 

	
	Drive Model:
	Hitachi HDS5C3020BLE630 

	
	Drive Revision:
	MZ4OAAB0 

	
	Drive Serial Number:
	MCE7215P0TDUZV 

	
	World Wide Name:
	5000CCA37DCB1919 

	
	Drive Capacity:
	1,907,729 MBytes (2000 GB) 

	
	Drive Capacity [MB]:
	1907729 

	
	Media Rotation Rate:
	5700 RPM 

	
	Nominal Form Factor:
	3.5" 

	 
	
	

	[Drive Geometry] 

	
	Number of Cylinders:
	16383 

	
	Number of Heads:
	16 

	
	Sectors Per Track:
	63 

	
	Number Of ECC Bytes:
	56 

	
	Number of Sectors:
	16514064 

	
	Total 32-bit LBA Sectors:
	268435455 

	
	Total 48-bit LBA Sectors:
	3907029168 

	
	Cache Buffer Size:
	22756 KBytes 

	
	Controller Type:
	Dual Ported, Multiple Sector Buffer, Read Cache 

	 
	
	

	[Transfer Modes] 

	
	Sectors Per Interrupt:
	Total: 16, Active: 16 

	
	Max. PIO Transfer Mode:
	4 

	
	Multiword DMA Mode:
	Total: 2, Active: - 

	
	Singleword DMA Mode:
	Total: -, Active: - 

	
	Ultra-DMA Mode:
	Total: 6 (ATA-133), Active: 6 (ATA-133) 

	
	Max. Multiword DMA Transfer Rate:
	16.7 MBytes/s 

	
	Max. PIO with IORDY Transfer Rate:
	16.7 MBytes/s 

	
	Max. PIO w/o IORDY Transfer Rate:
	16.7 MBytes/s 

	
	Transfer Width:
	Unknown 

	
	Native Command Queuing:
	Supported, Max. Depth: 32 

	
	TRIM Command:
	Not Supported 

	 
	
	

	[Device flags] 

	
	Fixed Drive:
	Present 

	
	Removable Drive:
	Not Present 

	
	Magnetic Storage:
	Present 

	
	LBA Mode:
	Supported 

	
	DMA Mode:
	Supported 

	
	IORDY:
	Supported 

	
	IORDY Disableable:
	Supported 

	 
	
	

	[Features] 

	
	Write Cache:
	Present, Active 

	
	S.M.A.R.T. Feature:
	Present, Active 

	
	Security Feature:
	Present, Inactive 

	
	Removable Media Feature:
	Not Present, Disabled 

	
	Power Management:
	Present, Active 

	
	Advanced Power Management:
	Present, Inactive 

	
	Packet Interface:
	Not Present, Disabled 

	
	Look-Ahead Buffer:
	Present, Active 

	
	Host Protected Area:
	Present, Enabled 

	
	Power-Up In Standby:
	Supported, Inactive 

	
	Automatic Acoustic Management:
	Not Suppported, Inactive 

	
	48-bit LBA:
	Supported, Active 

	
	Host-Initiated Link Power Management:
	Supported 

	
	Device-Initiated Link Power Management:
	Supported, Disabled 

	
	In-Order Data Delivery:
	Supported, Disabled 

	
	Hardware Feature Control:
	Not Supported 

	
	Software Settings Preservation:
	Supported, Enabled 

	
	NCQ Autosense:
	Not Supported 

	
	Link Power State Device Sleep:
	Not Supported 

	
	Hybrid Information Feature:
	Not Supported 

	
	All Write Cache Non-Volatile:
	Not Supported 

	
	Extended Number of User Addressable Sectors:
	Not Supported 

	
	Device Encrypts All User Data:
	Not Supported 

	
	CFast Specification:
	Not Supported 

	
	NCQ Priority Information:
	Supported 

	
	Host Automatic Partial to Slumber Transitions:
	Not Supported 

	
	Device Automatic Partial to Slumber Transitions:
	Not Supported 

	
	NCQ Streaming:
	Not Supported 

	
	NCQ Queue Management Command:
	Not Supported 

	
	DEVSLP to Reduced Power State:
	Not Supported 

	
	Extended Power Conditions Feature:
	Supported, Enabled 

	
	Sense Data Reporting Feature:
	Not Supported 

	
	Free-Fall Control Feature:
	Not Supported 

	 
	
	

	[Self-Monitoring, Analysis and Reporting Technology (S.M.A.R.T.)] 

	
	[01] Raw Read Error Rate:
	100/16, Worst: 100 

	
	[02] Throughput Performance:
	141/54, Worst: 141 (Data = 98) 

	
	[03] Spin Up Time:
	132/24, Worst: 132 (Data = 17170697) 

	
	[04] Start/Stop Count:
	100/Always OK, Worst: 100 (Data = 1018) 

	
	[05] Reallocated Sector Count:
	100/5, Worst: 100 

	
	[07] Seek Error Rate:
	100/67, Worst: 100 

	
	[08] Seek Time Performance:
	138/20, Worst: 138 (Data = 33) 

	
	[09] Power-On Hours/Cycle Count:
	99/Always OK, Worst: 99 (Data = 11358 hours / 1.30 years) 

	
	[0A] Spin Retry Count:
	100/60, Worst: 100 

	
	[0C] Power Cycle Count:
	100/Always OK, Worst: 100 (Data = 953) 

	
	[C0] Power-Off Retract Count:
	100/Always OK, Worst: 100 (Data = 1036) 

	
	[C1] Load/Unload Cycle Count:
	100/Always OK, Worst: 100 (Data = 1036) 

	
	[C2] Temperature
	157/Always OK, Worst: 157 (Data = 38.0 ﾰC) 

	
	[C4] Reallocation Event Count:
	100/Always OK, Worst: 100 

	
	[C5] Current Pending Sector Count:
	100/Always OK, Worst: 100 

	
	[C6] Off-Line Uncorrectable Sector Count:
	100/Always OK, Worst: 100 

	
	[C7] UltraDMA/SATA CRC Error Rate:
	200/Always OK, Worst: 200 


	WDC WD20EARX-008FB0

	


	
	 
	

	[General Information] 

	
	Drive Controller:
	Serial ATA 6Gb/s @ 1.5Gb/s <-> USB 

	
	Drive Model:
	WDC WD20EARX-008FB0 

	
	Drive Revision:
	51.0AB51 

	
	Drive Serial Number:
	WD-WCAZAL360878 

	
	World Wide Name:
	50014EE28247E2D 

	
	Drive Capacity:
	1,907,729 MBytes (2000 GB) 

	
	Drive Capacity [MB]:
	1907729 

	 
	
	

	[Drive Geometry] 

	
	Number of Cylinders:
	16383 

	
	Number of Heads:
	16 

	
	Sectors Per Track:
	63 

	
	Number of Sectors:
	16514064 

	
	Total 32-bit LBA Sectors:
	268435455 

	
	Total 48-bit LBA Sectors:
	3907029168 

	
	Cache Buffer Size:
	N/A 

	 
	
	

	[Transfer Modes] 

	
	Sectors Per Interrupt:
	Total: 16, Active: 0 

	
	Max. PIO Transfer Mode:
	4 

	
	Multiword DMA Mode:
	Total: 2, Active: 0 

	
	Singleword DMA Mode:
	Total: -, Active: - 

	
	Ultra-DMA Mode:
	Total: 6 (ATA-133), Inactive 

	
	Max. Multiword DMA Transfer Rate:
	16.7 MBytes/s 

	
	Max. PIO with IORDY Transfer Rate:
	16.7 MBytes/s 

	
	Max. PIO w/o IORDY Transfer Rate:
	16.7 MBytes/s 

	
	Transfer Width:
	16-bit 

	
	Native Command Queuing:
	Supported, Max. Depth: 32 

	
	TRIM Command:
	Not Supported 

	 
	
	

	[Device flags] 

	
	Fixed Drive:
	Present 

	
	Removable Drive:
	Not Present 

	
	Magnetic Storage:
	Present 

	
	LBA Mode:
	Supported 

	
	DMA Mode:
	Supported 

	
	IORDY:
	Supported 

	
	IORDY Disableable:
	Supported 

	 
	
	

	[Features] 

	
	Write Cache:
	Present, Active 

	
	S.M.A.R.T. Feature:
	Present, Active 

	
	Security Feature:
	Present, Inactive 

	
	Removable Media Feature:
	Not Present, Disabled 

	
	Power Management:
	Present, Active 

	
	Advanced Power Management:
	Not Present, Inactive 

	
	Packet Interface:
	Not Present, Disabled 

	
	Look-Ahead Buffer:
	Present, Active 

	
	Host Protected Area:
	Present, Enabled 

	
	Power-Up In Standby:
	Supported, Inactive 

	
	Automatic Acoustic Management:
	Not Suppported, Inactive 

	
	48-bit LBA:
	Supported, Active 

	
	Host-Initiated Link Power Management:
	Supported 

	
	Device-Initiated Link Power Management:
	Not Supported 

	
	In-Order Data Delivery:
	Not Supported 

	
	Hardware Feature Control:
	Not Supported 

	
	Software Settings Preservation:
	Supported, Enabled 

	
	NCQ Autosense:
	Not Supported 

	
	Link Power State Device Sleep:
	Not Supported 

	
	Hybrid Information Feature:
	Not Supported 

	
	All Write Cache Non-Volatile:
	Not Supported 

	
	Extended Number of User Addressable Sectors:
	Not Supported 

	
	Device Encrypts All User Data:
	Not Supported 

	
	CFast Specification:
	Not Supported 

	
	NCQ Priority Information:
	Supported 

	
	Host Automatic Partial to Slumber Transitions:
	Not Supported 

	
	Device Automatic Partial to Slumber Transitions:
	Not Supported 

	
	NCQ Streaming:
	Not Supported 

	
	NCQ Queue Management Command:
	Not Supported 

	
	DEVSLP to Reduced Power State:
	Not Supported 

	
	Extended Power Conditions Feature:
	Not Supported 

	
	Sense Data Reporting Feature:
	Not Supported 

	
	Free-Fall Control Feature:
	Not Supported 

	 
	
	

	[Self-Monitoring, Analysis and Reporting Technology (S.M.A.R.T.)] 

	
	[01] Raw Read Error Rate:
	200/51, Worst: 200 

	
	[03] Spin Up Time:
	187/21, Worst: 184 (Data = 5633) 

	
	[04] Start/Stop Count:
	100/Always OK, Worst: 100 (Data = 696) 

	
	[05] Reallocated Sector Count:
	200/140, Worst: 200 

	
	[07] Seek Error Rate:
	200/Always OK, Worst: 200 

	
	[09] Power-On Hours/Cycle Count:
	99/Always OK, Worst: 99 (Data = 1181 hours / 49.2 days) 

	
	[0A] Spin Retry Count:
	100/Always OK, Worst: 100 

	
	[0B] Calibration Retry Count:
	100/Always OK, Worst: 100 

	
	[0C] Power Cycle Count:
	100/Always OK, Worst: 100 (Data = 421) 

	
	[C0] Power-Off Retract Count:
	200/Always OK, Worst: 200 (Data = 8) 

	
	[C1] Load/Unload Cycle Count:
	200/Always OK, Worst: 200 (Data = 1741) 

	
	[C2] Temperature
	118/Always OK, Worst: 103 (Data = 32.0 ﾰC) 

	
	[C4] Reallocation Event Count:
	200/Always OK, Worst: 200 

	
	[C5] Current Pending Sector Count:
	200/Always OK, Worst: 200 

	
	[C6] Off-Line Uncorrectable Sector Count:
	200/Always OK, Worst: 200 

	
	[C7] UltraDMA/SATA CRC Error Rate:
	200/Always OK, Worst: 200 

	
	[C8] Write/Multi-Zone Error Rate:
	200/Always OK, Worst: 200 


	TSSTcorp CDDVDW SH-224DB

	


	
	 
	

	[General information] 

	
	Drive Model:
	TSSTcorp CDDVDW SH-224DB 

	
	Drive Revision:
	SB00 

	
	Serial Number:
	R93E6YAD400AP9 

	
	Device Type:
	DVD+R DL 

	 
	
	

	[Device capabilities] 

	
	Drive can read:
	CD-R, CD-RW, DVD-R, DVD-RW, DVD+R, DVD+RW, DVD-RAM, DVD+R DL 

	
	Drive can write:
	CD-R, CD-RW, DVD-R, DVD-RW, DVD+R, DVD+RW, DVD-RAM, DVD+R DL 


	Audio

	


	
	 
	


	ATI/AMD SB600 - High Definition Audio Controller

	


	
	 
	

	
	Audio Adapter:
	ATI/AMD SB600 - High Definition Audio Controller 

	
	Audio Controller Hardware ID:
	PCI\VEN_1002&DEV_4383&SUBSYS_F6411462&REV_00 

	 
	
	

	
	High Definition Audio Codec:
	Unknown 0 

	
	Audio Codec Hardware ID:
	HDAUDIO\FUNC_04&VEN_0000&DEV_0000&SUBSYS_00000000 


	ATI/AMD Cedar/Park/Robson - High Definition Audio Controller

	


	
	 
	

	
	Audio Adapter:
	ATI/AMD Cedar/Park/Robson - High Definition Audio Controller 

	
	Audio Controller Hardware ID:
	PCI\VEN_1002&DEV_AA68&SUBSYS_AA68148C&REV_00 

	 
	
	

	
	High Definition Audio Codec:
	ATi RADEON HDMI 

	
	Audio Codec Hardware ID:
	HDAUDIO\FUNC_01&VEN_1002&DEV_AA01&SUBSYS_00000000 

	 
	
	

	[Driver Information] 

	
	Driver Manufacturer:
	Advanced Micro Devices 

	
	Driver Description:
	AMD High Definition Audio Device 

	
	Driver Provider:
	Advanced Micro Devices 

	
	Driver Version:
	7.12.0.7719 

	
	Driver Date:
	20-Jun-2014 

	
	DeviceInstanceId
	HDAUDIO\FUNC_01&VEN_1002&DEV_AA01&SUBSYS_00AA0100&REV_1002\5&2E5A6745&0&0001 


	Network

	


	
	 
	


	RealTek Semiconductor RTL8168/8111 PCI-E Gigabit Ethernet NIC

	


	
	 
	

	[General information] 

	
	Network Card:
	RealTek Semiconductor RTL8168/8111 PCI-E Gigabit Ethernet NIC 

	
	Vendor Description:
	Realtek PCIe GBE Family Controller 

	
	MAC Address:
	D4-3D-7E-2A-DB-5B 

	 
	
	

	[Capabilities] 

	
	Maximum Link Speed:
	1000 Mbps 

	
	Transmit Buffer Size:
	193792 Bytes 

	
	Receive Buffer Size:
	775168 Bytes 

	
	Hardware ID:
	PCI\VEN_10EC&DEV_8168&SUBSYS_76411462&REV_06 

	 
	
	

	[Driver Information] 

	
	Driver Manufacturer:
	Realtek 

	
	Driver Description:
	Realtek PCIe GBE Family Controller 

	
	Driver Provider:
	Realtek 

	
	Driver Version:
	7.67.1226.2012 

	
	Driver Date:
	26-Dec-2012 

	
	DeviceInstanceId
	PCI\VEN_10EC&DEV_8168&SUBSYS_76411462&REV_06\4&3411228A&0&0028 


	D-Link DWA-140 Wireless N USB Adapter(rev.D)

	


	
	 
	

	[General information] 

	
	Network Card:
	D-Link DWA-140 Wireless N USB Adapter(rev.D) 

	
	Vendor Description:
	Microsoft 

	
	MAC Address:
	C4-A8-1D-E0-C3-92 

	 
	
	

	[Capabilities] 

	
	Maximum Link Speed:
	144 Mbps 

	
	Transmit Buffer Size:
	6201344 Bytes 

	
	Receive Buffer Size:
	6201344 Bytes 


	Ports

	


	
	 
	


	Serial Ports

	


	
	 
	


	Parallel Ports

	


	
	 
	


	USB

	


	
	 
	


	Standard OpenHCD USB-Hostcontroller

	


	
	 
	


	Root Hub

	


	
	 
	


	[Port1] : No Device Connected

	


	
	 
	


	[Port2] : No Device Connected

	


	
	 
	


	[Port3] : No Device Connected

	


	
	 
	


	Standard OpenHCD USB-Hostcontroller

	


	
	 
	


	Root Hub

	


	
	 
	


	[Port1] : No Device Connected

	


	
	 
	


	[Port2] : USB-Verbundger?

	


	
	 
	

	[Device Information] 

	
	Device Manufacturer:
	

	
	Product Name:
	

	
	Serial Number:
	

	
	USB Version Supported:
	2.00 

	
	USB Device Speed:
	USB 1.1 Low-speed 

	
	Driver Description:
	USB-Verbundger? 

	
	Hardware ID:
	USB\VID_04F3&PID_0103 

	 
	
	

	[Driver Information] 

	
	Driver Manufacturer:
	(Standard-USB-Hostcontroller) 

	
	Driver Description:
	USB-Verbundger? 

	
	Driver Provider:
	Microsoft 

	
	Driver Version:
	6.1.7601.18328 

	
	Driver Date:
	21-Jun-2006 

	
	DeviceInstanceId
	USB\VID_04F3&PID_0103\5&2BA28D42&0&2 


	[Port3] : USB-Eingabeger?

	


	
	 
	

	[Device Information] 

	
	Device Manufacturer:
	Logitech 

	
	Product Name:
	USB Optical Mouse 

	
	Serial Number:
	N/A 

	
	USB Version Supported:
	2.00 

	
	USB Device Speed:
	USB 1.1 Low-speed 

	
	Driver Description:
	USB-Eingabeger? 

	
	Hardware ID:
	USB\VID_046D&PID_C018 

	 
	
	

	[Driver Information] 

	
	Driver Manufacturer:
	(Standardsystemger?e) 

	
	Driver Description:
	USB-Eingabeger? 

	
	Driver Provider:
	Microsoft 

	
	Driver Version:
	6.1.7601.18199 

	
	Driver Date:
	21-Jun-2006 

	
	DeviceInstanceId
	USB\VID_046D&PID_C018\5&2BA28D42&0&3 


	Standard PCI-zu-USB erweiterter Hostcontroller

	


	
	 
	


	Root Hub

	


	
	 
	


	[Port1] : D-Link DWA-140 Wireless N USB Adapter(rev.D)

	


	
	 
	

	[Device Information] 

	
	Device Manufacturer:
	Ralink 

	
	Product Name:
	802.11 n WLAN 

	
	Serial Number:
	1.0 

	
	USB Version Supported:
	2.00 

	
	USB Device Speed:
	USB 2.0 High-speed 

	
	Driver Description:
	D-Link DWA-140 Wireless N USB Adapter(rev.D) 

	
	Hardware ID:
	USB\VID_2001&PID_3C20 

	 
	
	

	[Driver Information] 

	
	Driver Manufacturer:
	D-Link Corporation 

	
	Driver Description:
	D-Link DWA-140 Wireless N USB Adapter(rev.D) 

	
	Driver Provider:
	D-Link Corporation 

	
	Driver Version:
	5.0.1.0 

	
	Driver Date:
	09-Oct-2012 

	
	DeviceInstanceId
	USB\VID_2001&PID_3C20\1.0 


	[Port2] : No Device Connected

	


	
	 
	


	[Port3] : No Device Connected

	


	
	 
	


	[Port4] : No Device Connected

	


	
	 
	


	[Port5] : No Device Connected

	


	
	 
	


	[Port6] : No Device Connected

	


	
	 
	


	Standard OpenHCD USB-Hostcontroller

	


	
	 
	


	Root Hub

	


	
	 
	


	[Port1] : No Device Connected

	


	
	 
	


	[Port2] : No Device Connected

	


	
	 
	


	[Port3] : No Device Connected

	


	
	 
	


	Standard OpenHCD USB-Hostcontroller

	


	
	 
	


	Root Hub

	


	
	 
	


	[Port1] : No Device Connected

	


	
	 
	


	[Port2] : No Device Connected

	


	
	 
	


	[Port3] : No Device Connected

	


	
	 
	


	Standard PCI-zu-USB erweiterter Hostcontroller

	


	
	 
	


	Root Hub

	


	
	 
	


	[Port1] : USB-Massenspeicherger?

	


	
	 
	

	[Device Information] 

	
	Device Manufacturer:
	Western Digital 

	
	Product Name:
	Ext HDD 1021 

	
	Serial Number:
	5743415A414C333630383738 

	
	USB Version Supported:
	2.00 

	
	USB Device Speed:
	USB 2.0 High-speed 

	
	Driver Description:
	USB-Massenspeicherger? 

	
	Hardware ID:
	USB\VID_1058&PID_1021 

	 
	
	

	[Driver Information] 

	
	Driver Manufacturer:
	Kompatibles USB-Speicherger? 

	
	Driver Description:
	USB-Massenspeicherger? 

	
	Driver Provider:
	Microsoft 

	
	Driver Version:
	6.1.7601.17577 

	
	Driver Date:
	21-Jun-2006 

	
	DeviceInstanceId
	USB\VID_1058&PID_1021\5743415A414C333630383738 


	[Port2] : USB-Massenspeicherger?

	


	
	 
	

	[Device Information] 

	
	Device Manufacturer:
	Generic 

	
	Product Name:
	Mass Storage Device 

	
	Serial Number:
	058F63666471 

	
	USB Version Supported:
	2.00 

	
	USB Device Speed:
	USB 2.0 High-speed 

	
	Driver Description:
	USB-Massenspeicherger? 

	
	Hardware ID:
	USB\VID_058F&PID_6366 

	 
	
	

	[Driver Information] 

	
	Driver Manufacturer:
	Kompatibles USB-Speicherger? 

	
	Driver Description:
	USB-Massenspeicherger? 

	
	Driver Provider:
	Microsoft 

	
	Driver Version:
	6.1.7601.17577 

	
	Driver Date:
	21-Jun-2006 

	
	DeviceInstanceId
	USB\VID_058F&PID_6366\058F63666471 


	[Port3] : No Device Connected

	


	
	 
	


	[Port4] : No Device Connected

	


	
	 
	


	[Port5] : No Device Connected

	


	
	 
	


	[Port6] : No Device Connected

	


	
	 
	


	Standard OpenHCD USB-Hostcontroller

	


	
	 
	


	Root Hub

	


	
	 
	


	[Port1] : No Device Connected

	


	
	 
	


	[Port2] : No Device Connected

	


	
	 
	


